{"text_format":"2","workbook":"xlsx","n_sheets":8,"sheets":["Neopost Equipment","Neopost Software","DataPac","Rena","Supplies","Formax","MBM Corp","FP"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Neopost Equipment","index":0,"n_rows":120,"n_cols":12,"rows_kept":120,"cut":false,"hidden":false,"merged":[[20,7,22,7],[20,9,22,9],[20,11,22,11],[20,10,22,10],[20,3,22,3],[20,4,22,4],[20,6,22,6],[55,6,58,6],[55,7,58,7],[55,3,58,3],[51,3,52,3],[51,2,52,2],[51,6,52,6],[51,7,52,7],[37,6,41,6],[37,7,41,7],[37,3,41,3],[51,4,52,4]]}
["Category","Sub-Category (if applicable)","Product Name","Product Description","Specifications","Serial #","Vendor Site URL","Video Content URL(s)","Downloadable Content URL(s)","Pictures Saved?","Migrated?","Alternative Site URL"]
["Addressing Systems","Low Volume"]
[null,null,"AS-150 Addressing System","Versatile Address, Barcode and Graphics Printing Solution\nThe AS-150 is a user-friendly, entry-level printing solution perfect for small to mid-size mailrooms. This multi-purpose equipment can print small, coin-size envelopes but still run standard #9, #10 and 6” x 9” envelopes.\n\nSmall Media Inkjet Printer\n\nUtilizing exclusive HP print cartridges that come in formulas that allow you to print on a wide variety of stock, the AS-150 fixed head printer has four print quality levels ranging from 150 up to 600 dpi. It features an easy-to-use menu system with a display for quick access to menu features and has a compact footprint to accommodate tight production space.\n\nProcesses as many as 5,500 #10 envelopes per hour \nPrint up to 7,500 coin-size envelopes or seed packets per hour \nOffers four levels of print quality\nHolds up to 300 envelopes in feeder\nComplies with Intelligent Mail® barcode regulations\nSpot color capability\n","Performance\nAs many as 5,500 addresses per hour\n\nDocument Handling\nPrint area: Up to 1.5” x 9.25”\nMinimum media size (L x W): 4” x 2.125”\nMaximum media size (L x W): 9.25” x 6.5”\nMaximum media thickness: Up to 0.020”\n\nSystem Dimensions\n14”L x 13”D x 18.5”W",null,"https://www.neopostusa.com/equipment/as-150-addressing-system","https://www.youtube.com/watch?v=APZP85STxlc","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neopost_as-150_address_printer_0117.pdf","Yes","Yes"]
[null,"Mid Volume"]
[null,null,"AS-710 Addressing System","Versatile Address, Barcode and Graphics Printing Solution\nThe AS-710 features HP® print technology, provides one-touch controls and easy-to-use, Plug'n Play software to minimize set-up time.\n\nThe AS-710 will give mailings a professional look. It prints addresses, logos, barcodes and graphics almost anywhere on mail pieces.\n\nIncrease the AS-710’s effectiveness by adding an address management software solution. Take advantage of USPS® postal automation discounts, decrease duplicate mailings and save both time and money. \n\nAdaptable shuttle head technology\nOne-touch controls and easy-to-use, Plug'n Play software\nIntegrates with CASS- and PAVE-certified software for USPS postal automation discounts\nComplies with Intelligent Mail® barcode regulations  ","Performance\nAs many as 14,000 addresses per hour\n\nDocument Handling\nPrint area: 9” x 20”\nMinimum document size: 3” x 2.75”\nMaximum document size: 19” x 17”\nHopper capacity: 350 #10 envelopes\n\nSize\n22”L x 16”H x 18”D",null,"https://www.neopostusa.com/addressing-systems/as-710","https://www.youtube.com/watch?v=WTaiJIN7doM","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/as-710_product_sheet.pdf","Yes","Yes"]
[null,null,"AS-930 Addressing System","Mid-Range Printing Solution for Repetitive Mailing\n\nThe system features fixed-head technology capable of printing at nearly constant speed regardless of content. Print on a wide variety of documents: envelopes to magazines to newsletters.\n\nTake advantage of USPS® postal automation discounts and decrease duplicate mailings by combining the AS-930 with postal discounting software. Saves both time and money.\n\nPrints at high speeds thanks to fixed-head technology \nOne-touch controls and easy-to-use, Plug'n Play software\nIntegrates with CASS- and PAVE-certified software for USPS postal automation discounts\nComplies with Intelligent Mail® barcode regulations ","Performance\nPostcards: As many as 39,000 per hour\nEnvelopes: As many as 27,000 per hour\nPrint resolution as fine as 600 dpi\n\nDocument Handling\nPrint Area: 1.5” x 19.6”\nMinimum document size: 5.3” x 2.76”\nMaximum document size: 19” x 14”\nHopper capacity: 350 #10 envelopes\n\nSize\n26”L x 20”H x 16”D",null,"https://www.neopostusa.com/addressing-systems/as-930","https://www.youtube.com/watch?time_continue=73&v=diQxg-cTRwI","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/as-930_product_sheet.pdf","Yes","Yes"]
[null,null,"AS-940 Addressing System","Mid volume versatile address & graphics printing solutions\n\nThe AS-940's advanced technology, precision engineering and exceptional attention to detail make this high-performance addressing system the right one for growing businesses.\n\nWith a feeding system that has three rows of high-grip rollers and the capacity for materials as thick as 1/4”, the AS-940 can handle almost any job.\n\nThe dual print-head configuration can add return addresses, indicia, barcodes and more to the primary address in a single pass on a large, 2.5” print area. The result is a professional and unique look every time. The AS-940 makes quick work of even the largest jobs.","Performance\nAs many as 22,000 addresses per hour\nPrint resolution as fine as 600 dpi\n\nDocument Handling\nPrint area: 2.5” x 15”\nMinimum document size: 5” x 3”\nMaximum document size: 15” x 13.5”\n\nSize\n20”L x 21”H x 18”D",null,"https://www.neopostusa.com/addressing-systems/as-940","https://www.youtube.com/watch?v=mC__q69nOT8","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/as-940_product_sheet.pdf","Yes","Yes"]
[null,"High Volume"]
[null,null,"AS-960 Addressing System","Project a professional appearance with all mailings\n\nThe AS-960 prints machine-readable barcodes, like the Intelligent Mail® barcode, that are fully compatible with the Postal Service’s reading systems.\n\nThe AS-960 integrates with address quality management software such as Neopost’s Business Mailer or similar third-party software solution. That means custom-designed address layouts as well as address cleansing, address optimization and other money-saving features. ","Performance\nAs many as 26,000 addresses per hour\nPrint resolution as fine as 600 x 600 dpi\n\nDocument Handling\nPrint area: 3” x 20”\nMinimum document size: 3.46” x 5.31”\nMaximum document size: 15” x 20”\nHopper capacity: 500 #10 envelopes\n\nSize\n24”L x 29”H x 21”D",null,"https://www.neopostusa.com/addressing-systems/as-960","https://www.youtube.com/watch?v=cfkpZ5JNAPQ","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/as-960_product_sheet.pdf","Yes","Yes"]
[null,null,"AS-980 Addressing System","High Volume Addressing Solution\n\nThe AS-980 features a large, 3” print area and three independent print modules. That versatility means addresses, attention lines, postal barcodes, return addresses and indicia can be printed on a mail piece at the same time.\n\nThe multi-channel vacuum transport has repositionable outer transport belts and material guides that can be customized to keep pieces in place and ensure perfect registration every time.","Performance\nAs many as 26,000 addresses per hour\nPrint resolution as fine as to 600 x 600 dpi\n\nDocument Handling\nPrint area: 3” x 17”\nMinimum document size: 3” x 5”\nMaximum document size: 13.5” x 17”\n\nSize\n30”L x 24”H x 16”D",null,"https://www.neopostusa.com/addressing-systems/as-980","N/A","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/as-980_product_sheet.pdf","Yes","Yes"]
[null,"Production Volume"]
[null,null,"AS-3630 Addressing System","A Production Volume Addressing System\n\nFeatures six print heads with adjustable 3” print area\nComplies with Intelligent Mail® barcode regulations\nOffers spot-color printing for versatile messaging\nIncludes envelope design software for personalized mailings","Performance\nAs many as to 40,000 addresses per hour\nPrint resolution as fine as to 600 x 600 dpi\n\nDocument Handling\nPrint area: 3” x 20”\nMinimum document size: 3.5” x 3.5”\nMaximum document size: 15” x 16.5”\n\nSize\n35”L x 29”W x 13”H",null,"https://www.neopostusa.com/addressing-systems/as-3630","N/A","N/A","Yes","Yes"]
[null,null,"AS-3640 Addressing System","Production Addressing Solution Offers Flexibility and Exceptional Print Quality\n\nThe AS-3640 is capable of working in-line with folder/inserters and other document processing equipment or in stand-alone operation.\n\nProcesses as many as 40,000 addresses  per hour\nUtilizes 12 print heads and adjustable 6” print area\nComplies with Intelligent Mail® barcode regulations\nOffers spot-color printing for versatile messaging\nIncludes envelope design software for personalized mailings","Performance\nAs many as to 40,000 addresses per hour\nPrint resolution as fine as to 600 x 600 dpi\n\nDocument Handling\nPrint area: 6” x 20”\nMinimum document size: 1.5” x 2.5”\nMaximum document size: 15” x 30”\n\nSize\n58”L x 39”W x 55”H",null,"https://www.neopostusa.com/addressing-systems/as-3640","N/A","N/A","Yes","Yes"]
["Digital Printers"]
[null,null,"HD-C17n Full-Color Printer","Large-Format Color Printing Technology\n\nCompact in size yet big on media flexibility, this affordable color printer creates documents in letter, tabloid and even 52” banners in high definition color.\n\nFeatures HD color printing technology\nOffers fast print speeds: color output as fast as 30 ppm; monochrome at 32 ppm\nDelivers 1200 x 600 dpi resolution\nIncludes Single Pass Color™ digital technology for printing cover stock as thick as 80 lb\nFits into almost any business environment thanks to compact design and small footprint","Performance\nPrint speed as high as 30 color pages per minute\nMonthly duty cycle: 75,000 pages\n\nPaper Handling\nStandard paper input: 400 sheets (300-sheet letter/legal/tabloid/universal tray and 100-sheet multi-purpose feeder)\nMaximum paper input: 1,460 sheets with standard/optional second/third trays\nDuplex (two-sided) printing: optional\n\nSize\n19.1\"W x 22.8\"D x 13.6\"H",null,"https://www.neopostusa.com/digital-printers/hd-c17n-full-color-printer","N/A","N/A","Yes","Yes"]
[null,null,"MACH 5 Digital Color Printer","Give Your Mailings a Productivity Boost\n\nThe MACH 5 printer leverages Memjet® technology to dramatically improve direct mail and transpromotional marketing at an extremely low total cost of ownership.\n\nPerfect Mix of Speed and Color for Direct Marketing Campaigns\n\nThe MACH 5 allows mail centers, print shops and marketers of all sizes to take advantage of exceptional color printing resolution and printing speed across a wide variety of envelopes, paper and label stocks. The MACH 5 is ideally suited for applications such as envelopes and stationery, wedding, birthday, holiday cards and special event invitations printing, mail addressing and barcoding, postage printing, and more.\n\nCombined with the optional mColor RIP and Workflow Software, the MACH 5 delivers professional-level color quality control. Exceptional print quality plus speed translate into the lowest per-piece cost and fastest ROI for direct mail and transpromotional marketing printing.","Performance\nPrint resolution as fine as 1600 x 1600 dpi\nPrint speed as fast as 3,600 pages per hour\nAs many as 7,500 #10 envelopes per hour\nColor matrix as high as 16.8 million colors\n\nDocument Handling\nPrint area as great as to 8.5” x 17” with full-bleed capability\nMinimum material size (L x W) 4 1/4” x 3”\nMaximum material size (L x W) 17” x 9.5”\nMaterial thickness as thick as 1/48” \n\nSize\n24”L x 20”W x 18”H",null,"https://www.neopostusa.com/addressing-systems/mach5-digital-color-printer","https://www.youtube.com/watch?v=2-BbdUH4kMc","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo16516_mach5_brochupdate_hq.pdf","Yes","Yes"]
[null,null,"MACH 6 Digital Printer","Bringing a new dimension to full color print for mailing and packaging\nCombined with the optional mColor RIP and Workflow Software, the MACH 6 delivers professional-level color quality control. Exceptional print quality plus speed translate into the lowest per-piece cost and fastest ROI for direct mail and transpromotional marketing printing.\n \nMACH 6 Digital Printer\n\nA breakthrough in the world of mailing and packaging, the MACH 6 features a wide enough throat to accommodate 10” x 13” flats and mailers up to 10.5\" x 17\", as well as a 3/8” thick transport to be able to run padded envelopes, chipboard, corrugated cardboard, folded cartons and more. All of this in addition to the traditional #10 envelopes, cardstock, invitations and more that its predecessor, the MACH 5, could accommodate. Mail centers, print shops, packaging centers and marketers of all sizes can take advantage of exceptional color printing resolution and printing speed. The MACH 6 is also great for mail addressing, barcoding, postage printing, and more.","Performance\nPrint resolution as fine as 1600 x 1600 dpi\nPrint speed as fast as 3,600 pages per hour\nAs many as 8,000 #10 envelopes per hour\n\nDocument Handling\nPrint area as great as 8.77” x 40” with full-bleed capability under 8.6”\nMinimum material size (L x W) 4” x 3”\nMaximum material size (L x W) 17” x 10.5”\nMaterial thickness as thick as 3/8” or 10mm\n\nSize\n34\"L x 22\"W x 21\"H",null,"https://www.neopost.com/equipment/digital-printers/mach-6-digital-printer","https://www.youtube.com/watch?v=P6sOK9QnRik","https://www.neopost.com/sites/neopost.com/files/Product/Brochure/mach_6_cutsheet.pdf","Yes","Yes"]
[null,null,"MACH 8 Digital Printer","High-Volume Digital Color Printing\n\nThe MACH 8 Digital Color Printer features a high-capacity paper feeder and automatic output stacker that have the ability to hold as many as 5,000 sheets.\n\nFeatures HD color printing technology\nOffers fast color output as fast as 60 ppm\nReduces per-piece cost and accelerates ROI\nRequires no per-job set-up costs\nDelivers professional-level color quality control","Performance\nPrint speed as high as 3,600 letter-size pages per hour\nPrint area as big as up to 8.5” to 14.5” with full-bleed capability\n\nPaper Handling\nFeeder capacity: 5,000 single sheets/10 reams 20 lb paper\nPrint area: (W x L) as big as 8.5” to 14.5” with full-bleed capability\nMinimum material size: (W x L) 3” x 4.2”\nMaximum material size: (W x L) 9” x 14.5”\n\nSize\n33.5\"L x 23\"W x 37.5\"H",null,"https://www.neopostusa.com/digital-printers/mach-8","https://www.youtube.com/watch?v=iDgzjEh0JQ8","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/mach8_product_sheet.pdf","Yes","Yes"]
[null,null,"HD-CX Series Digital Color Printers","Multi-Media Power with Breathtaking 5-Color Production\n\nThe HD-CX Series provides print speeds up to 50 ppm and true 1200 x 1200 dpi resolution.\n\nStunning results at breathtaking speed\n\nMultimedia: When it comes to variety, size and thickness of media, the HD-CX Series greatly extends the Neopost range of media support. Both models easily handle 360-gsm extra-thick card stock, 14-point polyester, magnetic media, transparency films and much more—in sizes ranging from 3\" x 5\" index cards to 13\" x 52\" banners.\nProduction: HD-CX Series devices have affordable digital short-run capabilities. Produce striking comps, one-offs and reprints at up to 50 ppm. And the HD-CX1700 has the added flexibility of being able to apply white text and graphics to dark media, and to place clear toner selectively on a design, with eye-catching results.\nPlatform: These devices represent a new design driven by an aggressive goal—to create rugged, affordable and flexible printers aligned with the direction of today’s print production marketplace. They feature short-run capacities and fast print speed, and deliver stunning output across the widest range of media. Add the optional mColor RIP & Workflow software and get formidable, professional devices with enhanced color management and simplified workflows.\nIncluding the industry’s only 5-color LED device\n\nThe HD-CX Series lets you extend your in-house printing and presentation capabilities from the expected to the extraordinary. These affordable printing devices, with their ease of use and low total cost of ownership, enable you to produce stunning documents, offer new services, be competitive, and grow your business. It is also perfect for the Advertising, Graphic Arts and Design department, company or school—with their greater sensitivity to color—this device is perfect. With the optional mColor RIP & Workflow software, creative- and production-oriented users alike will love the color consistency and accuracy required for their projects and short-run print jobs. And keepers of the budget will be thrilled with such low costs per page, especially at higher volumes.\n\nHD-CX1600 - for efficiency-minded, budget-conscious office users and departments with a need for excellent color—such as Marketing and Corporate Communications—this is the ideal printer. Stunning results at breathtaking speed. Simple operation, with auto duplex and network standard. Plus all the media flexibility offered across the HD-CX Series platform.\nHD-CX1700 – all of the above, plus the extraordinary capability of applying white or clear gloss toner in addition to CMYK. Here is the cutting-edge, multimedia production platform that creative, opportunity-seeking Design Firms, Specialty Print Shops, even large Retailers have been dreaming of: a fast, flexible, affordable, easy-to-use 5-station device.","N/A",null,"https://www.neopostusa.com/digital-printers/hd-cx-digital-color-printer","https://www.youtube.com/watch?v=5jvBao87WN4","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo16200_hd_cx_broch_hq.pdf","Yes","Yes"]
["Document Folders"]
[null,null,"PF-60 Folder","Fully Automatic Letter Folding Solutions\n\nAutomatic document folders can be easily adjusted to process a variety of precision folds including single, letter, z-fold, gate, fold-out and double-parallel. With easy-to-use control panels and automatic job settings, simply select a fold type, press start and walk away.\n\nSave Time and Effort with Neopost Document Folding Equipment\n\nEasy setup and operation are the hallmark of Neopost document folders. The range of features and quiet operation make these models ideal for the office setting.\n\nEach model can hold a full ream of paper and perform six popular folds in 11\", 14\" and 17\" format using standard or custom measurements while the telescoping stacker provides convenient, effortless operation.","Fold Types\nsingle, letter, z-fold, gate, fold-out and double-parallel\n\nCapacity\nAs many as 500 20-lb sheets\n \n\nDocument Handling\nMinimum paper width: 3.5”\nMaximum paper width: 12.25”\nMinimum paper length: 5”\nMaximum paper length: 18”\n\nSystem Dimensions\nClosed: 33”L x 20”W x 19”H\nFully Extended: 60”L x 20”W x 19”H",null,"https://www.neopostusa.com/document-folders","https://www.youtube.com/watch?v=vYuNO0vA2fI","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/pf-90_product_sheet.pdf","Yes","Yes"]
[null,null,"PF-80 Folder",{"$nulls":5},"https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/pf-80_product_sheet_0.pdf"]
[null,null,"PF-90 Folder",{"$nulls":5},"https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/pf-60_product_sheet_0.pdf"]
["Folder Inserters","Low Volume"]
[null,null,"DS-35 Folder Inserter","Automatically fold, insert and seal up to 5,000 envelopes per month\n\nImagine you could assemble 1,000 pieces of mail in under an hour. Folded, stuffed, sealed, metered and out the door in very little time. The DS-35 folder inserter is a revelation for small- to medium-size businesses. Produce professional looking mail pieces each and every time while you devote time to other important tasks. \n\nBoost office productivity; assemble mail up to 10 times faster than by hand\n\nEase of Use\n\nThe color touch screen control panel makes operation simple. Load envelopes and documents, select a job and press the start button. The DS-35 is that easy to use.\n\nProductivity\n\nFolds, collates, inserts, seals, and counts up to 22 finished envelopes per minute. Load and run up to 100 documents at a time from each feeder without reloading.\n\nVersatility\n\nCompact and quiet, the DS-35 is ideal for any office environment. Document feeders can accommodate letter and legal-size documents in addition to inserts and business reply envelopes.\n\nAccuracy\n\nOur exclusive feeder thickness detection technology prevents double document errors, helping to ensure that each customer gets the right documents.","Capacity\nAs many as 1,350 documents per hour (22/minute)\nUp to 5,000 finished envelopes per month.\n\nDocument Handling\nHandles #10 and 6” x 9.5” envelopes\nFold up to 5 pages if single folded, or 3 pages letter folded (20 lb.) \n\nSystem Dimensions\n26”L x 17”D x 22”H – Without catch tray",null,"https://www.neopostusa.com/folder-inserters/ds-35","https://www.youtube.com/watch?v=vljUaTAIdWo","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo14867_ds_35_broch_hq_0.pdf","Yes","Yes"]
[null,null,"DS-63 Folder Inserter","Dependably collates, folds and inserts up to 15,000 envelopes per month\n\nAt speeds of up to 2,200 envelopes per hour, the DS-63 folding inserting system has the technology needed to efficiently prepare your business mailings. It automates the processing of checks, multi-page invoices, letters, legal-size documents, inserts and business reply envelopes. The optional scanner reads optical marks printed on your documents, allowing you to efficiently and securely process variable page documents.\n\nSimplify folding and inserting of documents and get communications out faster\n\nEase of Use\n\nThe 5.7” color touch screen and wizard-based guidance, simplify operation. Quickly recall up to 15 stored jobs or create new jobs with ease. Load documents and envelopes, press start and the DS-63 automatically measures the materials and sets itself up.\n\nProductivity\n\nContinuously feed 325 sheets from each feeder, or up to 650 documents using two feeders in cascading mode. Automatically collate, fold, insert, seal, and count up to 2,200 mail pieces per hour.\n\nVersatility\n\nDocument feeders accommodate a wide variety of material combinations, including full sheets, inserts and business reply envelopes. Four system configurations and three finished envelope exit options are available to meet your specific needs.\n\nAccuracy\n\nOur exclusive feeder technology prevents double document errors. When equipped with optional barcode reading, you can process variable-page document sets and selectively include enclosures with absolute accuracy.","Capacity\nAs many as 2,200 documents per hour (36/minute)\nUp to 15,000 finished envelopes per month.\n\nDocument Handling\nHandles #10 and 6\" x 9.5\" envelopes\nFold up to 5 pages if single folded, or 3 pages letter folded (20 lb.) \n\nSystem Dimensions\n49”L x 16.5”D x 36”H",null,"https://www.neopostusa.com/folder-inserters/ds-63","https://www.youtube.com/watch?time_continue=4&v=eUMK9vV4hhk","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo15016_ds_63_broch_hq.pdf","Yes","Yes"]
[null,null,"DS-65 Folder Inserter","Fold, insert and seal up to 20,000 envelopes per month\n\nThe DS-65 is one of our most advanced low-volume folding inserting systems. It can process checks, multi-page invoices, letters, legal-size documents, inserts and business reply envelopes. With a processing speed of up to 2,400 envelopes per hour, it can fold up to 8 sheets together and ensure a professional looking mail piece.   \n\nAutomate mail assembly and save time for more important office tasks\n\nEase of use\n\nThe color touch screen control panel simplifies operation with graphical user guidance and wizard-based programming. Automatic new job setup based on the documents and envelopes you place in the trays.\n\nProductivity\n\nFeeders and envelope stacker have matching capabilities to reduce time spent reloading. A built-in vertical stacker provides quick unloading of filled envelopes and also reserves the printing order.\n\nVersatility\n\nThe document feeders accommodate an impressive variety of material sizes and combinations from full sheets to short inserts. Four system configurations are available to meet your specific requirements.\n\nAccuracy\n\nOur exclusive feeder technology prevents double document errors. When equipped with optional barcode reading, it can process variable-page document sets and selectively include enclosures with absolute accuracy.","Capacity\nAs many as 2,400 documents per hour (40/minute)\nUp to 20,000 finished envelopes per month.\n\nDocument Handling\nHandles #10 and 6’ x 9.5” envelopes\nFold up to 8 pages if single folded, or 5 pages letter folded (20 lb.)\n\nSystem Dimensions\n31.5”L x 17.5”D x 26.9”H",null,"https://www.neopostusa.com/folder-inserters/ds-65","https://www.youtube.com/watch?time_continue=7&v=M0IvSbjpUoQ","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo14776_ds_65_broch_hq.pdf","Yes","Yes"]
[null,"Mid Volume"]
[null,null,"DS-75i Folder Inserter","Fold, insert and seal up to 40,000 envelopes per month\n\nThe DS-75i mid-volume folder inserter has the technology needed to handle a wide variety of business mailings at speeds up to 3,800 envelopes per hour. It can process checks, multi-page invoices, letters, legal-size documents, inserts and business reply envelopes.  The optional scanner can read a broad range of barcodes allowing you to efficiently collate and process multi-page documents.\n\nOptimize mail assembly and get important documents\nout the door accurately and efficiently\n\nEase of Use\n\nThe 7” color touch screen simplifies operation with wizard-based programming. Recall up to 50 jobs stored in memory or create new jobs with ease. Load documents and envelopes, press start and the DS-75i automatically measures the materials and sets itself up for easy operation.\n\nProductivity\n\nContinuously feed up to 975 documents using three standard feeders in cascading mode. Increase capacity to 1200 sheets with an optional high-capacity feeder. Utilize the vertical stacker for quick unloading of filled envelopes.\n\nVersatility\n\nDocument feeders accommodate a wide variety of material combinations from full sheets to short inserts. This flexible and scalable inserter is available in three configurations and designed to fit perfectly into any work environment.\n\nAccuracy\n\nExclusive feeder technology prevents double document errors. The barcode scanner reads codes, printed anywhere on the document, allowing you to process variable-page document sets and selectively include enclosures with absolute accuracy.","Capacity\nAs many as 3,800 documents per hour (63/minute)\nUp to 40,000 finished envelopes per month.\n\nDocument Handling\nHandles #10 and 6” x 9.5” envelopes\nFold up to 10 pages if single folded, or 8 pages letter folded (20 lb.)\n\nSystem Dimensions\n50”L x 20”D x 29”H\nBased on 3 feeders with catch tray.",null,"https://www.neopostusa.com/folder-inserters/DS-75i","https://www.youtube.com/watch?v=FjheOiCorFU","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo16566_ds75i_broch_hq.pdf","Yes","Yes"]
[null,null,"DS-85 Folder Inserter","Optimize mail assembly and process up to 60,000 envelopes per month\n\nThe DS-85 folding inserting system has the technology needed to handle a wide variety of business mailings at speeds up to 4,000 finished envelopes per hour. It will help you efficiently process checks, multi-page invoices, letters, legal-size documents, inserts and business reply envelopes. The optional scanner can read barcodes allowing you to collate and process multi-page document sets quickly and easily.\n\nSimplify folding and inserting of documents and get communications out faster\n\nEase of Use\n\nThe 5.7” reversible color touch screen and wizard-based programming simplify operation. Recall up to 25 stored jobs or create new jobs with ease. Load documents and envelopes, press start and the DS-85 automatically measures the materials and sets itself up for easy operation.\n\nProductivity\n\nContinuously feed up to 1,950 documents without reloading, by using multiple feeders in cascade mode. Increase processing capacity to 2,400 sheets with two optional high-capacity feeders. Utilize the integrated vertical stacker for quick unloading of filled envelopes.\n\nVersatility\n\nDocument feeders accommodate a wide variety of material combinations from full sheets to short inserts. This scalable folder inserter, with multiple productivity enhancing finished envelope exit options, is designed to grow to meet the expanding needs of your mail center.\n\nAccuracy\n\nExclusive technology prevents double document errors. Barcode scanning technology reads codes anywhere on the documents, allowing for flexible document layout. Process variable-page document sets and selectively include enclosures with absolute accuracy.","Capacity\nAs many as 4,000 documents per hour (66/minute)\nUp to 60,000 finished envelopes per month.\n\nDocument Handling\nHandles #10 and 6” x 9.5” envelopes\nSingle fold up to 10 pages, or up to 8 pages if letter folded (20 lb.)\n\nSystem Dimensions\n72”L x 16.5”D x 36.5”H\nBased on 6-stations",null,"https://www.neopostusa.com/folder-inserters/ds-85","N/A","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo14770_ds85_brochupdate_hq.pdf","Yes","Yes"]
[null,null,"DS-90i Folder Inserter","Collate, fold and insert up to 80,000 envelopes per month\n\nAt speeds of up to 4,300 envelopes per hour, the DS-90i folding inserting system has the technology needed to handle your business mailings. It processes checks, multi-page invoices, letters, legal-size documents, inserts and business reply envelopes. The optional scanner can read a broad range of optical marks and barcodes allowing you to efficiently process multi-page documents.\n\nEasily and efficiently automate the preparation of business documents\n\nEase of Use\n\nThe 10.4” reversible color touch screen and wizard-based programming simplify operation. Recall up to 50 stored jobs or create new jobs with ease. Load documents and envelopes, press start and the DS-90i automatically measures the materials and sets itself up making operation easy.    \n\nProductivity\n\nContinuously feed up to 1,950 documents without reloading by using multiple feeders in cascade mode. Increase processing capacity to 2,400 sheets with two optional high-capacity feeders. Utilize the integrated vertical stacker for quick unloading of filled envelopes.\n\nVersatility\nVERSATILITY\n\nDocument feeders accommodate a wide variety of material combinations from full sheets to short inserts. This scalable folder inserter, with multiple productivity enhancing finished envelope exit options, is designed to grow to meet the expanding needs of your mail center.\n\nAccuracy\nACCURACY\n\nExclusive technology prevents double document errors. Barcode scanning technology reads codes anywhere on the documents, allowing for flexible document layout. Process variable-page document sets and selectively include enclosures with absolute accuracy.","Capacity\nAs many as 4,300 documents per hour (71/minute)\nUp to 80,000 finished envelopes per month\n\nDocument Handling\nHandles #10 and 6” x 9.5” envelopes\nSingle fold up to 10 pages, or up to 8 pages if letter folded (20 lb.)\n\nSystem Dimensions\n59”L x 16.5”D x 36.5”H\nBased on 4-station configuration",null,"https://www.neopostusa.com/folder-inserters/ds-90i","https://www.youtube.com/watch?v=h0v6f4M1vFo","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo15095_ds_90i_broch_hq.pdf","Yes","Yes"]
[null,"High Volume"]
[null,null,"DS-180i Folder Inserter","Fold and insert up to 180,000 envelopes per month\n\nQuickly assemble your invoices and include personalized inserts using the double insert feeder. High-capacity document and envelope feeders combine with fast multi-sheet collation to maximize the productivity of your mail assembly process. Automated job changeover and an infinite number of preset jobs combine to ensure the versatility and ease of use of the DS-180i.\n\nMaximize mail center productivity and get the mail to your customers faster\n\nEase of Use\n\nThe 22” color touch screen and wizard-based programming simplify operation. Infinite memory capacity allows you to store all of your pre-programmed jobs for easy recall. Automatic system set up guarantees fast and easy job changeover while predictive intelligence estimates when your job will be complete.\n\nProductivity\n\nProcess filled envelopes at speeds up to 5,500 per hour with the DS-180i. Continuously feed up to 1,500 sheets or 400 inserts without reloading, by using multiple feeders in cascade mode. Collate up to two sheets at speeds up to 4,700 mail pieces per hour.\n\nVersatility\n\nDocument feeders accommodate a wide variety of material combinations from sheets up to 16” long to short inserts. Single fold or letter fold up to 8 sheets. This scalable folder inserter is designed to grow to up to 17 feed stations to meet the expanding needs of your mail center.\n\nAccuracy\n\nExclusive technology prevents double document errors. Barcode scanning technology reads codes anywhere on the documents, allowing for flexible document layout. Process variable-page document sets and selectively include enclosures with absolute accuracy.","Capacity\nAs many as 5,500 documents per hour (91/minute)\n\nUp to 150,000/180,000 finished envelopes per month\n\nDocument Handling\nHandles #10 and 6” x 9.5” envelopes\nFold up to 8 pages single or letter folded (20 lb.)",null,"https://www.neopostusa.com/folder-inserters/ds-180i","N/A","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo17682_ds180i_broch_singlepages_hq.pdf","Yes","Yes"]
[null,null,"DS-200i Folder Inserter","Process flats, booklets and everything in between\n\nDesigned to meets the workflow demands of almost every mailing application, the DS-200i is equipped with features to enhance finished document production. High capacity feeders and cascade feeding allow for continuous operation, without having to stop to reload. Intuitive color interface and unlimited job storage capacity enhance workflow programming. Sorting modules automatically send finished envelopes to up to three separate exits, based on criteria you define. Seamlessly meter your mail in one continuous operation by automatically transporting envelopes from the inserter’s exit into your mailing system.\n\nOptimize Mail Assembly and Maximize Mail Center Productivity\n\nEase of Use\n\nThe 22” color touch screen and wizard-based programming simplify operation. Unlimited memory capacity allows you to store all of your pre-programmed jobs for easy recall. Automatic system set up guarantees fast and easy job changeover, while predictive intelligence estimates when your job will be complete.\n\nProductivity\n\nProcess flats at speeds up to 3,000 per hour and #10 envelopes at 5,000 per hour. Continuously feed up to 2,000 sheets without reloading, by using multiple feeders in cascade mode. Eliminate human intervention and get envelopes out the door faster with optional postage meter interface.\n\nVersatility\n\nDocument feeders accommodate a wide variety of material combinations from sheets up to 16” long to short inserts. Process variable page document sets of up to 50 pages. Insert into either flats or standard business envelopes. Expandable up to 11 feed stations and available with up to three exits to meet your needs.\n\nAccuracy\n\nExclusive technology prevents double document errors. Barcode scanning reads codes anywhere on the documents, allowing for flexible document layout. Process variable-page documents sets and selectively include enclosures with absolute accuracy. Add optional AIMS software to optimize mail piece integrity and security.","Capacity\nAs many as 5,000 #10 envelopes per hour (80/minute)\nAs many as 3,000 9”x12” flats per hour (50/minute)\n\nUp to 200,000 finished envelopes per month.\n\nDocument Handling\nHandles 9”x12”, 10”x13” flats landscape, #9, #10, and 6” x 9.5” envelopes\nFold up to 8 pages single or letter folded (20 lb.)\n\nSystem Dimensions\n107”L x 25” D x 36”H\n\nBased on 3-station configuration",null,"https://www.neopostusa.com/folder-inserters/ds-200i","https://www.youtube.com/watch?v=RsO3Bn6QntQ","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo17684_ds200i_broch_hq.pdf","Yes","Yes"]
[null,null,"DS-600i Folder Inserter","Fold and insert up to 300,000 envelopes per month\n\nEliminate the need for window envelopes and ensure the privacy of important customer or patient information. Inline envelope printing enhances customer information and security. Each personalized document is recorded by the folder inserter and a single secure system prints the recipients name and address on a closed-face envelope. \n\nDesigned to meet the workflow demands of almost every application, the DS-600i also has the ability to process flats efficiently.\n\nPC-driven folder inserter technology maximizes\nthe productivity of your mail center.\n\nEase of Use\n\nThe widescreen color touch screen and wizard-based programming simplify operation. Infinite memory capacity allows you to store preprogrammed jobs for easy recall. Automated system set up guarantees fast and easy job changeover while predictive intelligence estimates when your job will be complete.\n\nProductivity\n\nAssemble mailings at speeds of up to 6,000 pieces per hour. Advanced accumulation speed, the ability to process flats with up to 72 pages and booklets up to 6 mm maximum output. Inline printing and metering are available to optimize your mail assembly process.\n\nVersatility\n\nDocument feeders accommodate a wide variety of material combinations from sheets up to 16” to inserts as small as 3x5”. It can also fold up to 8 sheets single or letter fold. This scalable folder inserter is designed to grow to up to 11 feed stations to meet your needs as they expand.\n\nAccuracy\n\nExclusive technology prevents double document errors. Barcode scanning technology reads codes anywhere on the documents, allowing for flexible document layout. Process variable-page document sets and selectively include enclosures with absolute accuracy.","Capacity\nAs many as 6,000 documents per hour (75/minute)\nUp to 300,000 finished envelopes per month\n\nDocument Handling\nHandles #10, 6” x 9.5, 9” x 12”, 10” x 13” envelopes\nFold up to 8 pages single or letter folded (20 lb.)\n\nSystem Dimensions\n104”L x 25”D x 59”H\nBased on 1 feeder plus tower folder and furniture.",null,"https://www.neopostusa.com/folder-inserters/ds-600i","https://www.youtube.com/watch?v=7JBNpb3WsdY","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo16602_ds600i_broch_10.pdf","Yes","Yes"]
[null,null,"DS-1200 G4 Folder Inserter","Automatically assemble up to 800,000 envelopes per month\n\nWhether you’re processing invoices, personalized direct mail, or highly confidential financial documents into envelopes or flats, the DS-1200 is the ideal solution. Frequent application changeovers or small job runs are quick and easy with a simple touch of a button. Each job is programmed using the graphical touch screen, and most job changes are completed in less time than it takes to load the materials. The simplicity of user controls ensures that set-up time is reduced to seconds rather than hours, significantly reducing the need for a dedicated operator and on-site support.\n\nIntegrated System Integrity Ensures Mailpiece Accuracy\n\nEase of Use\n\nIntegrated 19” color touch screen and wizard-based programming minimizes operator training. Automatic system setup guarantees fast and easy job changeover. Each feeder automatically calibrates to the new job. Flat paper transport path provides clear access to all documents maximizing productivity.\n\nProductivity\n\nProcess envelopes at speeds up to 12,000 per hour. High capacity feeders can be loaded-on-the-fly. Mobile document trolleys load directly from a printer while the system is running. Process #10, 6” x 9.5”and flat envelope jobs simultaneously, increasing efficiency and throughput.\n\nVersatility\n\nThe folder inserter is expandable to 16 feed stations and available with multiple output options. Document feeders accommodate a wide variety of material combinations from sheets up to 16” long to short inserts. The system can dynamically select the envelope size based on the page count, control marks or electronic file controls.\n\nAccuracy\n\nBarcode scanning technology reads codes anywhere on the documents, allowing for flexible document layout. The IMOS operating system electronically records the movement of each document being inserted. Neopost’s optional AIMS software ensures closed-loop verification and that each piece was successfully and accurately processed.","Capacity\nAs many as 12,000 documents per hour (200/minute)\nAs many as 32,000 documents per hour (533/minute)\nUp to 800,000 finished envelopes per month.\n\nDocument Handling\nHandles 9”x12”, 10”x13” flats landscape, #9, #10, and 6” x 9.5” envelopes\nFold up to 10 pages single or letter folded (20 lb.)\n\nOperational Efficiency\nUnlimited job memory\nAutomatic job change\nMobil trolley system from printer\nMailing system interface\nInline dynamic envelope printer",null,"https://www.neopostusa.com/folder-inserters/ds-1200-g3","https://www.youtube.com/watch?v=KQC6Ws7aLhs","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo15065_ds1200g3_broch_hq.pdf","Yes","Yes"]
["Letter Openers"]
[null,null,"IM-30 Mail Opener","A Fast and Secure Solution for Opening and Extracting Your Incoming Mail\n\nNeopost's range of mail opener and extractors handle mixed mail sizes and extract the contents for immediate processing while protecting contents and preserving document integrity.","Processing Speed: 2,000 - 2,400  envelopes per hour\nEnvelope Height: 3.3\" - 6.5\"\nEnvelope Width: 5.5\" - 10.2\"\nEnvelope Thickness: .16\"",null,"https://www.neopostusa.com/letter-openers","N/A","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/im-30_product_sheet_0.pdf","Yes","Yes"]
[null,null,"IM-16C Mail Opener",null,"Processing Speed: As many as 18,000 envelopes per hour, 300 per minute\nEnvelope Height: 5.5\" - 13\"\nEnvelope Width: 3.5\" - 10.2\"\nEnvelope Thickness: 4 mm",null,null,null,"https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/im-16c_product_sheet_0.pdf","Yes","Yes"]
[null,null,"IM-35 Mail Opener",null,"Processing Speed: 2,000 - 2,400  envelopes per hour\nEnvelope Height: 3.3\" - 6.5\"\nEnvelope Width: 5.5\" - 10.2\"\nEnvelope Thickness: .16\"",null,null,null,"https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/im-35_product_sheet.pdf","Yes","Yes"]
[null,null,"IM-2112 Mail Opener",null,"Processing Speed: 24,000 envelopes per hour, 400 per minute\nEnvelope Size: Any (including overnight packs)\nEnvelope Thickness: 4.8mm",null,null,null,"https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/im-2112_product_sheet_0.pdf","Yes","Yes"]
[null,null,"IM-306 Mail Opener",null,"Processing Speed: 40,000 envelopes per hour\nEnvelope Size: Lengths as long as 13.5\" (including overnight packs)\nEnvelope Thickness: .5\"",null,null,null,"https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/im-306_product_sheet_0.pdf","Yes","Yes"]
["Postage Meters","Low Volume"]
[null,null,"IS-280 iMeter Postage Meter","Perfect for small office and home office mailing\n\nNo more waiting in line at the Post Office™ or overpaying with stamps. The IS-280 is designed for offices which run small amounts of mail, yet want the convenience and benefits of mailing with a postage meter.\n\nA user-friendly rate wizard simplifies the process of selecting the correct mail class and the accurate postal rate with simple, step-by-step instructions.\n\nOne simple solution for both mailing and shipping\n\nPRODUCTIVITY\n\nGoing to the post office is a thing of the past. With the IS-280, simply insert your envelope, postcard, or label, to print the exact postage you need on each item. Refilling postage funds, downloading the latest USPS® rates or feature upgrades for your system has never been easier. Simply connect the postage meter using either a dedicated Internet connection or iMeter™ PC Link.\n\nVERSATILITY\n\nPersonalize your mail pieces with an image, logo or message using NeoSlogan. Select from a library of over 100 stock images or create your own in minutes. Ship directly from your desktop with NeoShip and ensure full IM®pb compliance for all your USPS packages.\n\nEASE OF USE\n\nNever guess the weights of the items you are mailing. With a standard 2 lb. or optional 5 lb. scale, the IS-280 ensures you know the correct weight to prevent over posting. The Rate Wizard simplifies the process of selecting the correct postal class and rate. Shortcut keys save time by providing instant job set up.\n\nCOST CONTROL\n\nPay just 46 cents (3 cent savings) for First-Class postage, access Commercial Base Pricing for USPS shipments using NeoShip online shipping software, and enjoy the benefits of electronic rate discounts when using our e-Services application. Each IS-280 comes standard with NeoStats postage expense reporting.","Performance\nProcessing speed up to 18 mail pieces per minute\nTrack postage spending for up to ten departments (1 dept. standard, 5 or 10 depts. optional)\n\niMeter Apps\nPostal Rates App\nOnline Postal Expense Manager™ App\nE-Services App\nE-Services with Electronic Return Receipt App\nNeoFunds® App\n\nMaterial Handling\nPostcards, letters and small packages\n\nSystem Dimensions\n13”L x 9”D x 8”H",null,"https://www.neopostusa.com/equipment/postage-meters/is-280","https://www.youtube.com/watch?v=EYl4cnOLVxU","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo14891_is_280_broch_hq.pdf","Yes","Yes"]
[null,null,"IN-360 Postage Meter","The ideal solution for small office mailing and shipping\n\nDesigned for businesses with lower mail volume, the IN-360 has an optional differential weighing feature that allows you to easily and efficiently process envelopes of different sizes and shapes.\n\nEach time an envelope is removed from the weighing platform, the power feeder automatically starts and is ready to process mail with the correct amount of postage.\n\nOne simple solution for both mailing and shipping\n\nProductivity\n\nSmoothly process batches of mail at the rate of 45 letters per minute. Simply insert your mail piece and print the exact postage you need. Refilling postage funds, downloading the latest USPS® rates or feature upgrades for your system has never been easier. Simply connect the postage meter using either a dedicated Internet connection or analog line.\n\nVersatility\n\nPersonalize your mail pieces with an image, logo or message using NeoSlogan. Select from a library of over 100 stock images or create your own in minutes. Ship directly from your desktop with NeoShip and ensure full IM®pb compliance for all your USPS packages.\n\nEase of Use\n\nNever guess the weights of the items you are mailing. With a standard 5 lb. or optional 10, 30, or 70 lb. external weighing platform, the IN-360 ensures you know the correct weight, to prevent over posting. The Rate Wizard simplifies the process of selecting the correct postal rate and class and rate. Shortcut keys save time by providing instant job set up.\n\nCost Control\n\nPay just 46 cents (3 cent savings) for First-Class postage, access Commercial Base Pricing for USPS® shipments using NeoShip online shipping software, and enjoy the benefits of electronic rate discounts when using our e-Services application. Each IN-360 comes standard with NeoStats postage expense reporting.","Performance\nProcessing speed up to 45 mail pieces per minute\nTrack postage spending for up to 300 departments (30 dept. standard, 100 or 300 depts. optional)\n\niMeter Apps\nPostal Rates App\nOnline Postal Expense Manager™ App\nE-Services App\nE-Services with Electronic Return Receipt App\nNeoFunds® App\n\nMaterials Handling\nPostcards, letters and small packages\nMinimum: 3.5” x 5”\nMaximum: 10” x 13”\nThickness: Up to 3/8”\n\nSystem Dimensions\n10”L x 17”D x 11”H\nBase w/integrated feeder and catch tray: 29”L x 17”D x 11”H",null,"https://www.neopostusa.com/postage-meters/in-360","https://www.youtube.com/watch?v=xIJfbtlqud0","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo14828_in_360_broch_hq.pdf","Yes","Yes"]
[null,"Mid Volume"]
[null,null,"IN-600 Series Mailing Systems","The postage machine designed for any mailroom environment\n\nIdeal for mid-level mail volume, the IN-600 Series is available in two models, power-assisted hand feed (IN-600 HF) or with auto-feed technology (IN-600 AF). With the IN-600 Series, you have access to a suite of services and apps to improve postal, parcel and related digital communications.\n\nBoth mailing and shipping in one versatile solution\n\nPRODUCTIVITY\n\nProcess batches of mail at a rate of 110 letters per minute with the IN-600 AF (75 lpm with IN-600 HF). Feed your mail piece and print the exact postage you need. Refilling postage funds, downloading the latest USPS® rates or feature upgrades for your system has never been easier.\n\nVersatility\n\nEquipped with an external weighing platform which meets your specific needs, the IN-600 Series ensures you know the exact weight of every piece and ensures you never over-post. Personalize your mail pieces with an image, logo or message using NeoSlogan. Ship directly from your desktop with NeoShip and ensure full IM®pb compliance for all of your USPS packages.\n\nEase of Use\n\nThe Rate Wizard simplifies the process of selecting the correct mail class and postal rate. Shortcut keys save time by providing instant job set up. Save time using the optional barcode scanner to load departments or to process e-Services.\n\nCost Control\n\nPay just 46 cents (3 cent savings) for First-Class postage, access Commercial Base Pricing for USPS shipments using NeoShip online shipping software, and enjoy the benefits of electronic rate discounts when using our e-Services application. The IN-600 Series even comes standard with NeoStats Basic postage expense reporting.","Performance\nProcessing speed up to 75 mail pieces per minute (IN-600 HF)\nProcessing speed up to 110 mail pieces per minute (IN-600 AF)\nTrack postage spending for up to 300 departments (35 dept. standard, 100 or 300 depts. optional)\n\niMeter™ Apps\nPostal Rates App\nOnline Postal Expense Manager™ App\nE-Services App\nE-Services with Electronic Return Receipt App\nNeoFunds® App\n\nSystem Dimensions\n33”L x 15”D x 12”H (IN-600 HF)\n50”L x 15”D x 12”H (IN-600 AF)\n\nMaterials Handling\nPostcards, letters and small packages\nMinimum: 3.5” x 5”\nMaximum: 10” x 13”\nThickness: Up to 3/8” (IN-600 HF)\nThickness: Up to 1/2” (IN-600 AF)",null,"https://www.neopostusa.com/postage-meters/in-600","https://www.youtube.com/watch?v=F5KI72V_7Qk","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo16327_in_600_broch_hq.pdf","Yes","Yes"]
[null,null,"IN-610 Mailing System powered by RunMyMail","All-in-one touch screen for convenient mailing, shipping and accounting\n\nProcess outgoing mail and parcels faster and more efficiently than ever before. The IN-610 transforms the user experience by centralizing all mail center operations into one workstation with a large touch screen display.Expedite mail processing operations with the touch of a finger\n\nEASE OF USE\n\nA large interactive display streamlines operation and reduces the equipment footprint. RunMyMail takes all the traditional mailing system controls and applies them to an all-in-one interactive PC. The IN-610 gives you the power to process batches of mail at a rate of 110 letters per minute and parcels faster and easier than ever before.\n\nVERSATILITY\n\nCreate USPS® IM®pb-compliant labels and ship packages directly from the IN-610 with optional NeoShip software. Monitor, track and control postage costs with optional NeoStats postage expense reporting application. Personalize your mail pieces with an image, logo or message using NeoSlogan.","Performance\nProcessing speed up to 110 mail pieces per minute\nTrack postage spending for up to 300 departments (35 dept. standard, 100 or 300 depts. optional)\n\niMeter Apps\nPostal Rates App\nOnline Postal Expense Manager™ App\nE-Services App\nE-Services with Electronic Return Receipt App\nNeoFunds App\n\nMaterials Handling\nPostcards, letters and small packages\nMinimum: 3.5” x 5”\nMaximum: 10” x 13”\nThickness: Up to 1/2”\n\nSystem Dimensions\n50”L x 15”D x 12”H\n60” custom table available",null,"https://www.neopostusa.com/products/postage-meters/in-610-mailing-system","https://www.youtube.com/watch?v=yQ6FA9DWkj4","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo16036_in610_broch_hq.pdf","Yes","Yes"]
[null,null,"IN-700 Series Mailing Systems","Maximize control of shipping and mailing operations\n\nIdeal for mid-level mail volume, the IN-700 Series is available with two different processing speeds to meet the demands of your mailing operations. With the IN-700 Series, you have access to a suite of apps and services to improve postal, parcel and related digital communications.\n\nBoth mailing and shipping in one versatile mailing system\n\nPRODUCTIVITY\n\nProcess batches of mail at the rate of 140 letters per minute with the IN-700 (75 lpm in dynamic weighing mode) and 175 lpm with the IN-750 (110 lpm in dynamic weighing mode). Feed your mail piece and print the exact postage you need. Refilling postage funds, downloading the latest USPS® rates or feature upgrades for your system has never been easier.\n\nVERSATILITY\n\nThe IN-700 Series ensures you know the exact weight of every piece so that you never over post. Personalize your mail pieces with an image, logo or message using NeoSlogan. Ship directly from your desktop with NeoShip and guarantee full IM®pb compliance for all of your USPS packages.\n\nEASE OF USE\n\nNavigation is a breeze with the color touch screen display, descriptive prompts and menus. The Rate Wizard simplifies the process of selecting the correct mail class and postal rate. Shortcut keys save time by providing instant job set up. Increase efficiency by using the optional barcode scanner for department or tracking number input.\n\nCOST CONTROL\n\nPay just 46 cents (3 cent savings) for First-Class postage, access Commercial Base Pricing for USPS shipments using NeoShip online shipping software, and enjoy the benefits of electronic rate discounts when using our e-Services application. IN-700 Series even comes standard with NeoStats to help you accurately report on each penny of postage spent.","Performance\nIN-700-Processing speed up to 140 mail pieces per minute/ 75 with Dynamic Scale\nIN-750-Processing speed up to 175 mail pieces per minute/110 with Dynamic Scale\n\nTrack postage spending for up to 500 departments (70 dept. standard, 100, 300 or 500 depts. optional)\n\niMeter Apps\nPostal Rates App\nOnline Postal Expense Manager™ App\nE-Services App\nE-Services with Electronic Return Receipt App\nNeoFunds® App\n\nMaterials Handling\nPostcards, letters and small packages\nMinimum: 3.5” x 5”\nMaximum: 10” x 13”\nThickness: Up to 5/8”\n\nSystem Dimensions\n50”L x 18”D x 13”H with catch tray (no DWP)\n\n67”L x 18”D x 13”H with dynamic scale and catch tray",null,"https://www.neopostusa.com/postage-meters/in-700","https://www.youtube.com/watch?time_continue=2&v=na0CWIZZCj8","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo16328_in_700_broch_rev_hq.pdf","Yes","Yes"]
[null,null,"IN-710/760 Mailing Solutions powered by RunMyMail","Mailing, shipping and accounting from one centralized workstation\n\nThe IN-710/760 transforms the user experience by centralizing all mail center operations into one workstation with a large touch screen display allowing you to process outgoing mail and parcels faster and more efficiently than ever before. For added productivity, the optional dynamic scale can weigh, rate and classify mail at speeds of up to 75 lpm (IN-710) and 110 lpm (IN-760).\n\nExpedite mail processing with the touch of your finger\n\nEASE OF USE\n\nA large interactive display streamlines operation and reduces the equipment footprint. RunMyMail takes all the traditional mailing system controls and applies them to an all-in-one interactive PC. With this powerful system, mail is processed at 140 letters per minute (IN-710) or 175 lpm (IN-760) and parcels can be sent both faster and easier than ever before.\n\nVERSATILITY\n\nCreate USPS® IM®pb-compliant labels and ship packages directly from the mailing system with optional NeoShip software. Monitor, track and control postage costs with the optional NeoStats postage expense reporting application. Personalize your mail pieces with an image, logo or message using NeoSlogan.","Performance\nIN-710/760:\nProcessing speed: 140/175 mail pieces per minute\nDynamic weighing speed: up to 75/110\nTrack postage spending for up to 500 departments (70 dept. standard, 100 or 300 depts. optional)\n\niMeter Apps\nPostal Rates\nOnline Postal Expense Manager™ \nE-Services \nE-Services with Electronic Return Receipt\nNeoFunds\n\nMaterials Handling\nPostcards, letters and small packages\nMinimum: 3.5” x 5”\nMaximum: 10” x 13”\nThickness: Up to 5/8”\n\nSystem Dimensions\n50”L x 18”D x 13”H with catch tray (no DWP)\n67”L x 18”D x 13”H with dynamic scale and catch tray\n84” custom table available",null,"https://www.neopostusa.com/products/postage-meters/in-710-760","https://www.youtube.com/watch?v=h4pkFz9E-Kg","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo1608_in710_760_broch_hq.pdf","Yes","Yes"]
[null,"High Volume"]
[null,null,"IS-5000/6000 Mailing Systems","Meter your mail at up to 300 pieces per minute\n\nDesigned with the operator in mind, all mailing operations are controlled from the same area, creating the ideal ergonomic process and increased mail finishing speed. Automatically weigh, measure, rate, seal, meter and stack large stacks of mail in minutes. Whether you’re sending trays of envelopes, postcards, large envelopes, or mixed weight mail, you can depend upon these systems to help you get it done quickly and efficiently.\n\nA dependable, high volume mailing system you can rely on\n\nProductivity\n\nHigh-capacity mixed mail feeder, optional dynamic scale, and conveyor combine to allow throughput of up to 300 mail pieces per minute. Large stacks of mixed size mail are quickly and efficiently sealed and metered.\n\nVersatility\n\nAvailable with either a 5.7” or large 15” color display, dynamic scale, power conveyor stacker, and many time saving options and apps, the IS-5000 or IS-6000 can be configured to meet your specific mailing needs.\n\nEase of Use\n\nErgonomic design includes a color touch screen repositionable interface to ensure efficient operation. New postal rates are automatically downloaded, and email alerts let you know when it’s time to reorder ink.\n\nCost Control\nCOST CONTROL\n\nAccurately account for all postage spent for up to 500 departments. Manage all mailing and shipping activities and reduce costs with EMS, Neopost’s multi-carrier shipping and mail accounting solution.","Performance\nProcessing speed up to 210, 260 or 300 mail pieces per minute\nDynamically weigh, measure and rate up to 180 pieces per minute\nDual-pump Jet-spray seals envelopes with flaps open or closed\nMixed Mail Feeder processes mixed size and weight mail\n\nScreen Size\nIS-5000 – 5.7” repositionable color touch screen display\nIS-6000 - 15” repositionable color touch screen display\n\nInk System\nUltra-high capacity ink tank prints up to 100,000 impressions/tank\nPermanent print head lasts the life of the system\n\nSystem Dimensions\nMailing system with catch tray - 58”L x 25”D x 14”H\nOptional Dynamic scale - 20”L x 25”D x 14”H\nOptional Power Conveyor Stacker - 40”L x 14”D x 12”H",null,"https://www.neopostusa.com/postage-meters/is-5000-6000","https://www.youtube.com/watch?v=IKY1ZSaLWGY","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo15050_is_5000_broch_hq_v2.pdf","Yes","Yes"]
[{"$nulls":8},"https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo14869_is_6000_broch_hq2_0.pdf","Yes","Yes"]
[null,null,"IJ-15K Digital Mailing System","High-Performance Digital In-Line Metering System\n\nThe Neopost IJ-15K is a specially designed, high-volume metering system that has the ability to connect in-line to production inserters.\n\nDesigned specifically to connect in-line to production inserters\nDelivers high productivity levels, state-of-the art serviceability and low cost of ownership\nSmoothly handles same or mixed weight mail at speeds of up to 15,000 per hour\nFreestanding status light tower allows you to monitor system status from a distance\nSeparate print head and 350ml hot-swappable reservoir for easy ink management\nAn intuitive touchscreen operating panel puts all system controls at your fingertips","Performance\nUp to 15,000 envelopes per hour (single and mixed-weight)\n\nAutomatic Label Dispenser\nBuilt-in\n\nInk Reservoir Capacity\n350 ml  \n\nProgrammable Jobs\n10\n\nSize\n13”L x 18”D x 14”H\n\nEnvelope Dimensions\nMinimum Length: 5” - 5”\nMaximum Width:  3.5” - 12”\nThickness: Up to 5/8”\nOrientation: Landscape",null,"https://www.neopostusa.com/postage-meters/ij-15k","N/A","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/ij-15k_product_sheet.pdf","Yes","Yes"]
["Tabbing Systems"]
[null,null,"TA-12 Tabbing System","Send mail that does not require the use of envelopes\n\nNeopost offers a versatile range of tabbers that can apply one, two or three tabs or wafer seals in single or multiple passes. These systems can work either in-line with existing mail processing equipment or as stand-alone units.","TA-12\nAs many as 12,000 tri-folds per hour\nAccepts tabs from 5/8” to 1.5”\nAccepts product as thick as 5/32”\nHandles media from 3” x 5” to 17” x 18”",null,"https://www.neopostusa.com/tabbing-systems","N/A","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/ta-12_product_sheet_0.pdf","Yes","Yes"]
[null,null,"TA-20 Tabbing System",null,"TA-20\nAs many as 20,000 single tabs per hour\nApplies as many as three tabs in a single pass\nHandles media from 3” x 5” to 13” x 17”\nFour programmable job settings",null,null,null,"https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/ta-20_product_sheet_0.pdf","Yes","Yes"]
[null,null,"TA-25 Tabbing System",null,"TA-25\nAs many as 25,000 tri-folds per hour\nSide-to-side tabbing as many as 15,000 letter-size booklets per hour\nStamping as many as 20,000 #10 envelopes per hour",null,null,null,"https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/ta-25_product_sheet_0.pdf","Yes","Yes"]
[null,null,"TA-30 Tabbing System",null,"TA-30\nAs many as 35,000 tri-folds per hour\nApplies as many as three tabs in a single pass\nHandles media from 3” x 5” to 13” x 17”\nFour programmable job settings",null,null,null,"https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/ta-30_product_sheet.pdf","Yes","Yes"]
["Packcity - Intelligent Parcel Lockers"]
[null,null,"Packcity - Intelligent Parcel Lockers","Automated Electronic Intelligent Lockers for Convenient Parcel Pick Up and Drop Off\n\nHaving Packcity intelligent lockers on campus alleviates crowded mailrooms and eliminates multiple delivery attempts. Consumers can pick up packages on their time — anytime.\n\nHow does it work?\n\nA delivery notification is sent via text or email when the parcel arrives.\nThe recipient enters their one-time PIN code.\nThe door opens for recipient to grab their parcel and go.\n\nLots of packages piling up? PackCity is the solution\n\nCONVENIENT\n\nNo more waiting for the mail center to open; packages are available for easy retrieval 24/7.\n\nSECURE\n\nPackcity logs every drop off and pickup: 100% chain of custody with sturdy, steel-construction lockers.\n\nREDUCES LABOR\n\nFewer resources are required for parcel management, distribution and pick up. Plus, you’ll have complete tracking visibility.\n\nCUSTOMIZABLE\n\nAdd your company’s logo and adjust the size of the lockers based on the space and needs of your business.",null,null,"https://www.neopostusa.com/software/shipping-and-tracking-solutions/packcity","https://www.youtube.com/watch?v=MtYrwXacEqk","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo16048_pckcty_prcllckrs_cutsht_hq.pdf","Yes","Yes"]
["Mail Center Furniture"]
["https://www.neopostusa.com/equipment/mail-center-furniture",{"$nulls":8},"No","Not Yet"]
["Shredders"]
["https://www.neopostusa.com/shredders",{"$nulls":8},"No","Not Yet"]
["Cutters"]
[null,null,"DS-10MCTTR Paper Cutter","Guillotine cutter accurately cuts through paper stacks up to 3.15” high, up to 18.7” wide\nLED laser cut line delivers pinpoint accuracy\nHigh-quality steel blade easily slices through paper stacks\nFront and rear transparent covers ensure operator safety\nManual lever cutting arm and geared clamping system guarantees ease of use\nSpindle-guide back gauge crank and calibrated scale for fine adjustments",null,null,"https://www.neopost.com/equipment/paper-cutters","N/A","https://www.neopost.com/sites/neopost.com/files/files/Neopost_DS-10MCTTR_Document_Cutter.pdf","Yes","Yes"]
[null,null,"DS-20SCTTR Paper Cutter","Guillotine cutter accurately cuts through paper stacks up to 1.75” high, up to 16.9” wide\nSemi-automatic with electronically-controlled two hand operation\nLED laser cut line delivers pinpoint accuracy\nHigh-quality hardened steel blade easily slices through paper stacks\nSpindle-guide back gauge crank and calibrated scale for fine adjustments\nElectronically-controlled front safety guard, transparent rear cover, safety lock with key, blade lock, external blade depth adjustment and automatic blade return from any position",null,null,"https://www.neopost.com/equipment/paper-cutters","N/A","https://www.neopost.com/sites/neopost.com/files/files/Neopost_DS-20SCTTR_Guillotine_Document_Cutter.pdf","Yes","Yes"]
["Pressure Sealers"]
[null,null,"DS-6KPS Pressure Sealer","Ideal mid-volume solution for processing one-piece, pressure-sensitive mailers\nDrop-in top feed system for dependable feeding of forms - no paper fanning required\nProcess forms up to 14” in length at speeds up to 100 forms per minute\nFold types include Z, C, uneven Z and C, half and custom folds\nEasy-adjust pre-marked fold plates make changing fold type or form size easy",null,null,"https://www.neopost.com/equipment/pressure-sealers","N/A","https://www.neopost.com/sites/neopost.com/files/files/Neopost_DS-6KPS_Pressure_Sealer_v2.pdf","Yes","Yes"]
[null,null,"DS-8KPS Pressure Sealer","Powerful mid-volume desktop solution for processing pressure-sensitive self-mailers\nDrop-in three roller feed system for dependable feeding of forms - no paper fanning\nProcess panel forms up to 14” in length at speeds up to 800 forms per hour\nFold types include C, Z, V, uneven C and Z and custom folds\nEasy-adjust pre-marked fold plates make changing fold type or form size easy",null,null,"https://www.neopost.com/equipment/pressure-sealers","N/A","https://www.neopost.com/sites/neopost.com/files/files/Neopost_DS-8KPS_Pressure_Sealer_v2.pdf","Yes","Yes"]
[null,null,"DS-16KPS Pressure Sealer","High-volume tabletop solution for processing pressure sensitive one-piece mailers\nDrop-in three roller feed system for dependable feeding of forms - no paper fanning\nAutomatically detects and adjusts for 11”, 14” and 17” forms\nLarge 2.8” backlit LCD display and user-friendly control panel for easy operation\nFive pre-programmedfolds for uneven C, V, Z and store up to 35 custom folds\nAdjustable feed table pressure enables smoother feeding of thick and thin paper stock",null,null,"https://www.neopost.com/equipment/pressure-sealers","N/A","https://www.neopost.com/sites/neopost.com/files/files/Neopost_DS-16KPS_Pressure_Sealer_v2.pdf","Yes","Yes"]
["Shredders"]
[null,null,"ProfiPack 425 Cardboard Perforator","Transform Used Cardboard Into High-Quality Packing Material\n\nThe Neopost ProfiPack 425 Cardboard Perforator by HSM instantly converts bulky used-cardboard containers into an all-purpose packaging material.\n\nFeatures one-cycle cutting and perforation\nFeatures special cutting roller geometry\nIncludes a measuring scale\nMeets all national and international safety standards",null,null,"https://www.neopost.com/shredders","N/A","N/A","Yes","Yes"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]

{"sheet":"Neopost Software","index":1,"n_rows":61,"n_cols":12,"rows_kept":61,"cut":false,"hidden":false,"merged":[[30,3,33,3],[23,3,26,3],[8,2,9,2],[8,3,9,3],[23,2,26,2],[36,6,37,6],[36,2,37,2],[36,3,37,3],[30,2,33,2],[30,4,33,4],[36,4,37,4],[25,4,26,4],[30,6,33,6],[30,7,33,7],[8,7,9,7],[8,9,9,9],[23,7,26,7],[8,6,9,6],[8,10,9,10],[23,6,26,6],[23,9,26,9],[30,9,33,9],[30,10,33,10],[23,10,26,10],[36,10,37,10],[36,9,37,9],[36,7,37,7]]}
["Category","Sub-Category (if applicable)","Product Name","Product Description","Specifications","Serial #","Vendor Site URL","Video Content URL(s)","Downloadable Content URL(s)","Pictures Saved?","Migrated?","Alternative Site URL"]
["Business Solutions"]
[null,null,"NeoReceipts by Shoeboxed","NeoReceipts: Turning Receipts into an Organized, IRS-compliant Online Archive\n\nReceipt Organization : Precise scanning, OCR and human data verification\nBusiness Card Management : Online contact lists exportable to CRM\nExpense Reports : Send expense reports with receipt images from anywhere.\nMileage Tracking : Use your phone’s built-in GPS for unmatched ease and accuracy\nTax Preparation : Online organization with IRS accepted receipt images\nMagic Envelopes : Fill prepaid envelopes with your piles of paper clutter\n\nGo Paperless with Accurate, Verified Data\n\nGet Perfectly Organized\n\nYour documents are automatically categorized and stored online. Create new categories or reuse existing ones. Documents are always available and easily retrievable online, at any time, from anywhere and on any device. Create reports in a few clicks.\n\nOptimize Your Tax Deductions\n\nGet IRS compliant images of your receipts that are securely stored and that you can retrieve at any time. Do not miss tax deductibles and spend less time preparing for taxes.\n\nTurn Paper into Verified Digital Data\n\nSave time by outsourcing the digitization and the verification of your paper receipts",null,null,"https://www.neopostusa.com/software/NeoReceipts-receipt-document-management","https://www.youtube.com/watch?v=H9YyzltlWRQ","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/shoeboxed_brochure_paper2data_2016.pdf","Yes","Yes"]
[null,null,"NeoBookkeeper by OneUp","NeoBookkeeper: Solving the Small Business Puzzle with Automated Accounting\n\nAn all-in-one online for small business to streamline, automate and simplify financial management. Access your business data anywhere, anytime, from any device.\n\nFocus on Your Core Business: Spend more time on your core business and engage with your customers – not your spreadsheets.\nAutomate Your Processes: Convert quotes into invoices, bills or delivery notes into sales orders. Synchronize your inventory real time. Reconcile bank accounts. By automating many aspects of your business, avoid duplicate entries and errors. Monitor your business with reliable dashboards, always in sync.\nAll Features Included and Customizable: Customize the solution based on your needs, use it from your mobile device and activate additional modules as you grow your business at no additional price.\n\nFrom One Place : Accounting, Invoicing, Inventory, Contact Management & more\n\nAll Features Included and Customizable\n\nCustomize the solution based on your needs. Activate modules as your business grows, at no additional price. Access data anywhere, anytime, on any device\n\nAutomate Your Processes\n\nConvert quotes into invoices. Match up bank payments with invoices and outgoing payments with the items and services you bought.\n\nFocus on Your Core Business\n\nSpend more time adding value to your core business. Engage with your customers, not your Spreadsheets!",null,null,"https://www.neopostusa.com/software/NeoBookkeeper-business-management-software","https://www.youtube.com/watch?time_continue=90&v=7OITCAwMywA","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/one_up_neopost_a1115.pdf","Yes","Yes"]
[null,null,"NeoSlogan","NeoSlogan, Personalized Communications in 3 Easy Steps\n\nPersonalize your mail pieces with NeoSlogan! From text messages to eye catching images and company logos, NeoSlogan customizes your mail pieces in minutes! \n\nAdding a slogan to your envelope is as simple as 1, 2, 3 ...\n\n1. Select your mailing system.\n2. Choose a slogan from the library or upload your own custom image.\n3. Download the slogan artwork to your mailing system.\n\nFor use with IM/IS/IN-Series mailing systems only.\n\nCreate Your Own Unique Slogan\n\nCommunicate Anytime With Your Customers before they Open the Mail\n\nNeoslogan is one of the many services available on MyNeopost for Mailing System customers. The service is available 24/24 and 7/7. The slogan is available for download with a very quick turn around and less than 2 hours for the slogans from library.\n\nPersonalize Mail Pieces and Boost Your Open Rates\n\nPersonalized envelopes drive customers’ attention and interest. With NeoSlogan it is really easy to customize your envelope and change the message regularly depending on season or the reason. Create eye catching images and messages in minutes\n\nHundreds of designs for any season and any reason\n\nA library with hundreds of free slogans to choose from, covering many categories including: seasons, events, business messages and more…",null,null,"https://www.neopostusa.com/software/postage-meter-software/create-a-slogan-for-your-postage-machine-online","https://www.youtube.com/watch?v=rbVjPsVXcYQ","N/A","Yes","Yes"]
[null,null,"NeoSendit","NeoSendit: Save even more time when using QuickBooks®\n\nNeoSendit is an easy-to-use solution to free up your time, and save you the hassle of everyday invoice management all without complex installation and manual labor.\n\nNeoSendit offers a seamless integration with QuickBooks that allows you to save more time when sending quotes, invoices or any documents from your accounting solution.\n\nFocus on your business priorities instead of your mailing process\n\nOne-stop-shop: Send and track your invoices, estimates, marketing documents and more via USPS mail all from your desktop computer.\nFaster repayment: As invoices are ready, conveniently send them via mail or email to receive payment faster.  \nFully customizable: Choose from various formatting, color and size options to adapt to your business’ needs.\nTime Management: Eliminate tedious, manual and time-consuming tasks and allow us to do the work for you.\nSeamless Integration: Our QuickBooks integration makes it far simpler to send quotes, invoices or other relevant documents.\n \n\nSave Time and Money\n\nWhat’s more precious than your time? Each moment invested in worrying about printing, sorting, folding and inserting is costing your business and exposing it to human error risks. NeoSendit eliminates the manual investment, conserves energy and allows you to refocus on the tasks that matter most to your business.\n\nGet Paid Faster\n\nNobody will pay your invoice without receiving it right? Send invoices as they are created so they can reach your customers faster, and you can receive payment sooner. If you are a QuickBooks Online user, it’s even faster with our NeoSendit QBO integration.\n\nBecome Cost-Efficient\n\nWouldn’t it be great if you can eliminate the excessive paper and print storage at your office? With NeoSendit, you no longer need to store large amounts of paper, envelopes, ink cartridges and printers. We can also provide a free audit of your cost savings with our savings calculator to show you how much you would save.\n\nTrack Your Mail and Email\n\nWould you like to know where your mail is going and how long it will take to get there? With NeoSendit, you can securely send and easily track all your physical mail and emails sent to your clients. Its conveniently available to you 24/7 so rest assured, you will always have a pulse on where your communication is at all times.",null,null,"https://www.neopostusa.com/software/neosendit","https://www.youtube.com/watch?v=yPTRQ4iSSCc","N/A","Yes","Yes"]
["Data Accuracy and Enrichment"]
[null,null,"ConnectSuite e-Validate","Address Validation Made Easy\n\nEnsure no mail is left undelivered again with e-Validate; the simple cloud-based address correction service, that quickly and easily validates customer addresses in a few simple clicks - no downloads or training required.\n\nUSPS CASS Certified™ for address validation\nReal-time NCOA updates, to ensure your database is kept current\nAppend additional information to your enhance your contact lists\nSave up to $25 per mail piece by eliminating returned mail and parcels\nMaximize sales by ensuring marketing materials reach the right people\n\nProtect and correct your customer database\n\nConnectSuite e-Validate is a powerful, user-friendly tool that can identify and repair bad addresses. Let e-Validate do the hard work, in three easy steps:\n\nUpload your contact list\nMap your data\nSubmit your file to be cleansed\nAddress information is verified against the USPS® database and incorrect data is identified and automatically corrected.\n\nEnhance your contact lists even more, by adding Data Services such as email append or validation, phone append or reverse phone look up, identify the head of household, and more.\n\nConnectSuite e-Validate; the only tool needed to end Undeliverable-as-Addressed mail.",null,null,"https://www.neopostusa.com/data-management/e-validate","https://www.youtube.com/watch?v=WLX2Oc0RICU","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/cnctsute_evlidte_cutsht.pdf","Yes","Yes"]
[null,null,"Satori Infuse Database Connector","Ensure High Quality Data Across Your Entire Organization\n\nBuild and maintain the highest quality contact database that is accurate, complete and up to date.\n\nEnhance your address records and enable more personalized communications\n\nTake advantage of a unique combination of Professional Services, client software, pre-built database connectors, and Data Services from a single, trusted provider.\n\nLet Satori do the heavy lifting – while leveraging years of experience and numerous implementations.\n\nIdentify source databases\nConnect using Open Database Connectivity\nRead contact data\nProcess data through the Satori Infuse Platform, running services such as Address Validation, Move Update, Apartment Append, Suppression Suite, Phone Information, Email Validation and more\nReturn cleansed and updated data to your source databases\nSatori Database Connector enables you to processes records through the Satori cloud-based Infuse platform using stored procedures for automated job scripting, so there’s no manual intervention required – simply set it and forget it!  \n\nSatori Software’s cloud-based Infuse Web Services can quickly update customer records across multiple systems, maintains accuracy and enhances your records to enable more personalized direct marketing programs.",null,null,"https://www.neopostusa.com/data-management/satori-infuse-database-connector","N/A","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/infusedatabaseconnector_neopost.pdf","Yes","Yes"]
[{"$nulls":8},"https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/infusewebservices_neopost_print.pdf"]
[null,null,"Satori Bulk Mailer","Make your mailing operation much more productive\n\nUse Bulk Mailer to increase mail deliverability, navigate complex postal regulations and achieve the lowest postage rates\n\nNavigate complex postal regulations and achieve the lowest postage rates\n\nPrepare USPS® compliant direct mail faster and more easily. Superior productivity features include wizard-based processes, reusable templates, comprehensive data exchange and an unmatched mail piece designer. Upgrade to Bulk Mailer Business for faster performance with the largest address data files.\n\nBuilt for the highest-volume mailers, Bulk Mailer Business offers advanced capabilities that offer faster performance with large address files and support team-based processes.\n\nIntegrated Microsoft SQL Server database\nMultiuser environment supports template sharing\nPackage mailings with reports for backup or transfer\nArchive older mailings",null,null,"https://www.neopostusa.com/data-management/satori-bulk-mailer","N/A","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/bm_4pg_brochure-neopost.pdf","Yes","Yes"]
[null,null,"Satori Architect","Integrated Mail Preparation and Address Correction Software\n\nSatori Architect is a powerful software solution that helps you maintain the accuracy of your address data while achieving the best postage rates.\n\nComprehensive Contact Data Quality\n\nArchitect seamlessly integrates with Neopost USA’s output management software to enhance your document preparation process and gain ultimate operational efficiency.\n\nUtilizes USPS® CASS Certified™ for address validation\nIncludes USPS PAVE™ certified postal presorting for best postage rates\nOffers real-time Move Update and NCOA updates to ensure that your  communications reach their intended recipients\nIntegrates with Neopost USA’s output management software\nOffers optional EasyTrack mail stream monitoring service which provides real-time visibility of your mail as it passes through the USPS® mail stream",null,null,"https://www.neopostusa.com/data-management/satori-architect","N/A","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/satoriarchitect_4pgbrochure-neopost.pdf","Yes","Yes"]
[null,null,"Satori EasyTrack","Real-time Mail Stream Monitoring Service\n\nEfficiently monitor letters and flats with useful, easily understandable reports based on the scan data collected by USPS automation equipment.\n\nYou can generate a summary of all scan activity for a single mailing or upgrade to access more detailed information about the status of a portion of a mailing or a single mail piece. Reports show where mail was last scanned, provide a breakdown by ZIP Code™ and can even help you identify late deliveries.",null,null,"https://www.neopostusa.com/data-management/satori-easytrack","N/A","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/easytrack_add-on-neopost.pdf","Yes","Yes"]
[" Physical and Digital Document Automation"]
[null,null,"OMS-200 Output Management Software","Simplify your communications with an automated solution\n\nOMS-200 document output management software simplifies and automates document creation and elevates the security of customer communications.\n\nImprove the integrity and efficiency of your document processing\nAdd targeted promotional inserts to increase revenue and improve customer relations\n\nAutomate and Optimize Document Process Automation\n\nBarcodes or OMR marks are added easily to your documents through an intuitive interface to ensure your documents reach their intended recipients. The same technology directs the system to collate, fold, insert and seal your communications using Neopost’s wide range of folder inserters.\n\nIt allows you to:\n\nAutomate the creation of optical marks on documents before printing (OMR, barcode, 2D)\nSend the right document with the right insert to the right customer in a fast and cost-efficient way\nAutomatically handle mail with a variable number of pages to save time\nMerge different documents for the same customer into one envelope to save money on postal costs\nSort your mail into different batches",null,null,"https://www.neopostusa.com/document-output-management/oms-200","https://www.youtube.com/watch?v=h06P5gO9PUY","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo16015_oms200_ctsht_hq.pdf","Yes","Yes"]
[null,null,"OMS-500 Output Management Software","Simplifying the Preparation of Customer Communications\n\nOMS-500 gives you complete control over your customer communications processes by automating and centralizing the preparation of your business documents.\n\nBrowser-Based Intuitive Multi-Channel Communications Management Software\n\nAutomates and centralizes the creation and production of your business-critical communications\nUses intelligent barcodes to secure the content of each mailing piece and control folder inserters\nMulti-channel capabilities allows you to deliver digital communications or print documents\nHelps avoid undeliverable mail and optimizes postal costs by integrating with Satori address correction and presort software \nBrowser-based intuitive interface offers real-time reporting and centralized user administration",null,null,"https://www.neopostusa.com/document-output-management/oms-500","https://www.youtube.com/watch?v=3yRYicxv12A","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo16529_oms500_brochure_hq.pdf","Yes","Yes"]
[null,null,"GMC Inspire","Deliver Interactive, Personalized Messages Through an Enterprise Communication Platform\n\nGMC Inspire enables your business to deliver relevant personalized messages at the right time via your customer’s preferred channel.\n\nCreate stronger engagements with timely, individualized and relevant communications\n\nGMC Inspire is the only single-design Customer Communication Management (CCM) solution that lets you create, manage and deliver quality customer communications that span the entire customer journey. Its multichannel preview, proof, and signoff capabilities are an industry first, allowing you to optimize every customer interaction wherever it takes place: call center, mobile phone, tablet, web, email, even print.\n\nProvides a high-performance document composition platform\nOptimizes template design for multi-channel communication\nTracks production in real time via robust reporting capabilities\nIntegrates with almost any data source\nDrives relevant, targeted customer communications for increased customer satisfaction\n \n\nUse GMC Inspire to communicate across the customer journey and deliver:\n\nChoice – Customers choose the channel by which they want you to communicate with them. A single design deploys across all channels.\nConsistency – Ensure that your company speaks with one voice through a library of templates, and accountability for workflow processes. When customers interact with your company they will experience consistency in brand and message.\nContext – Personalized communications are more engaging. Upsell and cross sell more products and services when you design communications based on individual customer needs and situations.\nSpeed – Customers are impatient so don’t make them wait. Speed up response time and enable real-time two-way interactions with self-service communication.",null,null,"https://www.neopostusa.com/software/gmc-inspire","https://www.youtube.com/watch?v=VEdCy0D7hYI","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/gmc-inspire-overview-brochure-web.pdf","Yes","Not Yet"]
[null,null,"Neotouch Document Delivery","Send One, Ten or Even Thousands of Letters from Your Computer in Minutes\n\nWith Neotouch, you can just as easily send your communications via email, fax or text in addition to our traditional mail services. All it takes is a few clicks.\n\nSend a single document or a batch job of thousands in no time\nPersonalize your business mail by adding promotional inserts and including varying page lengths\nTrack your mail in real time with our user-friendly online interface\nSave on postage costs by grouping all your mail for the same recipient into a single envelope\nRest assured that our advanced mail production facilities will prepare and route your documents using a secure and automated process\n\nNeotouch Makes Mailing Fast and Simple\n\nINCREASE PRODUCTIVITY\n\nSimplify your mail preparation process. With Neotouch, mail prep is done in no time, allowing you to focus on more important business tasks.\n\nRECEIVE PAYMENTS FASTER\n\nSend invoices as they are created so they can reach your customers faster, and you can receive payment sooner.\n\nMULTICHANNEL DELIVERY OPTIONS\n\nNeotouch not only prepares and delivers your documents through traditional postal mail, but also allows you to send via email, fax or text.\n\nSECURITY AND PEACE OF MIND\n\nEach document has a unique barcode, allowing you to know with certainty that the right document and number of pages were delivered. It’s all available for you to track using our web portal.",null,null,"https://www.neopostusa.com/software/physical-and-digital-document-automation/neotouch","https://www.youtube.com/watch?v=ND-5r05gRSg","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo16853_neotouchcutsht_hq2.pdf","Yes","Not Yet"]
[null,null,"ConnectSuite e-Certify Electronic Certified Mail","Simplify the Preparation, Tracking and Storage of Your Certified Mail\n\nIf you need assurance and proof your important documents have been both delivered and received, without the hassle of preparing the mail pieces and storing the Return Receipt “green cards”, then ConnectSuite e-Certify is for you.\n\nUpgrade to a time-saving, digitally traceable Certified Mail solution\n\nPreparing your Certified Mail electronically not only saves time and money, ConnectSuite e-Certify enables you to easily access specific delivery information and images of recipient signatures, all of which are securely stored in the cloud. \n\nSimplifies the preparation of Certified Mail with Electronic Return Receipt\nA user-friendly, browser-based solution – no downloads required!\nGenerates the official USPS Certified Mail barcode\nProvides centralized tracking of mail piece with updated delivery status\nCaptures and stores electronic images of customer signatures securely in the cloud\nSearch and retrieve delivery information and signatures via online interface\nSaves $1.35 on every Certified Mail piece with Return Receipt",null,null,"https://www.neopostusa.com/software/document-output-management/connectsuite-e-certify-electronic-certified-mail-solution","N/A","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo17683_cnnctste_ecrtfy_ctsht_05.pdf","Yes","Not Yet"]
[null,null,"ConnectSuite e-Preference","Effectively Manage your Multi-Channel Communications\n\nA simple yet powerful cloud-based solution that helps companies manage customers’ preferences for traditional mail or digital communications.\n\nOffers a powerful, cloud-based solution with user-friendly interface\nManages customer delivery preference for important business communications\nTracks delivery status in real time for instant visibility\nDecreases costs with one-click paperless enrollment\nPromotes faster payment of invoices with simplified electronic payment capabilitiesDrive migration from traditional mail to secure email communication\n\nCompanies and customers want to choose the communication channel they prefer to deliver and receive their business-critical information. Research shows that a rapidly increasing number of customers prefer digital communications. ConnectSuite e-Delivery is a simple yet powerful cloud-based solution that helps companies manage those preferences and maximize their ability to easily send critical customer communications through traditional mail or a digital channel. \n\nEvolve to Digital Communication while Maintaining Physical Mail Delivery\n\nDetermining a digital communication strategy while maintaining physical mail delivery can be a daunting task for any company. ConnectSuite e-Delivery is a unique solution that meets this need by allowing companies to continue to send physical mail while enabling recipients to evolve to e-delivery. When recipients select their preferred delivery method, ConnectSuite e-Delivery saves their preference and automatically sends documents physically by traditional mail or electronically through email. Better yet, it manages the entire e-consent process and drives adoption through automated opt-in campaigns. Using this proven “PUSH” email delivery method effectively migrates your customers from paper-based communication to electronic delivery – dramatically increasing paper supression.\n\nOnline Payment Capabilities can Simplify Transactions and Reduce Costs\n\nAs more recipients switch to electronic mail delivery and paying bills online, senders will achieve significant cost savings on paper, ink and postage. With ConnectSuite e-Delivery, customers can utilize a solution that’s twice as efficient as traditional physical mail delivery at more than half the cost! \n\nBy helping companies adapt to the market’s changing needs, ConnectSuite e-Delivery simplifies customer communications, helps reduce costs, enhances company image and improves overall customer satisfaction. \n\nComplete Your e-Delivery Strategy\n\nYour website is an essential vehicle to communicate important news about your organization and promote products and solutions. To effectively complement your web presence, ConnectSuite e-Delivery uses a powerful email delivery method that drives more customers to your site, allows you to target them with specific offers and further promotes customer self-service. \n\nReal-Time Reporting Maximizes Electronic Delivery Efficiency\n\nUsing an easy-to-read online interface, ConnectSuite e-Delivery offers real-time reporting that enables companies to track the status of their electronic customer communications and easily manage exceptions. Robust reporting capabilities provide full audit trail and message tracking that displays customer opt-in status, message type and shows if the email was opened, clicked, delivered or bounced. If an error is displayed, the sender can quickly take action by correcting the email address or switch to physical mail delivery.",null,null,"https://www.neopostusa.com/multi-channel-communication/connectsuite-edelivery","N/A","https://www.neopost.com/sites/neopost.com/files/Product/Brochure/neo171254_epreference_ctsht_06.pdf","Yes","Yes"]
[null,null,"Quadient Data Services","Ensure High Quality Data Across Your Entire Organization\nBuild and maintain the highest quality contact database that is accurate, complete and up to date.","Enhance your address records and enable more personalized communications\nGain easy access to new value-add data quality services, data enrichment and mail tracking services, driving business growth. With Quadient Data Services, triple your response rate by accurately targeting your campaigns using:\n\nHead-of-Household\nGeocoding\nSuppression checks\nName Correction\n \n\nLet Quadient Data Services do the heavy lifting – while leveraging years of experience and numerous implementations. Data Services enables you to process records, without manual intervention, in a highly secure cloud environment.\n\nMaintain a clean and safe email database\nemail list accuracyEmail deliverability is a critical component of IP (internet protocol) reputation, which is harmed when too many emails bounce or are branded as spam. If you get blacklisted or clocked, every email sent will end up in the dreaded spam folder.\n\nOur Email Validation service safeguards your business and offers piece of mind as you run email campaigns for yourself or on behalf of your clients.\n\n \n\nBecome a best-in-class mailer\nAs a mailer, your success hinges upon the integrity of your data. If your data isn’t complete, is missing information, or has inaccuracies, your business will suffer.\n\nIncrease delivery rates by adding unit numbers with Apartment Append\nReduce undeliverable mail with 48-month NCOALink®, Move Update and Extended Change of Address services\nMaximize postal discounts with USPS® High Density and Saturation with Walk Sequence",null,"https://www.neopost.com/data-management/quadient-data-services","N/A","https://www.neopost.com/sites/neopost.com/files/Product/Brochure/brochure-quadient-neopost-dataservices-overview2018_0.pdf"]
["Postage Meter Software"]
[null,null,"NeoStats","Manage postage expenses and track them online\n\nTake control of your postage expenses with this powerful reporting solution. With its intuitive and easy-to-use interface, you can track expenses from anywhere at anytime, access usage history and share reports seamlessly across your company.\n\nNeoStats is available in three solutions to best meet your business needs\n\nBASIC\nNeoStats BASIC is included with all new LAN-based IS/IN-Series mailing systems. This powerful reporting system provides a summary report of the total number of pieces processed on your mailing system and the amount of postage spent each month.\n\nENHANCED\nBuilding off of NeoStats BASIC, the ENHANCED option includes Trend and Detailed Reporting categories offering the flexibility to select from predefined reporting periods, or create your own.\n\nTrend Reports provide postage expense detail broken down by Account/Department, Mail Class or Operator. Detailed Reports empower you to create your own reports based any combination of the following categories: Account/Department, Mail Class, Operator, Presort and Weight Break.\n\nCONSOLIDATED\nNeoStats CONSOLIDATED includes all of the features available in ENHANCED plus the ability to centralize postage expense data for multiple mailing systems at one location or multiple mailing systems across many locations. \n\nGenerate reports, create eye catching colorful graphs and spreadsheets in minutes. Analyze use of USPS® Mail Classes and postage trends to optimize potential savings. View, export and share reports based on Accounts/Departments, Mail Class, Operator, Presort and Weight Break.",null,null,"https://www.neopostusa.com/software/postage-meter-software/neostats","N/A","N/A","Yes","Yes"]
[null,null,"NeoShip Online Shipping Solution","The Simple Choice for Online Shipping\n\nNeopost’s powerful online shipping solution ensures full IM®pb compliance from the USPS® for all your package shipping requirements. Simply access NeoShip through your MyNeopost online account, follow the illustrated prompts and create your shipping label.\n\nNeoShip PLUS Delivers Added Benefits\n\nEliminate Manual Entry of Addresses \nSave time and avoid errors attributed to manual entry. Import up to 10,000 addresses to the Public Address Book and up to 1,000 addresses to the Private Address Book, per user.\n\nObtain and Store USPS Proof of Delivery Letter \nThe Postal Service retains delivery data for each shipment, with associated signature and address images, when Extra Services options are applied. The proof of delivery letter is stored and available for viewing and printing.\n\nMaximize Your Desktop Shipping Solution \nCouple a USB scale and thermal label printer with your laptop or desktop computer, and you never have to leave your desk to ship a package.\n\nManage User Roles and Privileges \nAssign roles and control a user’s level of access to the system's functionality based on the role’s definition.","NeoShip BASIC\nSupports USPS® First Class Package Service™, Priority Mail®, Priority Mail Express™, Priority Mail Regional Rate Box A1-A2, B1-B2, Library Mail and Media Mail\nUSPS® Extra Services including: USPS® Tracking™, Signature Confirmation™, Insurance, Adult Signature Required, Adult Signature Restricted Delivery, Return Receipt, Electronic Return Receipt and Restricted Delivery\nWeb Tracking\nAddress Book\nAddress Verification\nPostage Refunds (when applicable)\nUSPS® Pickup Request/Cancel Shipment\nThermal Label Printer Support\nRich reporting capabilities",null,"https://www.neopostusa.com/software/shipping-and-tracking-solutions/neoship-online-shipping-software","https://www.youtube.com/watch?v=f7fyiKd7CAs","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo16085_neoship_ctsht_hq.pdf","Yes","Yes"]
[{"$nulls":4},"NeoShip PLUS\nAll the features of NeoShip BASIC\nAddress Book Import\nProof of Delivery (POD)\nRoles & Privileges Management\nSupport for USB Scales",null,null,null,"https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo16091_neoshipadvncd_ctsht_hq.pdf"]
[{"$nulls":4},"NeoShip ADVANCED\nAll of the features of NeoShip PLUS\nSingle-Screen Interface\nBatch Processing Capability\nConvenient Address Groups",null,null,null,"https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neoshipbasicplusfaqs.pdf"]
[{"$nulls":8},"https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neoshipadvancedfaq.pdf"]
[null,null,"iMeter Apps","Enhance the functionality of your mailing system\n\nSelect from a broad range of apps to enhance performance providing many functions beyond those of traditional postage meters.\n\nConnect your mailing system to easy-to-use online tools and reports\nHelps manage your mailing operations with a few simple clicks\nReadily available through your MyNeopost account\n\nDiscover our range of apps to enhance the performance of your mailroom center\n\nThe Neopost iMeter™ postage meter is an Internet-connected smart device that provides many functions beyond those of traditional postage meters. Existing customers with compatible iMeters may select from a broad range of apps to enhance performance.\n\nA valid MyNeopost account is required to purchase and use iMeter Apps.\n\nPostal Rates App that delivers postage rate updates automaticallyThe Postal Rates App delivers postage rate updates automatically when the United States Postal Service® announces a change to its rates, delivery service fees or postal zones.\n\nOnline Postal Expense Manager App provides web reporting on postage usage\n\nThe Online Postal Expense Manager™ App provides web reporting on postage usage and trends by department, time period and postal class.\n\nNeopost E-Services App tracks all of your outgoing mail anywhere, anytimeThe Neopost E-Services App tracks all of your outgoing mail anywhere, anytime. It tells you exactly when every mail piece went out and, more importantly, when every piece arrived at its destination.\n\nNeopost E-Services with Electronic Return Receipt AppThe Neopost E-Services with Electronic Return Receipt App provides you with a means to accurately track all of your outgoing mail anywhere, anytime. \n\nNeoFunds App provides the flexibility and convenience of funding an iMeterThe NeoFunds® App provides the flexibility and convenience of funding an iMeter™ with the download-now-pay-later NeoFunds postage payment plan. Add postage dollars to a Neopost iMeter™ postage meter with the click of a button.","N/A",null,"https://www.neopostusa.com/postage-meters-software/imeter-apps","N/A","N/A","Yes","Yes"]
[null,null,"ARM - Account Report Manager","Manage your postage expenses\n\nChange the way you manage postage expenses with a comprehensive software solution that tracks postage activity in real time.\n\nMonitor, track and control postage expenses\nGenerate customized expense reports\nEliminate manual postage reconciliation\nIdentify postage expense savings opportunities\n\nPrecise Tracking and Maximum Control of Postage Expenses\n\nOffering a wide range of reports and tools, Neopost’s Account Report Manager (ARM) maximizes potential savings for a single mailing system or multiple-site enterprise.\n\nManaging mail operation costs are critical objectives in today’s competitive environment. More and more, leaders are challenged with increasing efficiency, productivity and reducing operating costs. Without the right tools, reconciling postage expenses can be a burdensome manual process that is time consuming and prone to error.\n\nARM software can enhance the functionality of your mailing system(s) by adding the ability to collect, maintain and report postage usage, helping to track and better control mailing expenses. Data is updated in real time for absolute accuracy. Access to postage expense data is simple via ARM’s dashboard display that accounts for all postage meter activity, regardless of physical location.","N/A",null,"https://www.neopostusa.com/postage-meter-software/account-report-manager","N/A","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo15069_arm_ctsht_hq.pdf","Yes","Yes"]
["Shipping and Tracking Solutions"]
[null,null,"EMS - Enhanced Mailing and Shipping","Mail and ship packages quickly, efficiently and economically from your mail center\n\nAnalyze your shipping operations, change incorrect addresses, pinpoint lost packages and identify money and time-saving opportunities.\n\nShipping software designed to manage costs and build customer relationships\n\nKeeping the lines of communication open with customers is one area where businesses may fall short, not by any fault of their own. Much of it is due to incorrect addresses and lost packages in the mailing and shipping stream. These lost packages result in unaccounted mailing costs and unhappy customers. Besides eroding the bottom line, the expense of not communicating with a customer is even greater – it diminishes loyalty.\n\nCustomers expect their packages to arrive on time, therefore, you should expect a simple solution to process your mail and save money. Don’t settle for anything less.\n\nThe powerful analytics of EMS offer an assortment of tools designed to manage costs and build customer relationships. This technology can analyze your company’s mail and shipping operations and pinpoint incorrect addresses, lost packages and identify where money is being wasted. The address correction feature eliminates many of the problems that lead to returned and misdirected deliveries, delayed deliveries and address correction fees. Additionally, EMS helps you manage and allocate costs by account, carrier, special service and operator productivity.","N/A",null,"https://www.neopostusa.com/shipping-tracking-solution/enhanced-mailing-shipping","N/A","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neopost_ems_ctsht_1116.pdf","Yes","Yes"]
[{"$nulls":8},"https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/ems_faq_0115.pdf"]
[{"$nulls":8},"https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neoship_ems_setup_2015.pdf"]
[{"$nulls":8},"https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neoship_ems_labels_2015.pdf"]
[null,null,"ESS - Enterprise Shipping System","Implement powerful shipping cost controls\n\nControlling shipping expenses can be daunting, especially when employees are working from many different offices and remote locations. Neopost’s Enterprise Shipping System (ESS) allows users to choose the most cost-effective carrier and service based on desired delivery date, all from their desktop – no matter where the user is located.\n\nStreamline your company’s shipping process while saving time and money\n\nSCALABLE CLOUD TECHNOLOGY\n\nOur cloud based technology allows any of your employees to ship from any of your offices or remote locations.\n\nPOWERFUL COST CONTROLS\n\nSave 10-30% per package by empowering your employees to make shipping choices from multiple carriers. Enable your employees to create a shipment or create a request to ship, where your mailroom then completes the shipment.\n\nADDRESS VALIDATION\n\nAddresses are updated and validated using the USPS® CASS™ Certified database, ensuring deliverability and helping to reduce costly, preventable carrier fees.\n\nEXPENSE ALLOCATION\n\nAllocate shipping costs to the appropriate cost center, project, person or department. Empower your employees to make the right shipping choices based on the cost and delivery objective.","N/A",null,"https://www.neopostusa.com/shipping-tracking-solutions/enterprise-shipping-system","N/A","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo15087_ess_ctsht_hq.pdf","Yes","Yes"]
[null,null,"ProShip","Global Multi-Carrier Shipping Software\n\nProShip offers the speed, carrier compliance and support you need to manage your large-volume, enterprise shipping operation and integrates with regional, national and international parcel carriers.\n\nThe flexible, powerful architecture of ProShip shipping software is currently in use at thousands of locations around the world, in industries ranging from aerospace, automotive and manufacturing, to retail, distribution and electronics.\n\nDeliver more orders faster by shipping from any inventory source\n\nProShip software can easily integrate into your order management, warehouse or ERP solutions and offers these key features that are critical in omnichannel fulfillment: Inventory control, faster shipment processing, compliance and support.\n\nThe fastest, most certified carrier compliant solution on the market\n\nDELIVER MORE—FASTER\n\nProShip has the fastest carrier rating engines in the industry, handling as many as one million transactions per hour on a single server.\n\nREDUCE FREIGHT COSTS\n\nAutomated rate shopping ensures the best value with every shipment while simplifying transportation decisions.\n\nSEAMLESS INTEGRATION\n\nProShip ties directly into the shipping process by integrating with your host system, as well as providing email notifications directly to your customer.\n\nADVANCED REPORTING\n\nProship offers the most comprehensive analytics and reporting tools providing real-time, 360 degree visibility through the entire shipping process.","N/A",null,"https://www.neopostusa.com/shipping-tracking-solutions/proship","https://www.youtube.com/watch?v=o2vN9NTRq6g","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/proship_general_brochure.pdf","Yes","Yes"]
[null,null,"WTS - Web Tracking System","A better way to manage inbound deliveries\n\nAre you finding it difficult and time consuming to handle the increasing amount of parcels and other inbound receivables your business has coming in every day? Do you sometimes lose track of them? Neopost’s Web Tracking System is designed to make sure you never do.\n\nOur all-in-one solution is comprised of recording and labeling software, a hand-held device for tracking, and a web-based reporting system, allowing you to track all inbound parcels within your organization in real time, whether it’s in receipt, transit or delivery.\n\nEasily track the internal movement of assets within your organization\n\nINSTANTLY FIND WHAT YOU’RE LOOKING FOR\n\nWTS gives you the visibility you need to simplify and better manage processes in your organization, right from your desktop.\n\nTRACK MORE THAN PARCELS\n\nCatalog, track and trace items such as electronic equipment, software licenses, furniture, tools, office supplies and more.\n\nFLEXIBLE HOSTING OPTIONS\n\nAvailable as either a cloud-based or on-premise software solution, WTS is customized to meet your preferences and business requirements.\n\nSCALABLE TO FIT YOUR NEEDS\n\nDesigned for businesses of all sizes, WTS works for small, single locations as well as large enterprises with multiple locations.","N/A",null,"https://www.neopostusa.com/shipping-tracking-solutions/web-tracking-system","https://www.youtube.com/watch?v=AfyOTN-9Y1w","https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo15059_wts_ctsht_hq.pdf","Yes","Yes"]
[{"$nulls":8},"https://www.neopostusa.com/sites/neopostusa.com/files/Product/Brochure/neo16528_wtslite_ctsht_hq.pdf"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]

{"sheet":"DataPac","index":2,"n_rows":60,"n_cols":9,"rows_kept":60,"cut":false,"hidden":false,"merged":[[35,7,36,7]]}
["Category","Product Name","Product Description","Specifications","Serial #","Vendor Site URL","Pictures Saved?","Migrated?","Alternative Site URL"]
["Software Solutions"]
[null,"eSMART-MAiL","-Mail Processing and Accounting\n-Multiple Mailing Methods\n-Interfaces to Data-Pac Meters Interfaces to Pitney Bowes Meters Interfaces to Hasler/ Neopost On-Demand Permit Printing Mail Manifesting Future Internet Postage Sensor Count & Price for any\n-Mail Production Equipment\n-Postage Accounting\n-SQL or Access Database\n-Open Database-Non Proprietary Data\n-Manual Entry\n-USPS Full Rate Engine\n-Exports to In-House Systems\n-Interfaces to eSMART- MAiL Manager",null,null,"https://www.data-pac.com/software/e-SMART-MAiL.php","Yes","Yes"]
[null,"eSMART-MAiL Manager","-Production Control / Shop floor management\n-Postage Accounting\n-Allows for Setting of Postage from Managers Desktop\n-Manual Entry & Editing\n-SQL or Access Database\n-Exports to In-House Systems\n-Real Time data consolidation\n-Consolidates data from all\n-eSMART- MAiL Applications\n\nApplication for Data Consolidation\n\neSmartMail Manager provides Postal Accounting and Charge Back Information on how much is being spent, on what, by who and when, Manages expenditures, personnel, equipment, and time. The system features Real-time Data Collection, is Network able and has Triple data redundancy for protection and control.\n\neSmartMail Manager has 45 standards reports including, account activity both in a transactional and summary format, productivity by; operator, unit, and job, presort reporting by weight, postage value and class.\n\neSmartMail Manager provides you with a shop floor management tool that will allow you to view the connected eSmartMail units form your PC. You can be alerted if ink is low or, postage is running low. You have the capability to add postage into the meters from eSmartMail Manager at your PC.\n\neSmartMail will control and collect data from; Data-Pac, Pitney Bowes, Hasler and Neopost mailing machines and may interface with many devices that handle paper; inserters, folders, bursters, addressing systems, copiers, and more.\n\nThe manager can do Searches and Displays Current Jobs on Screen, With Real-time Data from Your Desktop, by account, by operator, by job, by date and by time.\n\nOur willingness to work with our customers is the reason so many companies say that for all their mailing, shipping and Information management needs Data-Pac has The Total Solution.",null,null,"https://www.data-pac.com/software/e-SMART-MAiL_Manager.php","Yes","Yes"]
[null,"U SHIP SAVER","USHIPSAVER is a software application designed to provide a method to ship and mail USPS packages, First Class mail, all other mail classes and special services utilizing Internet Postage as the most efficient method of postage generation.\n\nUSHIPSAVER with Internet Postage for less than a $1.00 a day is designed to save an average of $10.00 a day.",null,null,"https://www.data-pac.com/software/UShipSaver.php","Yes","Yes"]
[null,"Pass Software","PASS is a Data-Pac software application that resides in a transparent mode with UPS WorldShipTM and logs each WorldshipTM transactions on a real-time basis and compares it to the appropriate USPS service. PASS logs the USPS data for a service-by-service cost comparison and a total cost comparison daily, weekly or monthly. PASS also analyzes if using USHIPSAVER Alternate Insurance will save money based on carrier rates for USPS and UPS®.\n\nThe objective of PASS is to determine if using USHIPSAVER will save your company money.\n\nThe $95 cost of PASS will be credited towards the purchase of USHIPSAVER",null,null,"https://www.data-pac.com/software/Pass_Software.php","Yes","Yes"]
[null,"Shape Based Solutions","With the introduction of Shape-Based Pricing as part of the USPS' May 14, 2007, Data-Pac offers a line of shape-based solutions that will help you lower rising costs and speed the processing of items in your Mail Center.\n\nShape Based System for Existing Mailing systems\nInterfaces to IJ, WJ, PowerPost, Hasler rotary, PB 6500 and DM500 thru DM 1000\nFull accounting available\nMeasures thickness, for 1/4 inch and 3/4 inch, Accurately allows standard to be set for puff and flex to meet USPS Shape Based Pricing\nWith the introduction of Shape-Based Pricing, Data-Pac's Mailing Solutions allow you to process mixed size, thickness and weight mail pieces at speeds of up to 200 letters per minute in Weigh in Motion.\n\nData-Pac's mailing solutions add greater functionality to mailing operations because it will automatically identify an item as a flat or envelope and will provide the appropriate rate based on both its shape and weight\n\nShaper Image Precision Scale Gauge and Software allows mailing machines without weigh in motion capability to accurately gauge the size and shape of a mail piece. The Shape Based Scale allows the operator to accurately measure the size for letters, flats and Parcels. The system has a thickness gauge that accounts for the \"puff or air\" in the mail to measure a mail pieces true thickness.\n\nShape Based System for Existing Mailing systems Interfaces to IJ, WJ, PowerPost, Hasler rotary, PB 6500 and DM 500 thru DM1000 Full accounting available Measures thickness for both 1/2 inch and 3/4 inch. Accurately allows standard to be set for puff and flex to meet USPS Shape Based Pricing.",null,null,"https://www.data-pac.com/software/Shape_Based_Solution.php","Yes","Yes"]
["Hardware Solutions"]
[null,"EZ-Mailer","The EZ-Mailer qualifies for various USPS discounts turning your mailcenter into a profit center\n\nThe EZ-Mailer Automatic mailing machine is a low to mid volume automatic mailing system that process letters and flats at speeds of up to 140LPM all with a 10 inch color operating screen and small footprint. Options for the EZ-Mailer are a 25lb or a 70lb scale, unlimited accounting and job reporting, operator reporting, presort reporting, full International mail manual with custom forms printing, e-certified forms printing with 3877 firm mailer book. With the Commercial rate option.\n\nThe EZ-Mailer has an option that will allow your mail to qualify for the commercial rate discount program saving you .95 cents per piece on priority mail with free electronic delivery conformation, savings of up to 2.05 per piece of international mail and e-Certified with a savings of up to 1.20 per piece on certified mail. Calculating the number of pieces of these types of mail you process per month may allow you to cost justify the entire monthly lease cost.\n\nThe EZ-Mailer has ink costs that are up to 75% less than the competitor's solutions. The EZ-Mailer sets postage through a high speed internet connection (Competitors mailing machines use old dial up technology).\n\nWith a small footprint all steel construction and built in PC, the Data-Pac EZ-Mailer is truly Americas Better Choice.","All Data-Pac products are designed and assembled in the United States, Buy American Buy Data-Pac\n\nMailing Machine with America2 Postage Meter and Meter or Permit printing\n\nCommercial Rate option allows for Discounts of up to 11%\n\nSOFTWARE FEATURES\neSmart-Mail\nEasy to use user configurable screens\nUser configurable ink saver function\nPostage Accounting with full Reporting\nInternet Data Transfer\nInternet Postage Loading\nConnects to eSmart-Mail Manager\nMail metering, manifesting and permits\nSend-to address and return address\nFull address database\nTracking\nMay qualification for commercial rate discounts and other USPS money saving programs\nElectronic Delivery and Signature confirmation\nCustoms forms 2976 and 2976a\nCertified Mail forms\nPrinting of 3877 Firm Mailer book including E-Certified\n\nHARDWARE FEATURES\nMailing Machine that process up to 140LPM\nAll-in-One Computer with 10\" Color screen for ease of use and increased efficiency\nLabel Printer that prints 1x4 meter tapes\nBuilt in Sealer\nLarger, high-capacity, steel feed deck for letters and flats up to 3/8\" thick\nOptional built in Return address printing\nOptional Power Stacker\nOptional Label Printer that prints 1x4 meter tapes and 4x6 USPS shipping labels\nOptional Complete, multi-level accounting by account, job, and class, as well as user configurable sub-accounts for attorney-client matter\nOptional 25lb or 70 lb. Scale with Shape-Based measurement and a built-in, non-dedicated computer for any other mail center applications\nThe EZ-Mailer with Commercial Rate Option prints 1x4 meter tapes and 4x6 shipping Labels that use the Commercial rate discount for a savings of .95 cents per piece.        Full IMM including customs forms printing and optional commercial rate discounts of $2.05 on International Mail        Optional Certified forms printing including 3877 firm mailer book, e-certified discounts of $1.20 per piece",null,"https://www.data-pac.com/hardware/ez-mailer.php","Yes","Yes"]
[null,"The Advanced Curve","Special Features with the Advanced Curve are:\nBulk Mail Discounts\nCASS & MASS Certification\nMLOCR Camera for Address Verification\nPrints IMB (Intelligent Mail Barcode)\nAt least 5.8 cent discount on qualified mail\n\nData-Pac's introduction of The Advanced Curve is leading the mailing industry once again! Utilizing USPS Bulk Mail discounts we have developed a machine that will allow your mailing center to reduce its costs and improve your ability to be profitable. Process enough mail and you can offset your entire lease cost and then some!\n\nSee your savings, use our calculator from the link above.\n\nFor more details on The Advance Curve, please click on the Advance Curve Details button above, located on the left below the video.\n\n*based on approximate lease cost of $2100/mo. without local service contract **\"Profit center\" is in reference to discounts that ultimately improve your bottom line\n\nThe Advanced Curve qualifies for various USPS discounts turning your mailcenter into a profit center.","The Advanced Curve \nThe First Mailing System with OCR Reading for USPS Discounts\n\nThe Advance Curve Intelligent Envelope Processing System has an OCR camera that reads the address at speeds of up to 6,000 per hour. As the Advanced Curve reads the address it processes the address for CASS, MASS and does the address corrections. The Advanced Curve system calculates the zip plus 4 plus 2 and then sprays the IMB on the bottom of the envelope. This process qualifies the customer for the letter mixed AADC rate with out doing any sorting, that equates to a 5.8 cent per piece discount allowing the system to be cost justified with as little as 1775 letter per day. The system also qualifies for the Flat mixed AADC discount rate saving 15.5 cents per piece allowing the entire cost of the system to be justified with as little as 675 flats per day.\n\nThe Advanced Curve System still has all of the other great features that are offered in the standard Curve such as weigh-in-motion capabilities and optional batch speeds of up to 12,000 per hour, with a built in 70lb scale, unlimited accounting and job reporting, operator reporting, presort reporting, full International mail manual with custom forms printing, e-certified forms printing with 3877 firm mailer book all with a 15\" color touch screen, The Curve has optional \"One Pass Printing\" with the ability to print the IMB and indicia or permit printing all at the same time. The Curve has address cleansing and correction and ink costs that are up to 75% less than the competitor's solutions. The Curve sets postage through a high-speed Internet connection.\n\nThe Advanced Curve qualifies for various USPS discounts turning your mailcenter into a profit center.\n\nMay Qualify for Commercial Rate (Discounts of up to 11%)\n\nSOFTWARE FEATURES\n\neSmart-Mail\nCASS Application Installed Optional\nPresort Application Installed Optional\nPostage Accounting with full Reporting\nInternet Data Transfer\nInternet Postage Loading\nConnects to eSmart-Mail Manager\nMail metering, manifesting and permits\nSend-to address and return address\nFull address database\nIntelligent Mail Barcode\nTracking\nMay qualify for commercial rate discounts and other USPS money saving programs\nElectronic Delivery and Signature confirmation\nCustoms forms\nCertified Mail forms\nPrinting of 3877 Firm Mailer book including E-Certified\n \t\nHARDWARE FEATURES\n\nMailing Machine with Weigh in Motion and Static Weighing Capabilities\nAll-in-One Computer with 15\" Color, touch-screen for ease of use and increased efficiency\nOptional built in Addressing Machine\nOptional Power Stacker\nLabel Printer that prints meter tapes and 4x6 USPS shipping labels\nBuilt in Sealer\nLarger, high-capacity, stainless steel feed deck for letters and flats up to 5/8\" thick\nComplete, multi-level accounting by account, job, and class, as well as user configurable sub-accounts for attorney-client matter\nBatch-mail processing speeds in excess of 11,000 pieces-per-hour\n70 lb. Scale with Shape-Based measurement sensors and a built-in, non-dedicated computer for any other mail center applications",null,"https://www.data-pac.com/hardware/advanced_curve_details.php","Yes","Yes"]
[null,"The Curve","Product Features:\n\nThe Curve Intelligent Envelope Processing system has weigh-in-motion capabilities, a built in 70lb scale, unlimited accounting and job reporting, operator reporting, presort reporting, full International mail manual with custom forms printing, e-certified forms printing with 3877 firm mailer book all with a 15\" color touch screen, The Curve has optional \"One Pass Printing\" with the ability to print the return address, the send to address including IMB, and indicia or permit printing all at the same time. The Curve has optional address cleansing and correction and ink costs that are up to 75% less than the competitor's solutions. The Curve sets postage through a high-speed Internet connection.\n\n\nThe Curve qualifies for various USPS discounts turning your mailcenter into a profit center","IMB Standard Security, IMB Cryptographic Security\nMailing Machine with America2 Postage Meter\nComplete envelope printing including return address, full address including IMB and Meter or Permit printing\n\nMay Qualify for Commercial Rate (Discounts of up to 11%)\n\nSOFTWARE FEATURES\neSmart-Mail\nCASS Application Installed Optional\nPresort Application Installed Optional\nPostage Accounting with full Reporting\nInternet Data Transfer\nInternet Postage Loading\nConnects to eSmart-Mail Manager\nMail metering, manifesting and permits\nSend-to address and return address\nFull address database\nIntelligent Mail Barcode\nTracking\nMay qualify for commercial rate discounts and other USPS money saving programs\nElectronic Delivery and Signature confirmation\nCustoms forms\nCertified Mail forms\nPrinting of 3877 Firm Mailer book including E-Certified\n \t\nHARDWARE FEATURES\nMailing Machine with Weigh in Motion and Static Weighing Capabilities\nAll-in-One Computer with 15\" Color, touch-screen for ease of use and increased efficiency\nOptional built in Addressing Machine\nOptional Power Stacker\nLabel Printer that prints meter tapes and 4x6 USPS shipping labels\nBuilt in Sealer\nLarger, high-capacity, stainless steel feed deck for letters and flats up to 5/8\" thick\nComplete, multi-level accounting by account, job, and class, as well as user configurable sub-accounts for attorney-client matter\nBatch-mail processing speeds in excess of 11,000 pieces-per-hour\n70 lb. Scale with Shape-Based measurement sensors and a built-in, non-dedicated computer for any other mail center applications",null,"https://www.data-pac.com/hardware/curve.php","Yes","Yes"]
[null,"DP 100W","Product Features:\n\nDigital Mailing System\n100 Letters per minute Weigh-on-the-Fly In-line Scale\n200 letters per minute in Batch mode with Shaped Based Measuring\nMixed Thickness Feeder\nSealer\n15 inch touch screen PC\n1 3/16\" Label Printer\nWeighing Platform Optional\neSMART- MAiL Software\nDifferential Weighing Optional",null,null,"https://www.data-pac.com/hardware/DP_100W.php","Yes","Yes"]
[null,"DP 140W","Product Features:\n\nDigital Mailing System\n140 Letters per minute Weigh-on-the-Fly In-line Scale\n200 letters per minute in Batch mode with Shaped Based Measuring\nMixed Thickness Feeder\nSealer\n15 inch touch screen PC\n1 3/16\" Label Printer\nWeighing Platform Optional\neSMART- MAiL Software\nDifferential Weighing Optional",null,null,"https://www.data-pac.com/hardware/DP_140W.php","Yes","Yes"]
[null,"DP 200W","Product Features:\n\nComplete Digital Mailing solution in Weigh in Motion and Shaped Based Measuring\nMixed Thickness Feeder / Sealer\nAll steel construction\n15 inch touch screen PC\nFull accounting Standard\nLowest ink cost on the market today 40% less than red ink\n1 3/16\" Label Printer\nWeighing Platform Optional\neSMART- MAiL Software\nDifferential Weighing Optional",null,null,"https://www.data-pac.com/hardware/DP_200W.php","Yes","Yes"]
[null,"DIB-200W LPM","Product Features\n\nDigital Mailing System for use with inserters for in line weighing.\nHigh Speed Envelope Printer\n15 inch touch screen PC\nRugged 24/7 Dependability\neSmart-Mail Software\nPostage Accounting\nData Consolidation with eSmart-Mail Manager",null,null,"https://www.data-pac.com/hardware/DIB_200W_LPM.php","Yes","Yes"]
[null,"DP 200B","Product Features:\n\nComplete Digital Mailing System\nMixed Thickness Feeder\n15 inch Touch Screen PC\nComplete Mailing solution\nAll steel construction\n200LPM in batch mode\nFull accounting Standard\nLowest ink cost on the market today 40% less than red ink\n3 1/2\" Flap Envelope Sealer\neSMART- MAiL Software\nDual Carrier Optional\nData Consolidation with eSMART- MAiL Manager",null,null,"https://www.data-pac.com/hardware/DP_200B.php","Yes","Yes"]
[null,"DP 240B","Product Features:\n\nDigital Mailing System\nMixed Thickness Feeder\n240 letters Per minute in Batch mode\n15 inch touch screen PC\n3 1/2\" Flap Envelope Sealer\neSMART- MAiL Software\nDual Carrier Optional\nPostage Accounting Complete Mailing solution\nAll steel construction\nLowest ink cost on the market today 40% less than red ink\nData Consolidation with eSMART- MAiL Manager",null,null,"https://www.data-pac.com/hardware/DP_240B.php","Yes","Yes"]
[null,"Digital Inserter Base (DIB)","Product Features\n\nDigital Mailing System for use with inserters\nHeight Speed Envelope Printer\n15 inch touch screen PC\nRugged 24/7 Dependability\neSmart-Mail Software\nPostage Accounting\nData Consolidation with eSmart-Mail Manager",null,null,"https://www.data-pac.com/hardware/DIB.php","Yes","Yes"]
[null,"AMERICA2 Postage Meter","The AMERICA2 PSD is the first authorized postage meter manufacturer in 25 years with Internet-based funds loading. The America2 postage meter has achieved FIPS-140-2 Certification\n\nThe America2 postage meter is now in active distribution.",null,null,"https://www.data-pac.com/hardware/America2_Postage_Meter.php","Yes","Yes"]
[{"$nulls":6},"No","Not Yet"]
[{"$nulls":6},"No","Not Yet"]
[{"$nulls":6},"No","Not Yet"]
[{"$nulls":6},"No","Not Yet"]
[{"$nulls":6},"No","Not Yet"]
[{"$nulls":6},"No","Not Yet"]
[{"$nulls":6},"No","Not Yet"]
[{"$nulls":6},"No","Not Yet"]
[{"$nulls":6},"No","Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]
[{"$nulls":7},"Not Yet"]

{"sheet":"Rena","index":3,"n_rows":101,"n_cols":12,"rows_kept":101,"cut":false,"hidden":false,"merged":[]}
["Category","Sub-Category (if applicable)","Product Name","Product Description","Specifications","Serial #","Vendor Site URL","Video Content URL(s)","Downloadable Content URL(s)","Pictures Saved?","Migrated?","Alternative Site URL"]
["Address Printing"]
[null,null,"AS-150","Key Features\n\n- Fixed head technology with three cartridges for 1.5\" of print height\n- 5,500 No. 10 envelopes/hr\n- 7,500 coin/seed packets/hr\n- Fixed Thickness\n- Clutch-Control Integrated Feeder\n- High Speed USB 2.0 Port\n\n\nThe AS-150 is a small media monochrome printer designed to print text and barcodes on small materials such as coin envelopes and seed packets. It can also print on #10 and 6x9 envelopes. The printer is easy to set up and features four print qualities from 150 to 600 dpi.","Print Technology\tThermal Inkjet, Three HP 45A-Style High Capacity Cartridges\nAddress Speed\t\n    5,500 /hour\n     (#10 Envelopes)\t7,500 /hour\n(Coin/Seed Packets)            \nPrint Quality (Dots Per Inch)\t\n   Description\tDots Per Inch\tResolution\n   High Quality\t600 d.p.i.\t600 x 600 dpi\n   Letter Quality\t300 d.p.i.\t600 x 300 dpi\n   Standard Quality\t200 d.p.i.\t600 x 200 dpi\n   Hi-Speed Quality\t150 d.p.i.\t600 x 150 dpi\nImage Area\t1.5” X 9.5”\nProcessor\tAMD TigerSharc 100 MHz DSP with Dual Calculation Technology\nMemory\t12 MB RAM\nFonts\tAll TrueType fonts available on PC\nPrint Orientation\tNormal and Reverse\nCounters\tOperator resettable job counter. Stores lifetime counter value.\nInk Monitor\tVisible on Display\nPrints\tAllows printing of graphics, logos, and barcodes\nMaterial Size\tMinimum (W x L):  2.125\" x 4\"\nMaximum (W x L):  6.5” x 9.5”\nMaterial Thickness\tUp to 0.020\"\nFeeder-Capacity\tUp to 300 #10 Envelopes\nSoftware\tWindowsTM Printer Drivers for Windows XP and 7\nPC Interface\tUSB 2.0\nDiagnostics\tResident in firmware\nFirmware Update\tFlash PROM update\nDuty Cycle\t350,000 letter-sized sheets per month\nDimensions\t18.5” H x 14” W x 13” D\nWeight\t32 lbs\nElectrical\t100-240 VAC, 50/60 Hz, 1 A\nOptions\tConveyor/Stacker/Dryer, Drop Tray",null,"http://www.renausa.com/products/50/as-150.html","https://www.youtube.com/watch?v=APZP85STxlc","http://www.renausa.com/brochures/as-150.pdf","Yes","Yes"]
[null,null,"ENVELOPE IMAGER 1.5 PLUS","Key Features\n\n- 30,000 Postcards/hr\n- 1.5\" of Print From One Print Module\n- 3/16\" Thickness Capability\n- Clutch-Control Integrated Feeder\n- Extended Material Hopper\n- High Speed USB 2.0 Port\n\nMany improvements adorn the Envelope Imager 1.5 Plus. This formidable little machine can churn out some serious productivity. Offering all of the same features as the entry-level 1.5, the Plus has an extended hopper that can hold a whole box of #10 envelopes (500) at a time. It can also take materials up to a class-leading 3/16” thick. The sleek control panel and professional grade color scheme lets you know that this printer means business.","Print Technology\tThermal Inkjet, Three HP 45A-Style High Capacity Cartridges\nAddress Speed\t\n   30,000 /hour at 150 dpi\n   25,000 /hour at 200 dpi\n   20,000 /hour at 300 dpi\n   11,500 /hour at 600 dpi\n     (9 Lines on 4”x6” Postcard)\t22,000 /hour at 150 dpi\n19,000 /hour at 200 dpi\n15,000 /hour at 300 dpi\n7,200 /hour at 600 dpi\n(9 Lines on #10 Envelopes)\nPrint Quality (Dots Per Inch)\t\n   Description\tDots Per Inch\tResolution\n   High Quality\t600 d.p.i.\t600 x 600 dpi\n   Letter Quality\t300 d.p.i.\t600 x 300 dpi\n   Standard Quality\t200 d.p.i.\t600 x 200 dpi\n   Hi-Speed Quality\t150 d.p.i.\t600 x 150 dpi\nImage Area\t1.5” X 14” w/ 9.5” Vertical Range\nPrint Head Split\t3 Pen Stitched Design\nProcessor\tAMD TigerSharc 100 MHz DSP with Dual Calculation Technology\nMemory\t64 MB RAM\nFonts\tAll TrueType fonts available on PC\nPrint Orientation\tNormal and Reverse\nCounters\tOne operator resettable job counter, one permanent lifetime counter\nInk Monitor\tVisible on Display\nPrints\tAllows printing of graphics, logos, and barcodes\nMaterial Size\tMinimum (W x L):  3\" x 5\"\nMaximum (W x L):  14” x 14”\nMaterial Thickness\tUp to 3/16”\nFeeder-Capacity\tUp to 500 #10 Envelopes\nSoftware\tWindowsTM Printer Drivers for WindowsTM 98,\n2000, NT, ME, and XP\nPC Interface\tParallel and USB 2.0\nDiagnostics\tResident in firmware\nFirmware Update\tFlash PROM update.\nDuty Cycle\t30 million addresses total or 500,000 per month over a 5-year life cycle.\nDimensions\t19” H x 21” L x 20.5” W\nWeight\t53 lbs\nElectrical\t115VAC or 240VAC 50/60 Hz\nOptions\tRENA Systems EASYInks, HP Versatile fast dry Black, and Spot Colors, Conveyor/Stacker/Dryer, Drop Tray",null,"http://www.renausa.com/products/11/envelope-imager-15-plus.html","https://www.youtube.com/watch?v=RfS5e-nXv-g","http://www.renausa.com/brochures/RENA_Systems_Env_Img_1-5_Plus.pdf","Yes","Yes"]
[null,null,"ENVELOPE IMAGER 2.5","Key Features\n\n- 2.5\" of Print From Two Print Modules\n- 30,000 Postcards/hr\n- Clutch-Control Integrated Feeder\n- Electronic Thickness Control (1/4\")\n- High Speed USB 2.0 Port\n- Very Affordable!\n\nThe versatile Envelope Imager 2.5 is a truly wonderful machine. Offering production printer stats with a price tag of an entry-level printer, it is tough to beat. With a feed system that has THREE rows of high grip rollers and the capacity for materials up to 1/4\" thick, it can handle any job. The key feature here is the split 3+2 printhead configuration that allows mailers to address and return addresses and indicia at the same time – a quantum leap in useable print area from the entry-level set of products.","Print Technology\tThermal Inkjet, Five HP 45A-Style High Capacity Cartridges\nAddress Speed\t\n   30,000 /hour at 150 dpi\n   25,000 /hour at 200 dpi\n   20,000 /hour at 300 dpi\n   11,500 /hour at 600 dpi\n     (9 Lines on 4”x6” Postcard)\t22,000 /hour at 150 dpi\n19,000 /hour at 200 dpi\n15,000 /hour at 300 dpi\n7,200 /hour at 600 dpi\n(9 Lines on #10 Envelopes)\nPrint Quality (Dots Per Inch)\t\n   Description\tDots Per Inch\tResolution\n   High Quality\t600 d.p.i.\t600 x 600 dpi\n   Letter Quality\t300 d.p.i.\t600 x 300 dpi\n   Standard Quality\t200 d.p.i.\t600 x 200 dpi\n   Hi-Speed Quality\t150 d.p.i.\t600 x 150 dpi\nImage Area\t2.5” x 15” w/ 9” Vertical Range\nPrint Head Split\t3 Pen Stitched + 2 Pen Stitched Design\nProcessor\tAMD TigerSharc 100 MHz DSP with Dual Calculation Technology\nMemory\t64 MB RAM\nFonts\tAll TrueType fonts available on PC\nPrint Orientation\tNormal and Reverse\nCounters\tOne operator resettable job counter, one permanent lifetime counter\nInk Monitor\tVisible on Display\nPrints\tAllows printing of graphics, logos, and barcodes\nMaterial Size\tMinimum (W x L):  3\" x 5\"\nMaximum (W x L):  13.5” x 15”\nMaterial Thickness\tUp to 1/4”\nFeeder-Capacity\tUp to 500 #10 Envelopes\nSoftware\tWindowsTM Printer Drivers for WindowsTM 98,\n2000, NT, ME, and XP\nPC Interface\tParallel and USB 2.0\nDiagnostics\tResident in firmware\nFirmware Update\tFlash PROM update.\nDuty Cycle\t51 million addresses total or 850,000 per month over a 5-year life cycle\nDimensions\t11.5” H x 19.56” L x 20” W\nWeight\t68 lbs\nElectrical\t115VAC or 240VAC 50/60 Hz\nOptions\tConveyor/Stacker/Dryer, Drop Tray, RENA Systems EASYInks, HP Versatile Black",null,"http://www.renausa.com/products/12/envelope-imager-25.html","https://www.youtube.com/watch?v=sIiWtCEUDbo","http://www.renausa.com/brochures/RENA_Systems_Env_Img_2-5.pdf","Yes","Yes"]
[null,null,"ENVELOPE IMAGER 3.0","Key Features\n\n- 3\" of Print From Two Print Modules\n- 34,000 Postcards/hr\n- Cartridge Capping Station\n- Electronic Thickness Control (3/8\")\n- Clutch-Control Integrated Feeder\n- High Speed USB 2.0 Port\n\nThe durable, heavy duty Envelope Imager 3.0 has a secret compartment – now that is cool. The secret to great print quality is proper maintenance of print heads, and the special compartment integrated below the material hopper is designed to store and seal up to eight (8) inkjet cartridges. We have also completely redesigned the firmware architecture in the Envelope Imager 3.0 with new features like Print Enhancement, Intelligent Pause Control, Electronic Thickness Control, Advanced Macro Management and a host of other improvements make the Envelope Imager 3.0 the machine to beat.","Print Technology\tThermal Inkjet, Six HP 45A-Style High Capacity Cartridges\nAddress Speed\t\n   34,000 /hour at 150 dpi\n   25,000 /hour at 200 dpi\n   20,000 /hour at 300 dpi\n   11,500 /hour at 600 dpi\n     (9 Lines on 4”x6” Postcard)\t26,000 /hour at 150 dpi\n19,000 /hour at 200 dpi\n15,000 /hour at 300 dpi\n7,200 /hour at 600 dpi\n(9 Lines on #10 Envelopes)\nPrint Quality (Dots Per Inch)\t\n   Description\tDots Per Inch\tResolution\n   High Quality\t600 d.p.i.\t600 x 600 dpi\n   Letter Quality\t300 d.p.i.\t600 x 300 dpi\n   Standard Quality\t200 d.p.i.\t600 x 200 dpi\n   Hi-Speed Quality\t150 d.p.i.\t600 x 150 dpi\nImage Area\t4” X 17” w/ 12” Vertical Range\nPrint Head Split\t3 Pen Stitched + 3 Pen Stitched Design\nProcessor\tAMD TigerSharc 100 MHz DSP with Dual Calculation Technology\nMemory\t64 MB RAM\nFonts\tAll TrueType fonts available on PC\nPrint Orientation\tNormal and Reverse\nCounters\tOne operator resettable job counter, one permanent lifetime counter\nInk Monitor\tVisible on Display\nPrints\tAllows printing of graphics, logos, and barcodes\nMaterial Size\tMinimum (W x L):  3\" x 5\"\nMaximum (W x L):  13.5” x 17”\nMaterial Thickness\tUp to 3/8”\nFeeder-Capacity\tUp to 750 #10 Envelopes\nSoftware\tWindowsTM Printer Drivers for WindowsTM 98,\n2000, NT, ME, and XP\nPC Interface\tParallel and USB 2.0\nDiagnostics\tResident in firmware\nFirmware Update\tFlash PROM update\nDuty Cycle\t120 million addresses total or 2,000,000 per month over a 5-year life cycle\nDimensions\t25” H x 28” L x 22” W\nWeight\t80 lbs\nElectrical\t115VAC or 240VAC 50/60 Hz\nOptions\tConveyor/Stacker/Dryer, Drop Tray",null,"http://www.renausa.com/products/13/envelope-imager-30.html","https://www.youtube.com/watch?v=3Q34IIh4ls4","http://www.renausa.com/brochures/RENA_Systems_Env_Img_3-0.pdf","Yes","Yes"]
[null,null,"MACH 5 DIGITAL COLOR PRINTER","Key Features:\n\n- 7,500 envelopes/hr\n- Full bleed capability\n- Automatic Capping & Cleaning Station\n- Built-in Top Load Friction Feeder\n- Five 250 mL ink tanks (CMYKK)\n \n\nWith exceptional technology from Memjet, The Mach 5 Digital Color Printer is unlike any other envelope printer in its class. It’s fast, reliable, AND it will boost your return on investment. You will ask yourself how your business ever survived without it!\n\n \n\nThe Mach 5 is capable of printing full color at 6 inches per second and an amazing 1600 x 1600 dots per inch. The faster option is 1600 x 800 dpi at 12 inches per second which still produces a clear image. This means you will be producing up to 7,500 pieces per hour! The Mach 5 clearly wins out over the 1200 dpi at 3,000 pieces per hour of LED or laser printers.  That’s because Memjet packed five ink channels (Cyan, Yellow, Magenta, Black, and Black) into the single 8.77” wide print bar. Inside these channels is a whopping 70,400 nozzles from which the ink is sprayed onto the substrate.\n\n \n\nIf you want a cost-efficient machine, the Mach 5 is just that. The five ink tanks each hold 250 mL of ink for long job runs and low cost per piece. If your business is looking for a machine that will produce short runs, the Mach 5 is perfect for that as well. Print what you need, when you need it. It will eliminate outdated cardstock and free you up on storage.\n\n \n\nWhen paired with mColor, a color management software, you can match the exact color of your company's logo in no time using spot color adjustment. Click here to learn more.","Speed\n\nUp to 3,600 pages per hour (1600 x 800 dpi @ 12 ips - 8.5\" x 11\" sheets)\nUp to 7,500 #10 envelopes per hour (1600 x 800 dpi @ 12 ips)\nMaterial Size\tMIN: 3\" W x 4-1/8\" L    MAX: 9.5\" W x 17\" L\nMaterial Thickness           \tUp to 1/48\" (0.5mm / 430 gsm / 160# Cover / 240# Index)\nPrint Quality\tNormal (1600 x 800 dpi @ 12 ips); Best (1600 x 1600 dpi @ 6 ips)\nTechnology\tMemjet Thermal Inkjet\nInk Capacity\tCyan (250 ml); Yellow (250 ml); Magenta (250 ml); Black (500 ml)\nPrint Area\t8.5\" x 17\" with full bleed capability\nColor Matrix\tUp to 16.8 million colors\nFeeder\tTop Load Friction Feeder Built-In\nPC Interface\tUSB & ETHERNET\nFirmware Update \tElectronic Download via PC Connection\nTransport\tPressure Roller System with Star Rollers\nFeatures\tFull color inkjet; fixed head design; high capacity ink tanks; automatic printhead cleaning and capping service station\nFonts\tAll available TruType or Postscript system fonts\nDimensions\t24\" W x 18\" H x 20\" D\nWeight\t90 lbs\nElectrical\t110-240 VAC 60Hz / 2A\nOptions\tConveyors & IR Dryers; Satori Bulk Mailer Software\nDuty Cycle\t30 million pieces total or 500,000 per month over a 5-year life cycle",null,"http://www.renausa.com/products/15/mach-5-digital-color-printer.html","N/A","http://www.renausa.com/brochures/mach-5-digital-color-printer.pdf","Yes","Yes"]
[null,null,"MACH 5DX","Key Features:\n\n- One or two-sided printing\n- 3,600 letter size sheets/hr\n- 7,500 envelopes/hr\n- Full bleed capability\n- Automatic Capping & Cleaning Station\n- Built-in Top Load Friction Feeder\n- Five 250 mL ink tanks (CMYKK)\n \n\nWe have added duplex ability to the Mach 5! It's the same exceptional technology from Memjet, but this time, it can print on both sides! \n\nThe Mach 5DX is capable of printing full color at 6 inches per second and an amazing 1600 x 1600 dots per inch. The faster option is 1600 x 800 dpi at 12 inches per second. These speeds are both for single and double-sided printing. The Mach 5DX is still packed with the same Memjet five ink channels (Cyan, Yellow, Magenta, Black, and Black) and the same single 8.77” wide print bar. Inside these channels is a whopping 70,400 nozzles from which the ink is sprayed onto the substrate.\n\nThe five ink tanks each hold 250 mL of ink for long job runs and low cost per piece. If your business is looking for a machine that will produce short runs, the Mach 5 is perfect for that as well. Print what you need, when you need it. It will eliminate outdated cardstock and free you up on storage.\n\nWhen paired with mColor, a color management software, you can match the exact color of your company's logo in no time using spot color adjustment. Click here to learn more.\n\n ","Speed\n\nUp to 3,600 pages per hour (1600 x 800 dpi @ 12 ips - 8.5\" x 11\" sheets)\nUp to 7,500 #10 envelopes per hour (1600 x 800 dpi @ 12 ips)\nMinimum Material Size\t2-side: 5\" L x 3\" W\n1-side: 4.2\" L x 3\" W\nMaximum Material Size\t2-side: 17\" L x 9\" W\n1-side: 17\" L x 9.5\" W\nMaterial Thickness           \tUp to 0.020\" (0.5 mm)\nPrint Quality\tNormal (1600 x 800 dpi @ 12 ips); Best (1600 x 1600 dpi @ 6 ips)\nTechnology\tMemjet Thermal Inkjet\nInk Capacity\tCyan (250 ml); Yellow (250 ml); Magenta (250 ml); Black (500 ml)\nPrint Area\t8.5\" x 30\" with full bleed capability\nColor Matrix\tUp to 16.8 million colors\nFeeder\tTop Load Friction Feeder Built-In\nPC Interface\tUSB & ETHERNET\nFirmware Update \tElectronic Download via PC Connection\nTransport\tPressure Roller System with Star Rollers\nFeatures\tFull color inkjet; fixed head design; high capacity ink tanks; automatic printhead cleaning and capping service station; duplexing unit\nFonts\tAll available TruType or Postscript system fonts\nDimensions\tWith Printer: 39\" L x 54.5\" H x 21.5\" D\nWithout Printer: 28.25\" L x 33\" x 21.5\" D\nWeight\tWith Printer: 146 lbs\nWithout Printer: 72 lbs\nElectrical\t115-240 VAC 60Hz / 2A\nOptions\tConveyors & IR Dryers; Satori Bulk Mailer Software\nDuty Cycle\t350,000 letter-sized sheets per month over a 5-year life cycle\n ",null,"http://www.renausa.com/products/49/mach-5dx.html","N/A","http://www.renausa.com/brochures/mach-5dx.pdf","Yes","Yes"]
[null,null,"ENVELOPE IMAGER XT 3.0\n","Key Features\n\n- AccuTrak Vacuum Transport\n- 3\" of Print From Three Print Modules\n- 34,000 Postcards/hr\n- Cartridge Capping Station (view here)\n- Tab 'N Print Inline With The T-950 or T-750\n\nThe power house Envelope Imager XT series starts with the 3.0 and offers an industry leading combination capabilities. The feature-laden Envelope Imager XT 3.0 offers tremendous advantages over the competition with its exceptional price, high operating speeds, innovative design, and bullet-proof construction. The power of 34,000 postcards/hr and 26,000 #10s/hr gets the job done fast. The Envelope Imager XT 3.0’s USB 2.0 port works seamlessly while the advanced microprocessor and 64 MB of RAM crunch data like no other printer. The 3” print area from three independent printheads gives you total freedom in envelope imaging. With unparalleled material handling, it’s power you can actually use.","Print Technology\tThermal Inkjet, Six HP 45A-Style High Capacity Cartridges\nAddress Speed\t\n   34,000 /hour at 150 dpi\n   25,000 /hour at 200 dpi\n   20,000 /hour at 300 dpi\n   11,500 /hour at 600 dpi\n     (9 Lines on 4”x6” Postcard)\t26,000 /hour at 150 dpi\n19,000 /hour at 200 dpi\n15,000 /hour at 300 dpi\n7,200 /hour at 600 dpi\n(9 Lines on #10 Envelopes)\nPrint Quality (Dots Per Inch)\t\n   Description\tDots Per Inch\tResolution\n   High Quality\t600 d.p.i.\t600 x 600 dpi\n   Letter Quality\t300 d.p.i.\t600 x 300 dpi\n   Standard Quality\t200 d.p.i.\t600 x 200 dpi\n   Hi-Speed Quality\t150 d.p.i.\t600 x 150 dpi\nImage Area\t3” X 17” w/ 12” Vertical Range\nPrint Head Split\t3 Pen Stitched + 2 Pen Stitched + 1 Pen Design\nProcessor\tAMD TigerSharc 100 MHz DSP with Dual Calculation Technology\nMemory\t64 MB RAM\nFonts\tAll TrueType fonts available on PC\nPrint Orientation\tNormal and Reverse\nCounters\tOne operator resettable job counter, one permanent lifetime counter\nInk Monitor\tVisible on Display\nPrints\tAllows printing of graphics, logos, and barcodes\nMaterial Size\tMinimum (W x L):  3\" x 5\"\nMaximum (W x L):  13.5” x 17”\nMaterial Thickness\tUp to 3/8”\nFeeder-Capacity\tFeeder Dependent\nSoftware\tWindowsTM Printer Drivers for WindowsTM 98,\n2000, NT, ME, and XP\nPC Interface\tParallel and USB 2.0\nDiagnostics\tResident in firmware\nFirmware Update\tFlash PROM update\nDuty Cycle\t120 million addresses total or 2,000,000 per month over a 5-year life cycle\nDimensions\t16” H x 30” L x 24” W\nWeight\t110 lbs\nElectrical\t115VAC or 240VAC 50/60 Hz\nOptions\tConveyor/Stacker/Dryer, Drop Tray",null,"http://www.renausa.com/products/16/envelope-imager-xt-30.html","https://www.youtube.com/watch?v=K9AaP-bvBG8","http://www.renausa.com/brochures/RENA_Systems_Env_Img_XT_3-0.pdf","Yes","Yes"]
[null,null,"ENVELOPE IMAGER XT 4.0\n","Key Features\n\n- 4\" of Print From Four Print Modules\n- AccuTrak Vacuum Transport\n- 34,000 Postcards/hr\n- Tab 'N Print Inline With The T-950 or T-750\n- Cartridge Capping Station\n\nThe Sport Utility Printer of our product line leads the industry with 4” of print area with a unique 3+2+2+1 head configuration and versatile in-line design. The Envelope Imager XT 4.0’s advanced microprocessor and 64 MB of RAM crunch data like no other printer and the USB 2.0 port works seamlessly with today’s PCs. Our exclusive Five-Channel AccuTrak™ vacuum transport has repositionable outer transport belts and material guides that run under the belts for dead-on registration. Three powerful vacuum fans tenaciously grab material via five channels for consistent pressure. The integrated Cartridge Storage Station keeps cartridge fresh and minimizes waste. Electronic Thickness Control uses a precise servo-motor system to effortlessly set the perfect output pressure. All these features translate to the best print quality possible.","Print Technology\tThermal Inkjet, Eight HP 45A-Style High Capacity Cartridges\nAddress Speed\t\n   34,000 /hour at 150 dpi\n   25,000 /hour at 200 dpi\n   20,000 /hour at 300 dpi\n   11,500 /hour at 600 dpi\n     (9 Lines on 4”x6” Postcard)\t26,000 /hour at 150 dpi\n19,000 /hour at 200 dpi\n15,000 /hour at 300 dpi\n7,200 /hour at 600 dpi\n(9 Lines on #10 Envelopes)\nPrint Quality (Dots Per Inch)\t\n   Description\tDots Per Inch\tResolution\n   High Quality\t600 d.p.i.\t600 x 600 dpi\n   Letter Quality\t300 d.p.i.\t600 x 300 dpi\n   Standard Quality\t200 d.p.i.\t600 x 200 dpi\n   Hi-Speed Quality\t150 d.p.i.\t600 x 150 dpi\nImage Area\t   4” X 17” w/ 12” Vertical Range\nPrint Head Split\t   3 Pen Stitched + 2 Pen Stitched + 2 Pen Stitched + 1 Pen Design\nProcessor\t    AMD TigerSharc 100 MHz DSP with Dual Calculation Technology\nMemory\t   64 MB RAM\nFonts\t   All TrueType fonts available on PC\nPrint Orientation\t   Normal and Reverse\nCounters\t   One operator resettable job counter, one permanent lifetime counter\nInk Monitor\t   Visible on Display\nPrints\t   Allows printing of graphics, logos, and barcodes\nMaterial Size\t   Minimum (W x L):  3\" x 5\"\n   Maximum (W x L):  13.5” x 17”\nMaterial Thickness\t   Up to 3/8”\nFeeder-Capacity\t   Feeder Dependent\nSoftware\t   WindowsTM Printer Drivers for WindowsTM 98,\n   2000, NT, ME, and XP\nPC Interface\t   Parallel and USB 2.0\nDiagnostics\t   Resident in firmware\nFirmware Update\t   Flash PROM update\nDuty Cycle\t   120 million addresses total or 2,000,000 per month over a 5-year life cycle\nDimensions\t   25” H x 28” L x 22” W\nWeight\t   80 lbs\nElectrical\t   115VAC or 240VAC 50/60 Hz\nOptions\t   Conveyor/Stacker/Dryer, Drop Tray",null,"http://www.renausa.com/products/17/envelope-imager-xt-40.html","https://www.youtube.com/watch?v=K9AaP-bvBG8","http://www.renausa.com/2007_line/brochures/RENA_Systems_Env_Img_XT_4-0.pdf","Yes","Yes"]
[null,"XPS PROFESSIONAL MAILER SERIES"]
[null,null,"XPS-PROMAIL CONSOLE SYSTEM","Professional Grade Inkjet Console System\n\nKey Features\n- Heavy Duty Construction\n- 34,000 Per Hour\n- Integrated Productivity Accessories\n- 3\" or 4\" of Available Print\n- Exclusive AccuTrak Vacuum Transport\n- See a close-up of base\n\n\nIntroducing the new inkjet console system from RENA Systems. We completely revamped our professional grade line to offer RENA Systems owners the absolute best upgrade option. The XPS-ProMail System is not a machine-shop approach. It was engineered and designed from the ground up as a high performance inkjet printer - and it shows. The XPS-ProMail System and its accessories are made from steel and aluminum with a duty cycle of 240 million pieces. Best of all, it’s precision engineered and built right here in the USA.","Print Technology\tThermal Inkjet, Six or Eight HP 45A-Style High Capacity Cartridges\nAddress Speed\t\n   34,000 /hour at 150 dpi\n   25,000 /hour at 200 dpi\n   20,000 /hour at 300 dpi\n   11,500 /hour at 600 dpi\n     (9 Lines on 4”x6” Postcard)\t26,000 /hour at 150 dpi\n19,000 /hour at 200 dpi\n15,000 /hour at 300 dpi\n7,200 /hour at 600 dpi\n(9 Lines on #10 Envelopes)\nPrint Quality (Dots Per Inch)\t\n   Description\tDots Per Inch\tResolution\n   High Quality\t600 d.p.i.\t600 x 600 dpi\n   Letter Quality\t300 d.p.i.\t600 x 300 dpi\n   Standard Quality\t200 d.p.i.\t600 x 200 dpi\n   Hi-Speed Quality\t150 d.p.i.\t600 x 150 dpi\nImage Area\t3” or 4\" X 17” w/ 12” Vertical Range\nPrint Head Split\t3 Pen Stitched + 2 Pen Stitched (+ 2 Pen Stitched w/ 4.0) + 1 Pen Design\nProcessor\tAMD TigerSharc 100 MHz DSP with Dual Calculation Technology\nMemory\t64 MB RAM\nFonts\tAll TrueType fonts available on PC\nPrint Orientation\tNormal and Reverse\nCounters\tOne operator resettable job counter, one permanent lifetime counter\nInk Monitor\tVisible on Display\nPrints\tAllows printing of graphics, logos, and barcodes\nMaterial Size\tMinimum (W x L):  3\" x 5\"\nMaximum (W x L):  13.5” x 17”\nMaterial Thickness\tUp to 1-1/4”\nFeeder-Capacity\tFeeder Dependent\nSoftware\tWindowsTM Printer Drivers for WindowsTM 98,\n2000, NT, ME, and XP\nPC Interface\tParallel and USB 2.0\nDiagnostics\tResident in firmware\nFirmware Update\tFlash PROM update\nDuty Cycle\t240 million addresses total or 4,000,000 per month over a 5-year life cycle\nDimensions\t11” H x 14” W x 28” D\nWeight\t75 lbs (printer only)\nElectrical\t115VAC or 240VAC 50/60 Hz\nOptions\tConveyor/Stacker/Dryer, Drop Tray",null,"http://www.renausa.com/products/2/xps-promail-console-system.html","https://www.youtube.com/watch?v=Bcod7P71_h4","http://www.renausa.com/brochures/XPS-ProMail_web.pdf","Yes","Yes"]
[null,null,"XPS-PROMAIL 3.0 & 4.0","Modular Add-on Inkjet System\n\nKey Features\n- Universal Mounting Capability\n- 34,000 Per Hour\n- Unique Contact Roller Control\n- 3\" or 4\" of Available Print\n- 1.25\" Thickness Capability\n- View XPS-ProMail 3.0","Print Technology\t Thermal Inkjet, Six or Eight HP 45A-Style High Capacity Cartridges\nAddress Speed\t\n   34,000 /hour at 150 dpi\n   25,000 /hour at 200 dpi\n   20,000 /hour at 300 dpi\n   11,500 /hour at 600 dpi\n     (9 Lines on 4”x6” Postcard)\t26,000 /hour at 150 dpi\n19,000 /hour at 200 dpi\n15,000 /hour at 300 dpi\n7,200 /hour at 600 dpi\n(9 Lines on #10 Envelopes)\nPrint Quality (Dots Per Inch)\t\n   Description\tDots Per Inch\tResolution\n   High Quality\t600 d.p.i.\t600 x 600 dpi\n   Letter Quality\t300 d.p.i.\t600 x 300 dpi\n   Standard Quality\t200 d.p.i.\t600 x 200 dpi\n   Hi-Speed Quality\t150 d.p.i.\t600 x 150 dpi\nImage Area\t3” or 4\" X 17” w/ 12” Vertical Range\nPrint Head Split\t3 Pen Stitched + 2 Pen Stitched (+ 2 Pen Stitched w/ 4.0) + 1 Pen Design\nProcessor\tAMD TigerSharc 100 MHz DSP with Dual Calculation Technology\nMemory\t64 MB RAM\nFonts\tAll TrueType fonts available on PC\nPrint Orientation\tNormal and Reverse\nCounters\tOne operator resettable job counter, one permanent lifetime counter\nInk Monitor\tVisible on Display\nPrints\tAllows printing of graphics, logos, and barcodes\nMaterial Size\tMinimum (W x L):  3\" x 5\"\nMaximum (W x L):  13.5” x 17”\nMaterial Thickness\tUp to 1-1/4”\nFeeder-Capacity\tFeeder Dependent\nSoftware\tWindowsTM Printer Drivers for WindowsTM 98, 2000, NT, ME, and XP\nPC Interface\tParallel and USB 2.0\nDiagnostics\tResident in firmware\nFirmware Update\tFlash PROM update\nDuty Cycle\t240 million addresses total or 4,000,000 per month over a 5-year life cycle\nDimensions\t11” H x 14” W x 28” D\nWeight\t75 lbs (printer only)\nElectrical\t115VAC or 240VAC 50/60 Hz\nOptions\tConveyor/Stacker/Dryer, Drop Tray",null,"http://www.renausa.com/products/3/xps-promail-30-40.html","https://www.youtube.com/watch?v=Bcod7P71_h4","http://www.renausa.com/brochures/XPS-ProMail_web.pdf","Yes","Yes"]
[null,null,"XPS-PROTAB 4.0 TABBING SYSTEM","Professional Grade Tabber/Labeler/Stamp Affixer\n\nKey Features\n- 35,000 Tabs/Stamps Per Hour\n- 4\" Wide Head Standard.\n- Versatile In-Line Design\n- Applies 1, 2 or 3 Tabs/Stamps At Once\n- Clear, Translucent or Paper Tabs\n- See It Inline With A Full Console System\n- View The Stand Alone System","Tab Materials\tClear, Translucent, or Paper\nTabbing Speed\tSingle Tab: Up to 35,000 pieces per hour\nDouble Tab: Up to 30,000 pieces per hour\nTriple Tab: Up to 20,000 pieces per hour (11” min. piece length)\nLabeling Speed\tFan-Folded Labels: Up to  9,500 pieces per hour*\n1\" x 4\" Roll Labels: Up to 24,000 pieces per hour\n*RENA RS-35-15-1A Only\nMaterial Size\tMinimum (W x L):  3\" x 5\"\nMaximum (W x L):  13” x 17”\nMaterial Thickness\tUp to 1/2”\nLabel Size\tUp To 4” x 7\" wide with supplied Wide Applicator Head\nTab Size\tMIN: 3/4” x 3/4”\nMAX: 2” x 7”\nTab Sensitivity\tAdjusts for density in tab/wafer seals\nReel Capacity\t19” Diameter (3” core)\nNumber Of Tabs\t1, 2, or 3 Tabs\nTab Accuracy\t+/- 1/8”\nFeeder Control\tStart/Stop Control for other RENA Systems Feeders\nProduction Monitors\tLife and Job Count and Production rate and speed\nError Reporting\tYes\nFeatures\tLeft to Right Operation\nCan apply up to three stamps\nSafety\tInterlocks on all adjustments\nEmergency Stop Switch\nDuty Cycle\t120 million addresses total or 2,000,000 per month over a 5-year life cycle\nDimensions\t27” W x 33” D x 71” H\nWeight\t200 lbs\nElectrical\t115VAC or 240VAC 50/60 Hz\nOptions\tConveyor/Stacker/Dryer, Drop Tray",null,"http://www.renausa.com/products/4/xps-protab-40-tabbing-system.html","https://www.youtube.com/watch?v=Bcod7P71_h4","http://www.renausa.com/brochures/XPS-ProTab_web.pdf","Yes","Yes"]
[null,null,"XPS-PRODRY 8.0","Professional Grade Output Options\n\nKey Features\n- 8,000 Watt IR Dryer (Yes 8,000!)\n- Low-Glare Bulbs\n- Controlled From Base\n- Automatic Speed Synchronization\n- Separate 0-100% Intensity Control\n- Emergency Stop/Safety Tilt Switch\n- See It With Our Full Console System","Throughput Speed\t0-300 fpm (Controlled From Base)\nLamp Type\tShort-Wave Quartz Infrared, 1600 Watt, 240 Volt, Ruby Glare-Reduction w/ Gold Reflector (Dryer Uses Five Lamps)\nOutput Load\tVariable Control 0 to 8,000 Watts\nMaterial Size\tMinimum (W x L):  3\" x 5\"\nMaximum (W x L):  15” x 17”\nMaterial Thickness\tUp to 1-1/4”\nFeatures\tRemote Sensor; Material Control Guides\nHeat Removal Vacuum System;  Adjustable Lamp Height.\nSafety\tMaterial Guides, Safety Interlocks, Lamp Timeout, Belt Crawl, Tilt-Switch\nDuty Cycle\t240 million addresses total or 4,000,000 per month over a 5-year life cycle\nLamps Rated for 1-year of Typical Service\nDimensions\t34-39” Deck, 42-47” H x 27” W x 36” D\nWeight\t200 lbs\nElectrical\t220VAC Three-Wire Single Phase 34A (requires 50-60A service)\nOptions\t2,000W Dryer, Drop Tray, Syncs Up To Three Units",null,"http://www.renausa.com/products/5/xps-prodry-80.html","https://www.youtube.com/watch?v=Bcod7P71_h4","http://www.renausa.com/brochures/XPS-ProMail_web.pdf","Yes","Yes"]
[null,null,"XPS-PROFEED SHUTTLE","Professional Grade Vacuum Shuttle Feeder\n\nKey Features\n- 30,000 Piece/hr Throughput\n- Unique Roller + Shuttle Design.\n- Integrated With XPS-ProMail Base\n- Heavy Duty Vacuum Pump\n- View Feed Section Close-Up\n- See It Inline With A Full Console System","Feeder Speed\tUp to 30,000 pieces per hour\nMaterial Size\t3” x 5” to 13” x 17”\nMaterial Thickness\tUp to 5/8”\nMaterial Thickness\tUp to 1/2”\nFeeder Type\tVacuum Shuttle Head\nFeeder Capacity\tUp to 750 #10 Envelopes\nCounter\tOperator Resettable Job Counter\nFeatures\tFour Unique Vacuum Shuttle Heads For Various Materials\nSolid Alloy Separation Assembly\nSafety\tEmergency Stop Switch\nDuty Cycle\t240 million addresses total or 4,000,000 per month over a 5-year life cycle\nDimensions\t34-39” Deck, 51” H x 43” W x 35” D\nWeight\t280 lbs\nElectrical\t115VAC - 10A\nOptions\tBase/Tabber Interface Cable",null,"http://www.renausa.com/products/6/xps-profeed-shuttle.html","https://www.youtube.com/watch?v=Bcod7P71_h4","http://www.renausa.com/brochures/XPS-ProFeed-Shuttle_web.pdf","Yes","Yes"]
[null,null,"XPS-BUMPTURN","Professional Grade Productivity Accessory\n\nKey Features\n- Runs Up To 30,000 Per Hour\n- Rotates Media 90 Degrees\n- Rotates To Left Or Right\n- Lexan Transport Cover\n- Variable Speed Control\n- Tilts To Span Varying Machine Heights","Throughput Speed\t20-500 fpm\nInput Height\tMinimum:  21\"\nMaximum:  35”\nOutput Height\tMinimum:  32\"\nMaximum:  35”\nMaterial Size\tMinimum (W x L):  2\" x 3\"\nMaximum (W x L):  12” x 12”\nMaterial Thickness\tUp to 1/8”\nFeatures\tAngle-Adjust Deck; Rotate Pieces Left or Right.\nSafety\tMaterial Transport Covers & Belt Crawl\nDuty Cycle\t240 million addresses total or 4,000,000 per month over a 5-year life cycle\nDimensions\t19.5”W x 35”L x 33”H\nWeight\t50 lbs\nElectrical\t120 VAC, 3 AMP\nOptions\t2,000W Dryer, Drop Tray, Syncs Up To Three Units",null,"http://www.renausa.com/products/7/xps-bumpturn.html","N/A","http://www.renausa.com/brochures/XPS-BumpTurn_web.pdf","Yes","Yes"]
[null,null,"TB-659 CONVEYOR","Professional Grade Output Options\n\nKey Features\n- Four Repositionable Belts\n- Adjustable Height Legs\n- Variable Speed Controlled From Base\n- Speed Up Sorting Function\n- Connect Three For 18' Of Output\n- Emergency Stop\n- See It With Our Full Console System","Throughput Speed\t0-100 fpm (Controlled From Base)\nMaterial Size\tMinimum (W x L):  3\" x 5\"\nMaximum (W x L):  15” x 17”\nMobility\tLocking Casters\nFeatures\tSpeed Up Function for Sort Breaks\nSynchronized Input/Output Connections\nSafety\tEmergency Stop Switch\nDuty Cycle\t240 million addresses total or 4,000,000 per month over a 5-year life cycle\nDimensions\t18” W x 80” D x 30-36” H\nWeight\t145 lbs\nElectrical\t115VAC or 240VAC 50/60 Hz\nOptions\t2,000W Dryer, Drop Tray, Syncs Up To Three Units",null,"http://www.renausa.com/products/8/tb-659-conveyor.html","https://www.youtube.com/watch?v=Bcod7P71_h4","http://www.renausa.com/brochures/XPS-ProMail_web.pdf","Yes","Yes"]
["Tabbing Systems"]
[null,null,"L-250 LABELER/TABBER","Key Features\n\n- Applies Clear, Translucent & Paper Tabs\n- Applies 1-up Labels\n- 25,000 Pieces/hr\n- Integrated Feeder\n- Holds Standard Rolls (3\" core)\n- Integrated Catch Tray\n\nThe L-250 Tabber is one cool little machine. Most tabbers in its class can do paper tabs only. The durable design of the L-250 gives it the ability to run clear, translucent & paper tabs at speeds up to 25,000 per hour on a typical tri-fold mailer. The new control panel design and professional grade color scheme allow the L-250 Labeler/Tabber to look good in workshops, warehouses, mailrooms and office environments while requiring less maintenance.","Tab Materials\tClear, Translucent, or Paper\nTabbing Speed\t25,000 pieces per hour\n(8.5\" tri-folded mailer)\nMaterial Size\tMinimum (W x L):  3\" x 5\"\nMaximum (W x L):  17” x 11”\nMaterial Thickness\tUp to 5/32”\nFeeder-Capacity\tUp to 300 #10 envelopes\nTab Size\nLabel Size\t5/8\" to 1-1/2\"\n1/2\" to 15\"\nTab Sensitivity\tAdjusts for density in tab/wafer seals\nReel Capacity\t9” Diameter (3” core)\nCounter\t5-digit LCD (operator resettable)\nDuty Cycle\t30 million addresses total or 500,000 per month over a 5-year life cycle\nDimensions\t25\" W x 15.5\" D x 22\" H\nWeight\t40 lbs\nElectrical\t115VAC or 240VAC 50/60 Hz\nOptions\tConveyor/Stacker/Dryer, Drop Tray",null,"http://www.renausa.com/products/18/l-250-labeler-tabber.html","N/A","http://www.renausa.com/brochures/RENA_Systems_L-250.pdf","Yes","Yes"]
[null,null,"L-350 LABELER/TABBER/STAMP AFFIXER","Key Features\n\n- Applies Clear, Translucent & Paper Tabs\n- Applies 1-Up Labels\n- Applies USPS Stamps\n- 25,000 Pieces/hr\n- Integrated Feeder\n- Holds Standard Rolls (3\" core)\n- Wide Paper Path\n\nThe L-350 is a classic jack of all trades. With a proven design that has years of field experience, this unit will run for a long, productive time. It runs clear, translucent and paper tabs at speeds up to 25,000 per hour on a typical tri-fold mailer. The new control panel design and professional grade color scheme allow the L-350 to look good in workshops, warehouses, mailrooms and office environments while requiring less maintenance. With new postal regulations for tabbing and the skyrocketing cost of postage meter supplies, this sweet machine can really make your day.","Tab Materials\tClear, Translucent, or Paper\nTabbing Speed\t25,000 pieces per hour\n(8.5\" tri-folded mailer)\nMaterial Size\tMinimum (W x L):  3\" x 5\"\nMaximum (W x L):  17” x 11”\nMaterial Thickness\tUp to 5/32”\nFeeder-Capacity\tUp to 300 #10 envelopes\nTab Size\nLabel Size\t5/8\" to 1-1/2\"\n1/2\" to 15\"\nTab Sensitivity\tAdjusts for density in tab/wafer seals\nReel Capacity\t9” Diameter (3” core)\nCounter\t5-digit LCD (operator resettable)\nDuty Cycle\t30 million addresses total or 500,000 per month over a 5-year life cycle\nDimensions\t25\" W x 15.5\" D x 22\" H\nWeight\t40 lbs\nElectrical\t115VAC or 240VAC 50/60 Hz\nOptions\tConveyor / Stacker / Dryer, Drop Tray",null,"http://www.renausa.com/products/19/l-350-labeler-tabber-stamp-affixer.html","N/A","http://www.renausa.com/brochures/RENA_Systems_L-350.pdf","Yes","Yes"]
[null,null,"T-250 TABBER","Key Features\n\n- Applies Clear, Translucent & Paper Tabs\n- 12,000 Pieces/hr\n- Integrated Feeder\n- Holds Standard Rolls (3\" core)\n- 17\" Wide Paper Path\n- Can Be Used As A Feeder\n\nThe T-250 Tabber is a great machine. Most tabbers in its class can do paper tabs only. The advanced design of the T-250 gives it the ability to run clear, translucent and paper tabs at speeds of up to 12,000 per hour on a typical tri-fold mailer. The new control panel design and professional grade color scheme allow the T-250 Tabber to look good in workshops, warehouses, mailrooms and office environments while requiring less maintenance.","Tab Materials\tClear, Translucent, or Paper\nTabbing Speed\t12,000 pieces per hour\n(8.5\" tri-folded mailer)\nMaterial Size\tMinimum (W x L):  3\" x 5\"\nMaximum (W x L):  17” x 11”\nMaterial Thickness\tUp to 5/32”\nFeeder-Capacity\tUp to 200 #10 envelopes\nTab Size\t5/8\" to 1-1/2\"\nTab Sensitivity\tAdjusts for density in tab/wafer seals\nReel Capacity\t9” Diameter (3” core)\nCounter\t5-digit LCD (operator resettable)\nDuty Cycle\t30 million addresses total or 500,000 per month over a 5-year life cycle\nDimensions\t25\" W x 15.5\" D x 22\" H\nWeight\t40 lbs\nElectrical\t115VAC or 240VAC 50/60 Hz\nOptions\tConveyor / Stacker / Dryer, Drop Tray",null,"http://www.renausa.com/products/20/t-250-tabber.html","https://www.youtube.com/watch?v=_QKn9_BGXm0","http://www.renausa.com/brochures/RENA_Systems_T-250.pdf","Yes","Yes"]
[null,null,"T-350 HIGH SPEED DUAL TABBER","Key Features\n\n- 18,000 Pieces/hr\n- Applies Clear, Translucent & Paper Tabs\n- Integrated Feeder\n- 300 Piece Hopper\n- Can Run Inline With Other Products\n- Handles Up To 9\" x 12\" Media\n- Uses RENA Fanfolded Tabs\n\nThe T-350 Dual Tabber is ready for work; lots of work. Work that takes its 18,000 pieces per hour throughput speed seriously and makes the T-350 prove itself every day. This is one hard-working tabber that will pay back the investment quickly and effortlessly. The investment is very reasonable and the T-350 is a feature-rich, easy to use dual tabber that offers class-leading precision and functionality with the legendary quality that only RENA offers.\n\nThe high capacity hopper holds over 300 tri-fold mailers for fewer interruptions. The feed hopper assembly can be removed, changing the T-350 from an off-line tabber to an in-line unit, complete with input guides and transport rollers. The most intriguing feature is the Sprocket Tab Drive System the T-350 employs. This design uses 100% mechanical action to place and advance the tabs. The tabs are driven from our innovative center drive sprockets. The integrated sprocket/peel-bar assemblies are adjustable, even while tabs are loaded, so fine-tuning tab placement is incredibly easy. The fanfolded strips are easy to handle and load, with none of the complex threading of roll tabs. The new T-350 from RENA Systems brings high quality and affordability together, the way only RENA can. It is built here in the US (manufactured, not just assembled) by skilled craftsmen. It is quality you can see and feel as the T-350 clicks away at 18,000 pieces per hour.","Tab Materials\tClear, Translucent, or Paper\nTabbing Speed\t18,000 pieces per hour\n(8.5\" tri-folded mailer)\nMaterial Size\tMinimum (L x W):  3.5\" x 5.5\"\nMaximum (L x W):  9” x 12”\nMaterial Thickness\tUp to 1/8”\nFeeder-Capacity\tUp to 300 Tri-Folded Mailers\nTab Size\t13/16\" x 13\"/16\" to 13/16\" x 15/16\"\nTab Capacity\t5,000/sleeve; 30,000/box\nFeeder\tBuilt-in Bottom Fed Friction Feed (Hopper Removes To Run In-Line)\nCounter\t5-digit LCD (operator resettable)\nDuty Cycle\t30 million addresses total or 500,000 per month over a 5-year life cycle\nDimensions\t10.5\" W x 19\" D x 15\" H\nWeight\t40 lbs\nElectrical\t110VAC 60Hz or 220VAC 50Hz | 1A\nOptions\tRENA Fanfold Tabs, Conveyor/Stacker/Dryer, Drop Tray",null,"http://www.renausa.com/products/21/t-350-high-speed-dual-tabber.html","https://www.youtube.com/watch?v=X2Ectpo1LwU","http://www.renausa.com/brochures/RENA_Systems_T-350.pdf","Yes","Yes"]
[null,null,"T-650 MULTI-SIDE TABBER","Key Features\n\n- Applies Tabs To Multiple Sides Of The Same Piece Simultaneously\n- Tabs Up To 25,000 Pieces/hr\n- Applies Clear, Translucent & Paper Tabs\n- Holds Standard Rolls (3\" core)\n- Built-in Registration Assembly\n- View The T-650S w/EASYFeed 120\n- View The T-650S & XT Printer Inline\n\nInnovation is the story with the T-650 tabber. It is quite simply the most technologically advanced tabletop tabbing system we’ve ever offered. In fact, the T-650 can do something that no other tabletop tabbing system on the market can do – apply tabs to the top and side of a mailpiece simultaneously. Even more impressive, it can apply tabs on opposite sides of the same piece (side-to-side tabbing) in a single pass! The ingenious design of the T-650 is really two tabbers in one. The one fixed tab head applies side tabs along an open edge while the repositionable tab head is able to switch from side tabbing to front (or leading edge) tabbing. This versatile design also allows the T-650 to apply stamps, small labels and flat tabs for gate-folded pieces. This really is one machine that can do it all. The T-650 applies clear, translucent or paper tabs with ease in a variety of tab sizes, including the new 1.5” tabs for letter-size booklets. Now, side-to-side booklet tabbing is no longer a difficult task requiring multiple passes or machines. Weather side-to-side tabbing or stamp affixing, the T-650 multi-side tabber/stamp affixer will make your job easier, more productive, profitable and efficient. Its heavy-duty aluminum and steel construction will guarantee you years of reliable, high performance use.","Tab Materials\tClear, Translucent, or Paper\nTabbing Speed\tSingle Tab: Up to 25,000 pieces per hour\nDouble Tab: Up to 15,000 pieces per hour\nTriple Tab: Up to 10,000 pieces per hour (11” min. piece length)\nMaterial Size\tMinimum (W x L):  5\" x 3.5\"\nMaximum (W x L):  11” x 15”\nMaterial Thickness\tUp to 1/4”\nFeeder\tIn-line design works with various input devices\nTab Size\tMIN: 3/4” x 3/4”\nMAX: 1.5” x 1.5”\nTab Sensitivity\tAdjusts for density in tab/wafer seals\nReel Capacity\t9” Diameter (3” core)\nNumber Of Tabs\t1, 2, or 3 Tabs\nTab Accuracy\t +/- 1/16”\nFeeder Control\tStart/Stop Control for RENA Systems Feeders\nProduction Monitors\tLife and Job Count and Production rate and speed\nError Reporting\tYes\nFeatures\tOptional Friction Feeder (EASYFeed 120)\nCan apply up to three tabs/stamps\nSafety\tInterlocks on all adjustments\nEmergency Stop Switch\nDuty Cycle\t30 million addresses total or 500,000 per month over a 5-year life cycle.\nDimensions\t19” W x 26” H x 30” D\nWeight\t75 lbs\nElectrical\t110VAC 50/60 Hz\nOptions\tConveyor/Stacker/Dryer, Drop Tray",null,"http://www.renausa.com/products/22/t-650-multi-side-tabber.html","https://www.youtube.com/watch?v=E51AXm8yZtA","http://www.renausa.com/brochures/RENA_Systems_T-650.pdf","Yes","Yes"]
[null,null,"T-750 INLINE TABBER/STAMP AFFIXER","Key Features\n\n- Applies Clear, Translucent & Paper Tabs\n- Tabs/Stamps 20,000 Pieces/hr\n- Optional Synchronized Feeder\n- Holds Standard Rolls (3\" core)\n- Built-in Registration Assembly\n- View The T-750S w/EASYFeed Lite\n\nThe T-750 Inline Tabber can apply tabs or stamps at speeds over 20,000 per hour. It has the ability to single, double and triple tab. It can run clear, translucent, or paper tabs all while running inline with several of our inkjet address printers. The automatic speed integration of our EASYFeed Lite feeder option makes the T-750 one affordable stand-alone tabber that outperforms all challengers. It has our new intelligent system control software that is easier to use and offers exclusive features like Automatic Tab Positioning and Automatic Length Measuring.","Tab Materials\tClear, Translucent, or Paper\nTabbing Speed\tSingle Tab: Up to 20,000 pieces per hour\nDouble Tab: Up to 12,000 pieces per hour\nTriple Tab: Up to 8,000 pieces per hour (11” min. piece length)\nMaterial Size\tMinimum (W x L):  3\" x 5\"\nMaximum (W x L):  13” x 17”\nMaterial Thickness\tUp to 3/8”\nFeeder\tIn-line design works with various input devices\nTab Size\tMIN: 3/4” x 3/4”\nMAX: 1.5” x 1.5”\nTab Sensitivity\tAdjusts for density in tab/wafer seals\nReel Capacity\t14” Diameter (3” core)\nNumber Of Tabs\t1, 2, or 3 Tabs\nTab Accuracy\t+/- 1/16”\nFeeder Control\tSynchronized Speed Control with EASYFeed Lite\nStart/Stop Control for other RENA Systems Feeders\nProduction Monitors\tLife and Job Count and Production rate and speed\nError Reporting\tYes\nFeatures\tOptional Synchronized Feeder (EASYFeed Lite)\nCan apply up to three stamps\nSafety\tInterlocks on all adjustments\nEmergency Stop Switch\nDuty Cycle\t60 million addresses total or 1,000,000 per month over a 5-year life cycle.\nDimensions\t25” W x 27” H x 25” L (41” with EASYFeed Lite\nWeight\t90 lbs\nElectrical\t115VAC or 240VAC 50/60 Hz\nOptions\tConveyor/Stacker/Dryer, Drop Tray",null,"http://www.renausa.com/products/23/t-750-inline-tabber-stamp-affixer.html","https://www.youtube.com/watch?v=ldrAQaPYiEU","http://www.renausa.com/brochures/RENA_Systems_T-750.pdf","Yes","Yes"]
[null,null,"T-950 INLINE TABBER/LABELER/STAMP AFFIXER","Key Features\n\n- Tabs/Stamps 35,000 Pieces/hr\n- Applies Clear, Translucent & Paper Tabs\n- Automatic Tab Positioning\n- Holds Standard Rolls (3\" core)\n- Available In Console Form (XPS-ProTab 4.0)\n- View The T-950S w/EASYFeed 120\n\nThe T-950 Tabber is the best high-speed system we have ever offered. It doesn’t just have high speed ratings like the competition; it runs and runs smoothly at over 35,000 per hour. Just watch our video. While the competition is vibrating and thrumming at less than 30,000 per hour, the T-950 runs like a fine European sports car. Fast, but controlled. Stamps? Check. Labels? Yep. Clear, Translucent, or Paper tabs? Of course. It can apply up to three tabs per pass and can apply multiple stamps at one time – something no other system can do. It has a precision cam system that raises the entire head to handle material 1/2\" thick. It also tabs from the front or back of the transport. The massive 16” reel capacity holds enough tabs to run uninterrupted for an hour straight – true productivity.","Tab Materials\tClear, Translucent, or Paper\nTabbing Speed\tSingle Tab: Up to 35,000 pieces per hour\nDouble Tab: Up to 30,000 pieces per hour\nTriple Tab: Up to 20,000 pieces per hour\n(11” min. piece length)\nLabeling Speed\tFan-Folded Labels: Up to  9,500 pieces per hour*\n1\" x 4\" Roll Labels: Up to 24,000 pieces per hour\n*RENA RS-35-15-1A Only\nMaterial Size\tMinimum (W x L):  3\" x 5\"\nMaximum (W x L):  13” x 17”\nMaterial Thickness\tUp to 1/2”\nLabel Size\tUp To 4” x 7\" wide with supplied Wide Applicator Head\nTab Size\tMIN: 3/4” x 3/4”\nMAX: 2” x 7”\nTab Sensitivity\tAdjusts for density in tab/wafer seals\nReel Capacity\t19” Diameter (3” core)\nNumber Of Tabs\t1, 2, or 3 Tabs\nTab Accuracy\t+/- 1/8”\nFeeder Control\tStart/Stop Control for other RENA Systems Feeders\nProduction Monitors\tLife and Job Count and Production rate and speed\nError Reporting\tYes\nFeatures\tLeft to Right Operation\nCan apply up to three stamps\nSafety\tInterlocks on all adjustments\nEmergency Stop Switch\nDuty Cycle\t120 million addresses total or 2,000,000 per month over a 5-year life cycle\nDimensions\t27” W x 33” D x 37” H\nWeight\t150 lbs\nElectrical\t115VAC or 240VAC 50/60 Hz\nOptions\tConveyor/Stacker/Dryer, Drop Tray",null,"http://www.renausa.com/products/24/t-950-inline-tabber-labeler-stamp-affixer.html","https://www.youtube.com/watch?v=VVmuDdRbRrQ","http://www.renausa.com/brochures/RENA_Systems_T-950.pdf","Yes","Yes"]
["Mailing Software"]
[null,null,"SATORI SOFTWARE","Powerfully advanced mailing software\n\nMake your mailing operation much more productive with Bulk Mailer — prepare USPS® compliant mailings faster and more easily. Achieve increased mail deliverability and the lowest postage rates all while avoiding the aggravation of deciphering complex postal regulations. This next generation of the Bulk Mailer series sports a sophisticated new interface and the option to upgrade to a Microsoft® SQL Server database for faster performance with the largest address data files.\n\nUnsurpassed Mail Preparation\n\nBulk Mailer is a full-featured, remarkably productive mailing software package, available in three versions designed to meet your specific needs:\n\nThe graphical interface for Bulk Mailer virtually walks users through each mailing preparation step.\nPAVE™ Certified\nIncludes advanced support for First-Class Mail®, Periodicals, Standard Mail®, and all reports and postage statements\nCASS Certified™ \nAddress Correction cleans, standardizes, uses DPV™ to confirm deliverability then adds ZIP + 4® codes and generates USPS® Form 3553\nReal-Time* NCOALink® service\nUpdate addresses of those who have moved BEFORE you mail via the Internet\nExtraordinary Data Exchange\nEasy and powerful import capabilities — plus you can even copy and paste to/from Microsoft® Excel®\nDuplication Search \nA variety of de-duplication options ensure the best results\nJob Builder \nAvailable in Bulk Mailer Professional and Business, Job Builder allows you to save a series of tasks into a template for automated execution.\nAddress Printer Support \nModel specific features are built-in, giving you the most from your high-speed address printer\nOptional Add-Ons\nChoose among Package Services sorts, Mixed-Weights sorts, Palletization, Geocode, International data sets and more\n\nEasy-to-use wizards guide users through address quality operations which include CASS processing, change-of-address updates, duplication elimination, and the optional list merge & purge functions.\n\nIntelligent field mapping and reusable templates make importing and exporting data fast and error free.\n\nAvailable in Bulk Mailer Professional & Business, the Job Builder allows you to save a series of tasks into a template for automated execution.\n\nModern, State-of-the-Art Interface\nBulk Mailer brings a revolutionary design to the mailing industry.\n\nAdvanced graphics\nMakes unlocking the power of Bulk Mailer easy\nWizard-based processes\nMakes complicated tasks error-free\nTemplate architecture\nSave frequently used tasks as reusable templates and save time\nGraphical label designer\nFull graphics, bar-coding and mail preparation capability within a cutting edge designer\nLive Links Keep You Current & Informed\nBulk Mailer is never static it is designed for the Internet age.\n\nLive Updates\nBulk Mailer checks for new versions via the Internet and notifies you of updates\nDynamic Resource Center\nHelp and mailing industry information are just a click away\nLinks to Satori Software\nEmail and Web site links built into the software make sending feedback quick and easy","Satori Bulk Mailer Series - Feature Comparison\nNow any size mailing operation can reap the benefits of increased address quality and maximum postage discounts. The three editions of Bulk Mailer, Business, Professional and Standard, deliver the right set of features needed by your organization. Bulk Mailer Business offers the most flexibility and advanced features, while those with small lists may be satisfied with the Standard edition.\n\nBulk Mailer Version\nFEATURE        STANDARD        PROFESSIONAL        BUSINESS\nAddress record limit        5000        up to 1 million        unlimited\nMicrosoft SQL Server database                          \nMultiuser environment                          \nCASS Certified™ for address correction:\nIncludes DPV®, LACSLink® and SuiteLink™ processing\n                \nPAVE™ certified postal presorting:\nFirst-Class Mail®, Standard Mail® and Periodicals\n                \nBuilt-in real-time* NCOALink® service        optional                \nAdds missing postal data:\nZIP + 4™, carrier route, eLOT® and more\n                \nDuplication removal                        \nEntry point discounts:\nSCF, BMC, ADC and DDU                        \nEnhanced sorts:\nCarrier route, walk sequence, automation and non-automation                        \nUSPS documents and qualification report:\nPS form 3553, 3602, 3541, and 3600                        \nGraphical mail piece designer                        \nHigh-speed printer support and drivers                        \nBarcoded sack and tray labels                        \nIntelligent Mail® barcode support                        \nUser-defined fields        22        22        unlimited\nJob Builder                         \nAdvanced PAVE Gold certified presorting:\nPackage Services, Mixed Weights, Palletization, Firm Bundles                 optional        optional\nMail.dat file generation                 optional        optional\nMerge/Purge                 optional        optional\nRDI™ Interface                 optional        optional\nGeocoding                 optional        optional\nLive Update                        \nFree online training                        \nToll-free technical support        unlimited        unlimited",null,"http://www.renausa.com/products/25/satori-software.html","N/A","http://www.renausa.com/brochures/Bulk-Mailer-brochure2010.pdf","Yes","Yes"]
["Digital Color Printing"]
[null,null,"MACH 8 DIGITAL COLOR DOCUMENT PRINTER","Key Features\n\n- 60 pages/min\n- Full bleed capability for up to 8.5\" x 14\" documents\n- 5,000 single sheet feeder capacity\n- Automatic Capping & Cleaning Station\n- Five 250 mL ink tanks (CMYKK)\n- Optional Automatic High Capacity Output Stacker\n\n \n\nThe MACH 8 digital color printer incorporates the innovative inkjet technology from Memjet® which has made the MACH 5 color printer so successful. The MACH 8 specializes in high-volume document printing, with a high-capacity feeder and optional automatic output stacker (MACH 8S). You get high volume production color at inkjet cost.\n\nThis machine produces beautiful print quality and impressive throughput speed. The MACH 8 is capable of printing 1600 x 800 dots per inch print quality while printing 12 inches per second and 1600 x 1600 dpi resolution at 6 inches per second, reaching speeds of 60 letter size pages per minute! Memjet technology gives the MACH 8 the ability to do this with its stationary printhead that has over 70,000 jet nozzles. To top it off, the affordable 250 ml ink tanks enable you to print long runs for maximum efficiency.\n\nPrint letters, legal documents, cut sheet labels, invoices, proposals and more in full color, affordable style. Any 8.5” x 11” document can have color running off the edges of the page — that means no more white borders!\n\nBetter yet, the MACH 8’s most remarkable feature is the ability to print up to 5,000 pages (10 reams) continuously. You won’t have to stop to reload the paper. The unique high-capacity feeder mechanically moves up and down to accommodate the amount of paper that is loaded before a job is printed. The automatic output stacker does the same as it adjusts itself to catch the output of the job.","Print Resolution\n\nBest Mode: 1600 x 1600 dpi\nNormal Mode: 1600 x 800 dpi\nSpeed\tUp to 3600 letter size pages per hour\nPrint Area\tUp to 8.5\" W to 14.5\" L with full bleed capability\nMaterial Size      \tMIN: 3\" W x 4.2\" L    MAX: 9\" W x 14.5\" L\nMaterial Thickness\tUp to 1/48\" (0.5 mm / 430 gsm / 160# Cover / 240# Index\nFeeder Capacity\t5,000 single sheets (10 reams)\nDuty Cycle\t350,000 per month\nSoftware\tWindows Printer Drivers for Windows XP, Vista, 7, 8\nInk\tDye-based ink. 5 individual 250 ml tanks (CMYKK)\nPrint Cartridge\tMemjet Replaceable Printhead\nPC Interface\tUSB 2.0\nNetwork Interface\tEthernet Port\nAccessory Interface\tPort for connecting optional Automatic High Capacity Output Stacker\nElectrical\t110 VAC, 50/60 Hz (220-240 VAC, 50/60 Hz available)\nDimensions\t23\" W x 33.5\" L x 37.5\" H\nWeight\t175 lbs (79 kg)\nOptions\tAutomatic High Capacity Output Stacker",null,"http://www.renausa.com/products/47/mach-8-digital-color-document-printer.html","https://www.youtube.com/watch?time_continue=169&v=WwkyqHble-A","http://www.renausa.com/brochures/mach-8-digital-color-document-printer.pdf","Yes","Yes"]
[null,null,"MACH 5 DIGITAL COLOR PRINTER","Key Features:\n\n- 7,500 envelopes/hr\n- Full bleed capability\n- Automatic Capping & Cleaning Station\n- Built-in Top Load Friction Feeder\n- Five 250 mL ink tanks (CMYKK)\n \n\nWith exceptional technology from Memjet, The Mach 5 Digital Color Printer is unlike any other envelope printer in its class. It’s fast, reliable, AND it will boost your return on investment. You will ask yourself how your business ever survived without it!\n\n \n\nThe Mach 5 is capable of printing full color at 6 inches per second and an amazing 1600 x 1600 dots per inch. The faster option is 1600 x 800 dpi at 12 inches per second which still produces a clear image. This means you will be producing up to 7,500 pieces per hour! The Mach 5 clearly wins out over the 1200 dpi at 3,000 pieces per hour of LED or laser printers.  That’s because Memjet packed five ink channels (Cyan, Yellow, Magenta, Black, and Black) into the single 8.77” wide print bar. Inside these channels is a whopping 70,400 nozzles from which the ink is sprayed onto the substrate.\n\n \n\nIf you want a cost-efficient machine, the Mach 5 is just that. The five ink tanks each hold 250 mL of ink for long job runs and low cost per piece. If your business is looking for a machine that will produce short runs, the Mach 5 is perfect for that as well. Print what you need, when you need it. It will eliminate outdated cardstock and free you up on storage.\n\n \n\nWhen paired with mColor, a color management software, you can match the exact color of your company's logo in no time using spot color adjustment. Click here to learn more.","Speed\n\nUp to 3,600 pages per hour (1600 x 800 dpi @ 12 ips - 8.5\" x 11\" sheets)\nUp to 7,500 #10 envelopes per hour (1600 x 800 dpi @ 12 ips)\nMaterial Size\tMIN: 3\" W x 4-1/8\" L    MAX: 9.5\" W x 17\" L\nMaterial Thickness           \tUp to 1/48\" (0.5mm / 430 gsm / 160# Cover / 240# Index)\nPrint Quality\tNormal (1600 x 800 dpi @ 12 ips); Best (1600 x 1600 dpi @ 6 ips)\nTechnology\tMemjet Thermal Inkjet\nInk Capacity\tCyan (250 ml); Yellow (250 ml); Magenta (250 ml); Black (500 ml)\nPrint Area\t8.5\" x 17\" with full bleed capability\nColor Matrix\tUp to 16.8 million colors\nFeeder\tTop Load Friction Feeder Built-In\nPC Interface\tUSB & ETHERNET\nFirmware Update \tElectronic Download via PC Connection\nTransport\tPressure Roller System with Star Rollers\nFeatures\tFull color inkjet; fixed head design; high capacity ink tanks; automatic printhead cleaning and capping service station\nFonts\tAll available TruType or Postscript system fonts\nDimensions\t24\" W x 18\" H x 20\" D\nWeight\t90 lbs\nElectrical\t110-240 VAC 60Hz / 2A\nOptions\tConveyors & IR Dryers; Satori Bulk Mailer Software\nDuty Cycle\t30 million pieces total or 500,000 per month over a 5-year life cycle",null,"http://www.renausa.com/products/15/mach-5-digital-color-printer.html","N/A","http://www.renausa.com/brochures/mach-5-digital-color-printer.pdf","Yes","Yes"]
[null,null,"MCOLOR SOFTWARE","mColor was created to bring professional grade color printing to the Mach 5. In a nutshell, it's an advanced color management and job workflow tool that is simple to use. It includes spot color adjustment which allows you to painlessly match existing logo colors. You can be anywhere on the network to submit, manage, and preview jobs.\n\nmColor processes artwork through a Harlequin RIP (Raster Image Processing). The RIP takes files and converts them into printing data with more accurate color output using embedded ICC profiles expertly created for the Mach 5 printer. The built-in ICC color profiles created by color experts insure the best possible output on a wide variety of papers. mColor lets you print out a swatch sheet on your media and pick the desired output. Fast and easy!\n\nGlobal color adjustment allows the operator to make quick last minute adjustments, or when adjusting spot colors are not the right solution. This comes in handy when using photographs, for example.","N/A",null,"http://www.renausa.com/products/41/mcolor-software.html","N/A","N/A","Yes","Yes"]
[null,null,"MACH X DIGITAL COLOR LABEL PRINTER","Key Features\n\n- Brilliant full color quality at 1600 x 1600 dpi\n- Roll-to-roll design for high productivity and ease of use\n- Digital platform allows for instant changes\n- Ultrafast color label printing at speeds up to 12 inches per second\n\n\nThe Mach X Digital Color Label Printer is the perfect production solution for efficient modern label printing needs. You can produce brilliant full color on rolls up to 9\" wide and 10\" in diameter. It is a fully digital inkjet label printer and it's the answer to your label printing needs. No setup costs, no plates, no production minimums. Print labels for almost anything you can imagine: wine, snacks, tools, household products, you name it. The great thing about this label printer is that it allows you to print short runs so you can save time and money on stock and also eliminate waste from outdated stock.","Speed\n\n6 inches per second; 30 feet per minute (BEST mode)\n12 inches per second; 60 feet per minute (NORMAL mode)\nMaterial Size\tMIN: 2\" wide rolls   MAX: 9\" wide rolls\nMaterial Thickness           \tUp to 13 pt (0.33 mm / 285 gsm / 158# Index)\nPrint Quality\tNormal (1600 x 800 dpi); Best (1600 x 1600 dpi)\nTechnology\tMemjet Inkjet System & dye-based inks\nInk Capacity\tCyan (250 ml); Yellow (250 ml); Magenta (250 ml); Black (500 ml)\nPrint Area\tUp to 8.5\" W x 30\" L with full bleed capability\nMedia Types\tRolls or fanfolded label stock\nMedia Handling\tAutofeed web design with integrated batch cutter\nMedia Sensing\tLabel gap, tick marks, notches\nRoll Capacity\tOptional unwinder & winder can hold up to 10\" O.D. Rolls. Prints up to \n500' continuously before cleaning is required.\nInterface\tUSB & Ethernet with Electronic Firmware Uploading\nFeatures\tFull color inkjet; fixed head design; high capacity ink tanks; automatic printhead cleaning and capping service station\nFonts\tAll available TruType or Postscript system fonts\nBarcodes\tAll available system or software barcodes\nDimensions\tPrinter: 22\" W x 12\" H x 19\" D; With both Winders: 44\" W\nWeight\tPrinter: 75 lbs; 115 lbs with both Winders\nElectrical\t110-240 VAC 60Hz / 2A\nOptions\tRoll unwinder for feeding; roll winder for take-up; Console table;\nmColor RIP & Workflow Software",null,"http://www.renausa.com/products/42/mach-x-digital-color-label-printer.html","https://www.youtube.com/watch?v=02c-Dz65Ge8","http://www.renausa.com/brochures/mach-x-digital-color-label-printer.pdf","Yes","Yes"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]

{"sheet":"Supplies","index":4,"n_rows":101,"n_cols":11,"rows_kept":101,"cut":false,"hidden":false,"merged":[]}
["Category","Sub-Category (if applicable)","Product Name","Product Description","Specifications","Serial #","Vendor Site URL","Video Content URL(s)","Downloadable Content URL(s)","Pictures Saved?","Alternative Site URL"]
["Inking Supplies"]
[null,null,"M5PRINT - H","HJ950C MEMJET 1600DPI PRINTHEAD",null,"A0004376",null,null,null,"Yes"]
[null,null,"M5C250 - H","HJ950 MEMJET 250-ml INK TANK - CYAN",{"$nulls":5},"Yes"]
[null,null,"M5K250 - H","HJ950 MEMJET 250-ml INK TANK - BLACK",{"$nulls":5},"Yes"]
[null,null,"M5M250 - H","HJ950 MEMJET 250-ml INK TANK - MAGENTA",{"$nulls":5},"Yes"]
[null,null,"M5Y250 - H","HJ950 MEMJET 250-ml INK TANK - YELLOW",{"$nulls":5},"Yes"]
[null,null,"M5PACK - H","HJ950 MEMJET INK TANK SET - CYMKK (1 pack of 5)",{"$nulls":5},"Yes"]
[null,null,"IH3INK","IH/IN 360 INK CARTRIDGE",null,"4135554T",null,null,null,"Yes"]
[null,null,"IHINK67","IH/IN SERIES 600/700/800 STANDARD CAPACITY INK CARTRIDGE",null,"4135554T",null,null,null,"Yes"]
[null,null,"IHINK67HC","IH/IN SERIES 600/700/800 HIGH CAPACITY CAPACITY INK CARTRIDGE",null,"4145711Y",null,null,null,"Yes"]
[null,null,"IMINK2","IM280 SERIES INK CARTRIDGE",null,"4145144H",null,null,null,"Yes"]
[null,null,"IMINK34","IM330 STANDARD CAPACITY INK CARTRIDGE",null,"4135554T",null,null,null,"Yes"]
[null,null,"IMINK34","IM350 STANDARD CAPACITY INK CARTRIDGE",null,"4135554T",null,null,null,"Yes"]
[null,null,"IMINK34","IM420 STANDARD CAPACITY INK CARTRIDGE",null,"4135554T",null,null,null,"Yes"]
[null,null,"IMINK34","IM440 STANDARD CAPACITY INK CARTRIDGE",null,"4135554T",null,null,null,"Yes"]
[null,null,"IMINK34","IM460 STANDARD CAPACITY INK CARTRIDGE",null,"4135554T",null,null,null,"Yes"]
[null,null,"IMINK34","IM480 STANDARD CAPACITY INK CARTRIDGE",null,"4135554T",null,null,null,"Yes"]
[null,null,"IMINK4HC","IM440 HIGH CAPACITY INK CARTRIDGE",null,"4145711Y",null,null,null,"Yes"]
[null,null,"IMINK4HC","IM460 HIGH CAPACITY INK CARTRIDGE",null,"4145711Y",null,null,null,"Yes"]
[null,null,"IMINK4HC","IM480 HIGH CAPACITY INK CARTRIDGE",null,"4145711Y",null,null,null,"Yes"]
[null,null,"IM56INK","IM5000/6000 SERIES INK TANK",null,"4137700D",null,null,null,"Yes"]
[null,null,"WJ20INK1","WJ20 SERIES INK CARTRIDGE",null,"3300262X",null,null,null,"Yes"]
[null,null,"WJ69INK","WJ60/90/95/110 SERIES HIGH CAPACITY INK CARTRIDGE",null,"4139518X",null,null,null,"Yes"]
[null,null,"WJ69INK2","WJ60/90/95/110 SERIES STANDARD CAPACITY INK CARTRIDGE",null,"4139519Y",null,null,null,"Yes"]
[null,null,"WJINK-1","WJ135/150/180/185/215 SERIES HIGH CAPACITY INK CARTRIDGE",null,"4129534P",null,null,null,"Yes"]
[null,null,"WJINK-2","WJ135/150/180/185/215 SERIES STANDARD CAPACITY INK CARTRIDGE",null,"4139545A",null,null,null,"Yes"]
[null,null,"220INKR","WJ220 INK RESERVOIR/TANK",null,"4150548M",null,null,null,"Yes"]
[null,null,"250INKR","WJ250 INK RESERVOIR/TANK",null,"4150549N",null,null,null,"Yes"]
[null,null,"INKHD","WJ220/250 INK HEAD/CARTRIDGE",null,"4139553J",null,null,null,"Yes"]
[null,null,"PROINK","WJPRO INK RESERVOIR/TANK - BLUE",null,"4133780V",null,null,null,"Yes"]
[null,null,"PROINK5","WJPRO INK RESERVOIR/TANK - BLUE (1 PACK OF 5)",null,"4133780V",null,null,null,"Yes"]
[null,null,"PROPH","WJPRO INK HEAD/CARTRIDGE - BLUE",null,"4139560R",null,null,null,"Yes"]
[null,null,"PROPH5","WJPRO INK HEAD/CARTRIDGE - BLUE (1 PACK OF 5)"," ","4139560R",null,null,null,"Yes"]
[null,null,"C8842A","RENA HP FAST DRY VERSATILE BLACK CARTRIDGE",{"$nulls":5},"Yes"]
[null,null,"C9050A","RENA EASYINK AQUEOUS CARTRIDGE",{"$nulls":5},"Yes"]
[null,null,"PG - 51645A","DATAPAC INK CARTRIDGE REMANUFACTURED",{"$nulls":5},"Yes"]
["Metering Supplies"]
[null,null,9004010.0,"WJ/IM400 SERIES FULL TAPE - 1000 PER BOX",{"$nulls":5},"Yes"]
[null,null,9004020.0,"WJ/IM400 SERIES HALF TAPE - 1000 PER BOX",{"$nulls":5},"Yes"]
[null,null,"BT1H/PC2H","POSTAGE SHEETS 75 PACK FOR WJ20/IM280/IM300/350/IH360",{"$nulls":5},"Yes"]
[null,null,"PT1H03","IM420/440/460/480/IH600/IH700/IH750 METER TAPES - SINGLE STRIPS - 300 PER PACK",{"$nulls":5},"Yes"]
[null,null,"PT2H03","IM420/440/460/480/IH600/IH700/IH750 METER TAPES - DOUBLE STRIPS - 300 PER PACK",{"$nulls":5},"Yes"]
[null,null,"PT1H12","IM5000/6000 METER TAPES - SINGLE STRIPS - 1200 PER PACK",{"$nulls":5},"Yes"]
[null,null,"PT2H12","IM5000/6000 METER TAPES - DOUBLE STRIPS - 1200 PER PACK",{"$nulls":5},"Yes"]
[null,null,"IMROLLTAPE","IM5000/6000 ROLL TAPE - 260 PER ROLL - 10 ROLLS PER BOX",{"$nulls":5},"Yes"]
[null,null,"WJR30/5R","WJR30 SERIES ROLL TAPE DISPENSER TAPE ROLLS - 600 LABELS PER ROLL - 5 ROLLS PER BOX",{"$nulls":5},"Yes"]
[null,null,"PC2H/BT1H","POSTAGE SHEETS 75 PACK FOR WJ20/IM280/IM300/350/IH360",{"$nulls":5},"Yes"]
[null,null,"PT/502PERFU/150","5\" x 3 1/2\" 2-UP SHEETS - PERFORATED - 300 APPLICATIONS PER BOX",{"$nulls":5},"Yes"]
[null,null,"PT/525FPN/300","4 3/8\" X 1 9/16\" - OVERALL 5 1/4 \" LONG SINGLE USE TAPES - 300 TAPES PER BOX",{"$nulls":5},"Yes"]
[null,null,"PT/600FPN/300","6\" X 1 9/16\" WITH 3/4\" PEEL TAB - 300 TAPES PER BOX",{"$nulls":5},"Yes"]
[null,null,"PT/700FPN/300","7\" X 1 9/16\" HALF TAPE (DOUBLE TAPE) - 300 SHEETS PER BOX",{"$nulls":5},"Yes"]
["Thermal Labels"]
[null,null,"L-10010036 ( C )","1\" X 3\" ZEBRA LABEL - 840 LABELS PER ROLL - 6 ROLLS PER CASE",{"$nulls":5},"Yes"]
[null,null,"L-225-200 DTE","2.25\" X 2\" DIRECT THERMAL LABEL - 725 LABELS PER ROLL",{"$nulls":5},"Yes"]
[null,null,"L-225-200 DTE ( C )","2.25\" X 2\" DIRECT THERMAL LABEL - 725 LABELS PER ROLL - 12 ROLLS PER CASE",{"$nulls":5},"Yes"]
[null,null,"L-400-300 DTE","4\" X 3\" DIRECT THERMAL LABEL - 500 LABELS PER ROLL",{"$nulls":5},"Yes"]
[null,null,"L-400-300 DTE ( C )","4\" X 3\" DIRECT THERMAL LABEL - 500 LABELS PER ROLL - 18 ROLLS PER CASE",{"$nulls":5},"Yes"]
[null,null,"L-400-600 DTE","4\" X 6\" DIRECT THERMAL LABELS (FOR NEOSHIP) - 250 LABELS PER ROLL",{"$nulls":5},"Yes"]
["Sealing Solutions"]
[null,null,"PSEAL/GAL","MAILING & INSERTING MACHINE SEALING SOLUTION (Contains 1 Gallon)",{"$nulls":5},"Yes"]
[null,null,"PSEAL/QUART","MAILING & INSERTING MACHINE SEALING SOLUTION (Contains 1 Quart)",{"$nulls":5},"Yes"]
["Tabs"]
[null,null,"HT10TR11KNP","1 INCH ROUND TRANSLUCENT TABS, NON-PERF - 11,000 PER 9 INCH ROLL",{"$nulls":5},"Yes"]
[null,null,"HT10TR11KNP ( C )","1 INCH ROUND TRANSLUCENT TABS, NON-PERF - 11,000 PER 9 INCH ROLL; (Case of 12 rolls)",{"$nulls":5},"Yes"]
[null,null,"HT15TR7KNP","1.5 INCH ROUND TRANSLUCENT TABS, NON-PERF - 7000 PER 9 INCH ROLL",{"$nulls":5},"Yes"]
[null,null,"HT15TR7KNP ( C )","1.5 INCH ROUND TRANSLUCENT TABS, NON-PERF - 7000 PER 9 INCH ROLL (Case of 8 rolls)",{"$nulls":5},"Yes"]
["Postal Bag - Sack - Tray Tags"]
[null,null,"LT325 - 200 - 4","POSTAL TRAY TAG 3 1/4\" X 2\" 7 PT WHITE LASER TAG; 1 CTN OF 400 SHEETS/10 TAGS PER SHEET",{"$nulls":5},"Yes"]
[null,null,"LT325 - 200 PK - 4","POSTAL TRAY TAG 3 1/4\" X 2\" 7 PT PINK LASER TAG; 1 CTN OF 400 SHEETS/10 TAGS PER SHEET",{"$nulls":5},"Yes"]
[null,null,"LT3375 - 9375 - 4","POSTAL TRAY TAG 3 3/8\" X 15/16\" 7 PT WHITE LASER TAG; 1 CTN OF 400 SHEETS/20 TAGS PER SHEET",{"$nulls":5},"Yes"]
[null,null,"LT3375 - 9375 PK - 4","POSTAL TRAY TAG 3 3/8\" X 15/16\" 7 PT PINK LASER TAG; 1 CTN OF 400 SHEETS/20 TAGS PER SHEET",{"$nulls":5},"Yes"]
["Shaped-Based Pricing"]
[null,null,"SBPGUIDE2","PLASTIC SBP RATE CLASSIFICATION GUIDE",{"$nulls":5},"Yes"]
["Shredder Supplies"]
[null,null,"PB4","SHREDDER BAGS (1 box of refills); 100 BAGS PER BOX",{"$nulls":5},"Yes"]
["Miscellaneous"]
[null,null,"PANASONIC TOUGHPAD BATTERY","PANASONIC TOUGHPAD BATTERY FOR WITS MOBILE DEVICES",{"$nulls":5},"Yes"]
[null,null,"DATALOGIC ELF BATTERY","DATALOGIC ELF BATTERY STANDARD CAPACITY",{"$nulls":5},"Yes"]
[null,null,"DWECERT695-1MH","6 X 9.5 DBL WINDOW CERTIFIED ENVELOPES - QTY 1000",{"$nulls":5},"Yes"]
[null,null,"DWECERT695-10MH​","6 X 9.5 DBL WINDOW CERT ENVELOPES - QTY 10,000",{"$nulls":5},"Yes"]
[null,null,"DWECERT10H-500","#10 DOUBLE WINDOW CERTIFIED MAIL ENVELOPES - QTY 500",{"$nulls":5},"Yes"]
[null,null,"DWECERT10H-500","#10 DOUBLE WINDOW CERTIFIED MAIL ENVELOPES - QTY 500",{"$nulls":5},"Yes"]
[null,null,"DWECERT9512H-10​0","9.5\" X 12\" DOUBLE WINDOW CERTIFIED MAIL ENVELOPE - QTY 100",{"$nulls":5},"Yes"]
[null,null,"DWECERT9512H","9.5\" X 12\" DOUBLE WINDOW CERTIFIED MAIL ENVELOPE - QTY 500",{"$nulls":5},"Yes"]
[{"$nulls":9},"No"]
[{"$nulls":9},"No"]
[{"$nulls":9},"No"]
[{"$nulls":9},"No"]
[{"$nulls":9},"No"]
[{"$nulls":9},"No"]
[{"$nulls":9},"No"]
[{"$nulls":9},"No"]
[{"$nulls":9},"No"]
[{"$nulls":9},"No"]
[{"$nulls":9},"No"]
[{"$nulls":9},"No"]
[{"$nulls":9},"No"]
[{"$nulls":9},"No"]
[{"$nulls":9},"No"]
[{"$nulls":9},"No"]

{"sheet":"Formax","index":5,"n_rows":163,"n_cols":12,"rows_kept":163,"cut":false,"hidden":false,"merged":[[114,3,118,3],[5,3,6,3],[3,2,4,2],[3,3,4,3],[5,2,6,2],[8,2,9,2],[8,3,9,3],[31,3,32,3],[31,2,32,2],[8,6,9,6],[31,6,32,6],[31,9,32,9],[31,8,32,8],[31,10,32,10],[8,10,9,10],[119,10,123,10],[114,10,118,10],[5,10,6,10],[5,9,6,9],[8,9,9,9],[8,8,9,8],[3,9,4,9],[3,8,4,8],[3,6,4,6],[5,6,6,6],[3,10,4,10],[5,8,6,8],[119,8,123,8],[114,8,118,8],[119,9,123,9],[114,9,118,9],[119,2,123,2],[119,3,123,3],[119,6,123,6],[114,6,118,6],[114,2,118,2]]}
["Category","Sub-Category (if applicable)","Product Name","Product Description","Specifications","Serial #","Vendor Site URL","Video Content URL(s)","Downloadable Content URL(s)","Pictures Saved?","Migrated?","Alternative Site URL"]
["Pressure Sealers","Low Volume"]
[null,null,"AutoSeal FD 1000","Key Features\nHand-feed pressure sealer\nSeals single pressure seal forms\nCompact, easy to use\nNo adjustments required\nThe FD 1000 AutoSeal® Hand-Feed Pressure Sealer is a quick and easy solution for processing single pressure seal forms.\n\nThe FD 1000 is ideal for one-off forms, re-runs, quickly sealing misfed forms offline, or as a backup for a primary pressure sealer. It’s easy to use right out of the box, with no adjustments, set-up or guesswork. Simply fold the form and feed it by hand into the FD 1000. In seconds, you’ll have a secure, mail-ready piece, without the need for envelopes. The FD 1000 is designed to accommodate a variety of form sizes and fold types, up to 5 ½” in folded width, and can process up to 24 pre-folded forms per minute.\n\nProudly built in the USA with proven Formax technology, the FD 1000 is an economical solution with the quality and reliability you have come to expect from Formax.",null,null,"https://www.formax.com/solutions/low-volume/fd-1000","https://www.youtube.com/watch?v=707zconBqtg","https://www.formax.com/sites/default/files/files/products/FD%201000%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"AutoSeal FD 1202","Key Features\nSpeed: Up to 38 pieces/min\nClearly-marked fold plates\nProcesses up to 14\" forms\nCatch tray\nThe FD 1202 AutoSeal® provides a user-friendly solution for processing of one-piece pressure-sensitive mailers. Combined with a laser printer and pressure seal forms, the FD 1202 creates secure, mail-ready pieces in minutes, without the need for envelopes.\n\nThe clearly marked fold plates, simple ergonomic controls and drop-in feed system provide easy set-up and operation, right out of the box. These features, plus a compact desktop design, make the FD 1202 ideal for any office environment with low-volume applications. A processing speed of up to 38 forms per minute and the added capability of processing 14” forms enable operators to complete daily processing jobs with ease.\n\nBuilt in the USA with proven Formax technology, the FD 1202 is an economical solution with the quality and reliability you have come to expect from Formax.",null,null,"https://www.formax.com/solutions/pressure-seal/low-volume/fd-1202","https://www.youtube.com/watch?v=oDdf1xAL0oc","https://www.formax.com/sites/default/files/files/products/FD%201202%20Spec%20Sheet.pdf","Yes","Yes"]
[{"$nulls":7},"https://www.youtube.com/watch?v=lNC40FXe8v0"]
[null,null,"AutoSeal® FD 1402","Key Features\nSpeed: Up to 75 pieces/min\nEasy-adjust pre-marked fold plates\nThree-roller top-feed\nProcesses up to 14\" forms\nResettable counter\nThe FD 1402 AutoSeal offers a user-friendly low-volume solution for processing one-piece pressure sensitive mailers. With a speed of up to 75 forms per minute and the ability to process forms up to 14” in length, the FD 1402 enables operators to complete daily processing jobs with ease.\n\nStandard features include redesigned fold plates that are clearly marked and easier to adjust, a control panel with six-digit resettable counter, and drop-in top feed system, all in a compact and sleek desktop design. Fold plates are pre-marked for standard folds for 11” and 14” form sizes, and can be easily adjusted for custom folds.\n\nBuilt in the USA with proven Formax technology, the FD 1402 is an economical solution with the quality and reliability you have come to expect from Formax.",null,null,"https://www.formax.com/solutions/pressure-seal/low-volume/fd-1402","https://www.youtube.com/watch?v=lFVcHlcm-hA","https://www.formax.com/sites/default/files/files/products/FD%201402%20Spec%20Sheet_0.pdf","Yes","Yes"]
[{"$nulls":7},"https://www.youtube.com/watch?v=B0hW9nvD198"]
[null,"Mid Volume"]
[null,null,"AutoSeal® FD 1502","Key Features\nSpeed: Up to 100 pieces/min\nEasy-adjust pre-marked fold plates\nThree-roller top-feed\nProcesses up to 14\" forms\nResettable counter\nThe FD 1502 AutoSeal is an ideal mid-volume solution for processing one-piece pressure sensitive mailers. With a speed of up to 100 forms per minute, in sizes up to 14” in length, the FD 1502 enables operators to complete daily jobs with ease.  \n\nNewly redesigned fold plates are clearly marked and easier to adjust, making the FD 1502 a breeze to setup, right out of the box. With the capacity to process 14” forms, it has the versatility to fold and seal virtually any mid-volume application to meet your needs. Fold plates are marked for four standard folds - Z, C, Uneven Z and Half folds - and can be easily reset for custom folds including Eccentric Z and C-fold mailers.\n\nThe compact, sleek design and ease of operation make this unit ideal for processing documents in an office environment with mid-volume applications. Built in the USA with proven Formax technology, the FD 1502 provides an economical solution with the quality and reliability you have come to expect from Formax.",null,null,"https://www.formax.com/solutions/pressure-seal-solutions/fd-1502","https://www.youtube.com/watch?v=fyYqKNko5Yg","https://www.formax.com/sites/default/files/files/products/FD%201502%20Spec%20Sheet_0.pdf","Yes","Yes"]
[{"$nulls":7},"https://www.youtube.com/watch?v=B0hW9nvD198"]
[null,null,"AutoSeal® FD 1502Plus","Key Features\nSpeed: Up to 6,250 pieces/hour\nPre-marked fold plates\nThree-roller top-feed\nProcesses up to 14\" forms\nIntegrated output conveyor\nThe FD 1502Plus AutoSeal offers a user-friendly mid-volume solution for processing one-piece pressure-sensitive mailers. A processing speed of up to 6,250 forms per hour enables operators to complete daily jobs with ease. Plus, the integrated output conveyor keeps processed forms in a neat, sequential order, ready for the mail.\n\nNewly redesigned fold plates are clearly marked and easier to adjust, making the FD 1502Plus a breeze to set up, right out of the box. With the capacity to process 14” forms, it has the versatility to fold and seal virtually any mid-volume application to meet your needs. Fold plates are marked for four standard folds - Z, C, Uneven Z and Half folds - and can be easily reset for custom folds including Eccentric Z and C-fold mailers.\n\nThe compact desktop design and ease of set-up and operation make this unit ideal for small offices or individual departments. Built in the USA with proven Formax technology, the FD 1502Plus is an economical solution with the quality and reliability you have come to expect from Formax.",null,null,"https://www.formax.com/solutions/pressure-seal-solutions/fd-1502Plus","https://www.youtube.com/watch?v=YuuMGKq3U_s","https://www.formax.com/sites/default/files/files/products/FD%201502Plus%20Spec%20Sheet_0.pdf","Yes","Yes"]
[null,null,"AutoSeal® FD 2002","Key Features\nSpeed: Up to 8,000/hour\nSliding fold plate design\nProcesses up to 14\" forms\nTouch-pad control panel\nThe FD 2002 AutoSeal® is a powerful desktop model designed to process pressure sensitive self-mailers. An easy to use touch-pad control panel and three roller drop-in feed system make this product both practical and dependable. Its redesigned sliding fold plates make setup and operation even easier, with fine tuning knobs for precision folds.\n\nStandard features include a six-digit counter, jog control, fault detection, and LED indicators. Up to 250 forms can be loaded in the hopper and processed at speeds up to 8,000 per hour.\n\nThe FD 2002 is also available as a package, the P2002, which includes a fully enclosed cabinet for storage and an 18\" conveyor with photo eye for neat and sequential stacking of processed forms. The cabinet and conveyor are options for the FD 2002.",null,null,"https://www.formax.com/solutions/pressure-seal-solutions/fd-2002","https://www.youtube.com/watch?v=oHerxqlmdXg","https://www.formax.com/sites/default/files/files/products/FD%202002%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"AutoSeal® FD 2002IL System","Key Features\nPrint, fold, seal in-line\nEnclosed paper path\nEnhanced security\nProcesses up to 14\" forms\nThe AutoSeal FD 2002IL System interfaces the industry-leading FD 2002 AutoSeal with model-specific MICR and non-MICR desktop laser printers (not included) to provide enhanced document security.\n\nThe System's enclosed paper path is specially designed to conceal sensitive documents including PIN notices, checks, school grade reports and health care information. This feature also eliminates the added task of unloading forms from the printer and loading them into the pressure sealer.\n\nThe IL System - which includes the IL Pressure Sealer and IL Alignment Base - features a user-friendly LED control panel and clearly marked fold settings for standard 11\" and 14\" documents. The compact, powerful design is capable of processing up to 50,000 forms per month.",null,null,"https://www.formax.com/solutions/pressure-seal-solutions/fd-2002il-system","https://www.youtube.com/watch?v=dTdsXGU9xX8","https://www.formax.com/sites/default/files/files/products/FD2002IL_0.pdf","Yes","Yes"]
[null,"High Volume"]
[null,null,"AutoSeal® FD 2032","Key Features\nSpeed: Up to 11,000/hour\nSliding fold plate design\nProcesses up to 14\" forms\nUneven \"Z\" and \"C\" folds\nThe FD 2032 AutoSeal® desktop pressure sealer provides a reliable and compact solution for processing pressure sensitive self-mailers. Up to 350 forms can be loaded in the feeder and processed at speeds up to 11,000 forms per hour.\n\nStandard features include a six-digit counter, jog control, fault detection, LED indicators and an operator friendly touch-pad control panel. Its redesigned sliding fold plates make setup and operation even easier, with fine tuning knobs for precision folds.\n\nAll of these features make the FD 2032 the perfect solution for streamlining your post processing. The FD 2032 also has an optional fully enclosed cabinet for storage, and a choice of two conveyors with photo-eye for neat and sequential stacking of processed forms.",null,null,"https://www.formax.com/solutions/pressure-seal-solutions/fd-2032","https://www.youtube.com/watch?v=9svpVdC4QXI","https://www.formax.com/sites/default/files/files/products/FD2032.pdf","Yes","Yes"]
[null,null,"AutoSeal® FD 2054","Key Features\nAutomatic fold settings\n17\" form capability\nIntegrated conveyor\n35 custom fold settings\nSpeed: up to 16,450/hour\nThe AutoSeal® FD 2054 is a fully automatic pressure sealer which provides the ultimate tabletop solution for processing pressure sensitive one-piece mailers. Designed with ease of operation and efficiency in mind, the FD 2054 automatically detects and adjusts for 11”, 14” and 17” forms. It features 5 pre-programmed standard folds for even panel C, V, Z and uneven/eccentric C and Z folds. It also has the ability to store up to 35 custom fold settings with the simple touch of a button.\n\nThe FD 2054 utilizes a drop-in three-roller feed system which produces dependable feeding of forms with no paper fanning required. Forms are processed at speeds up to 16,450 per hour, and are output to an integrated telescoping conveyor with automated nip roller positions, capable of holding up to 500 processed forms. The large 2.8” (71mm) backlit LCD display and user friendly control panel allow for untrained operators to walk up and start processing pressure seal forms with little to no instruction. Fully-automated stacker wheels eliminate the need to move them manually when switching form sizes and fold types.\n\nThe FD 2054 advanced software allows for all standard fold types and paper sizes to be customized to meet your particular needs.\n\nOptions include a fully enclosed cabinet for storage, 402 Series Joggers, and the V-Stack36 Stacker, which vertically stacks up to 22\" of processed forms, making them easier to unload for further processing.\n\nThese features combine to make the FD 2054 an ideal solution for streamlining your post processing.",null,null,"https://www.formax.com/solutions/pressure-seal-solutions/fd-2054","https://www.youtube.com/watch?v=kTJgIjwc6rM","https://www.formax.com/sites/default/files/files/products/FD2054.pdf","Yes","Yes"]
[null,"Production Volume"]
[null,null,"AutoSeal® FD 2096","Key Features\nBottom-suction air-feed\nSpeed: Up to 30,000/hr\nRugged fold plates\nSound-dampening covers\n24\" output conveyor\nThe AutoSeal® FD 2096 uses patented pressure seal technology to efficiently process cut-sheet pressure seal forms in a mid-volume production environment, at speeds of up to 30,000 forms per hour. Its bottom-suction air-feed system provides accurate feeding and allows for continual loading of forms, dramatically reducing down time.\n\nSet-up is quick and easy with rugged metal fold pates, clearly marked with both standard and metric markings, and fold rollers made of heavy-duty polyurethane foam, which eliminates the need for gap adjustments. The sealing unit utilizes a 17” ball transport deck for a smooth, reliable transition from the fold rollers into the sealer, and requires no adjustments.\n\nUser-friendly features include sound-dampening fold plate covers for quieter operation, a 6-digit resettable LED counter, rugged locking casters, and a high-capacity 24” output conveyor which is collapsible for convenient storage when not in use.\n\nHeavy duty construction combines with quick set-up and operation to make the FD 2096 a powerful solution for processing mid-volume pressure-seal mailings.",null,null,"https://www.formax.com/solutions/production/fd-2096","https://www.youtube.com/watch?time_continue=1&v=Uo5FKOcxg5U","https://www.formax.com/sites/default/files/files/products/FD%202096%20Spec%20Sheet_0.pdf","Yes","Yes"]
[null,null,"AutoSeal® FD 2200 Series","Key Features\nFour in-feed options\nSpeed: Up to 40,000/hr\nUnlimited duty cycle\nAutomatic fold settings\nHeavy-duty rollers\nThe AutoSeal 2200 Series High Volume Pressure Sealers are designed to handle the highest volume jobs with ease and dependability. The 2200 Series offers fully automated settings to provide for quick and easy setup of different jobs. Processing speeds of up to 40,000 forms per hour sets the industry standard for speed and production capabilities.\n\nFour models are available in the 2200 Series which offer different in-feed options, three models for cut-sheet forms, and one for continuous forms. The FD 2200 utilizes an air-feed system with a capacity of up to 500 forms; the FD 2200-EX offers an extended air-feed system to reach a capacity of up to 1,000 forms; the FD 2250 utilizes a pile feed system to reach a total capacity of up to 3,500 loaded forms; and the FD 2280 works in-line with the Formax FD 676 Maxi Burster to process continuous forms.\n\nThe Formax V-Stack36 is an available option which stacks up to 22\" of processed forms, making them easier to unload for further processing.\n\nAll four models produce fast and accurate folds to deliver a secure and time-effective finished product ready for the mail. The 2200 Series clearly sets the new standard for high volume processing needs.",null,null,"https://www.formax.com/solutions/pressure-seal-solutions/fd-2200-series","https://www.youtube.com/watch?v=aSqgIxdSxrU","https://www.formax.com/sites/default/files/files/products/2200%20Series%20Spec.pdf","Yes","Yes"]
[null,null,"AutoSeal® FD 2200-10 Stand-Alone","Key Features\nSpeed: Up to 40,000/hr\nIntegrates easily\nHigh production\nThree interface connections\nThe AutoSeal FD 2200-10 Stand-Alone pressure sealer is the ideal solution for high-volume mailers who want to utilize existing floor model folding systems. The ability to purchase a \"sealer-only\" system versus a complete folding and sealing solution drastically reduces the up-front cost of adding pressure seal capability.\n\nThe 2200-10 utilizes a patented pressure seal system that has been carefully engineered and refined to process pressure seal forms at speeds of up to 40,000 pieces per hour, combined with heavy-duty construction built to last in the most demanding environments.\n\nStandard features include a precision ground clutching four-roller system, an 8-ball transport deck to provide a smooth transition from the fold rollers to the sealer, plus infrared fault detectors, safety interlock, and heavy-duty casters.",null,null,"https://www.formax.com/solutions/pressure-seal-solutions/fd-2200-10",null,"https://www.formax.com/sites/default/files/files/products/FD2200-10.pdf","Yes","Yes"]
[null,null,"AutoSeal® FD 2300 Series","Key Features\nFour in-feed options\nSpeed: Up to 43,000/hr\nColor touchscreen control\nProgram up to 200 jobs\nUnlimited duty cycle\nAutomatic fold settings\nHeavy-duty rollers\nThe AutoSeal® 2300 Series High-End Pressure Sealers are designed to handle the highest volume jobs with ease and dependability, with speeds of up to 43,000 forms per hour. User-friendly features include the graphics-based color touchscreen control panel, and the ability to program up to 200 custom jobs. Fully automated settings include the feeder, alignment rails, fold plate stops, deflectors and fold rollers, and delivery rollers.\n\nFour models are available in the 2300 Series which offer different in-feed options: the FD 2300 utilizes an air-feed system with a capacity of up to 500 forms; the FD 2300-EX offers an extended air-feed system to reach a capacity of up to 1,000 forms; the FD 2350 utilizes a pile-feed system to reach a total capacity of up to 3,500 loaded forms; and the FD 2380 works in-line with the Formax FD 676 Maxi Burster for processing continuous forms.\n\nThe Formax V-Stack36 Vertical Stacker is an available option which stacks up to 22” of processed forms, making them easier to unload for further handling.\n\nAll four models produce fast and accurate folds to deliver a secure and time-effective finished product ready for the mail. The 2300 Series clearly sets the new standard for high volume processing.",null,null,"https://www.formax.com/solutions/pressure-seal-solutions/fd-2300-series","N/A","https://www.formax.com/sites/default/files/files/products/2300%20Series%20Spec%20Sheet.pdf","Yes","Yes"]
["Mailing Solutions","Inserters"]
[null,null,"FD 6102","Key Features\nSpeed: Up to 1,360/hr\nPaper Size: Up to 8.5\" x 14\"\nUp to 15 programmable jobs\n#10 & 6\" x 9.5\" envelopes\nThe FD 6102 inserter offers the latest technology in entry-level tabletop inserters, making it possible for any business to automate its mailings. The affordability of this inserter eliminates the need to send out tens of thousands of mail pieces in order to justify the cost of automation. With the FD 6102, any size company can enjoy the benefits of automated folding and inserting.\n\nQuiet operation and a compact, desktop design fits any office environment. A large, color touchscreen control panel with wizard job feature easily guides operators through setup and operation. Up to 15 jobs can be programmed so that recurring and frequent jobs can be processed with the push of a button.\n\nDon’t waste any more valuable time and money manually folding and inserting. Automate your mailings with the FD 6102 and maximize your company’s efficiency.",null,null,"https://www.formax.com/solutions/inserters/fd-6102","https://www.youtube.com/watch?v=GK6atTbwtL0","https://www.formax.com/sites/default/files/files/products/FD6102.pdf","Yes","Yes"]
[null,null,"6204 Series","Key Features\nSpeed: Up to 2,200/hr\nColor touchscreen\nFeeders: Up to 325 sheets\n1, 1 1/2, 2 or 2 1/2 Feeders\nThe 6204 Series brings advanced folding & inserting technology and flexibility to the office environment. A large, color touchscreen control panel with wizard job feature easily guides operators through setup and operation. AutoSet™ allows for one-touch setup of new jobs by automatically measuring paper lengths, envelope sizes and fold lengths. Recurring and frequent jobs run in AutoSet™ can also be stored as one of 15 jobs accessed with the push of a button. The powerful folding system enables the 6204 Series to accurately fold up to five sheets of paper at the same time.\n\nFour configurations are available to meet your processing needs. The FD 6204-Basic 1 offers one automatic sheet feeder. The FD 6204-Basic 2 model is equipped with two automatic sheet feeders. The FD 6204-Advanced 1 model has one sheet feeder and one insert/BRE feeder. The FD 6204-Advanced 2 comes with two sheet feeders and one insert/BRE feeder.\n\nThe 6204 Series Inserters offer the power and reliability of larger machines with the ease of operation expected and required for the office environment.",null,null,"https://www.formax.com/solutions/inserters/6204-series","https://www.youtube.com/watch?v=vWQHD7d2Yno","https://www.formax.com/sites/default/files/files/products/6204.pdf","Yes","Yes"]
[null,null,"6306 Series","Key Features\nSpeed: Up to 3,800/hr\n7\" color touchscreen, advanced graphical interface\nPaper and envelope presence sensors\nHigh capacity vertical stacker\n50 programmable jobs\nThe 6306 Series Inserters combine user-friendly features with high productivity. Five models are available to meet the needs of any size office or mailroom. A variety of input configurations includes a high-capacity document feeder for up to 725 sheets, a high-capacity production feeder, standard and special feeders, and short feed trays.\n\nFeatures include a 7” full-color touchscreen control panel with graphical interface, high-capacity vertical stacker which holds up to 500 finished envelopes, automatic paper and envelope presence sensors with indicators on the control panel, and a large top-loading envelope hopper with a capacity of up to 400 envelopes. The 6306 Series includes an energy-saving feature which automatically puts the inserter into standby mode after 1 hour of being idle.\n\nVarious levels of 1D and 2D Barcode Recognition (BCR) and Optical Mark Recognition (OMR) are available and feature CIS scanning technology, which can scan codes printed in any location on a document. Optical Character Recognition (OCR) is also available, which uses page numbering in 1/1 or N-of-M format to ensure each set is complete before being inserted into an envelope.\n\nThe 6306 Series is powerful enough to fold up to 8 pages in tri-fold and up to 10 pages in half-fold modes. Its versatility allows for processing forms of various lengths and thickness all at the same time, up to 3,800 per hour and up to 40,000 pieces per month.\n\nOptions include a Production Feeder which holds up to1,200 sheets or 325 BREs, Advanced OMR and BCR, Formax MailDocTM Software, and a side exit tray for up to 400 filled envelopes.",null,null,"https://www.formax.com/solutions/inserters/6306-series","https://www.youtube.com/watch?v=I4HtKXu0u4s","https://www.formax.com/sites/default/files/files/products/6306%20Series%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"6404 Series","Key Features\nSpeed: Up to 4,000/hr\nFlip-down color touchscreen\nHigh-capacity outfeed stacker\nEnergy-saving standby mode\nThe versatile 6404 Series adapts to most any folding and inserting application. Models are available with 2 - 6 stations, offering the flexibility to meet your specific needs. A variety of input configurations include a high-capacity document feeder for up to 725 sheets, 1 or 2 high-capacity production feeders, standard and special feeders, and short feed trays. The 6404 Series is capable of folding and inserting top, middle and bottom-address documents into top-flap envelopes.\n\nStandard features include a full-color touchscreen control panel, a large output stacker which can hold up to 500 filled envelopes, and a large top-loading envelope hopper with a capacity of up to 325 envelopes. The 6404 Series also offers energy savings with its auto standby mode, which goes into effect after 1 hour of idle time.\n\nOptions include Barcode Recognition (BCR), Optical Mark Recognition (OMR), a variety of output choices, cabinets and 402 Series Joggers.",null,null,"https://www.formax.com/solutions/inserters/6404-series","https://www.youtube.com/watch?v=nJBr5roXeaI","https://www.formax.com/sites/default/files/files/products/6404.pdf","Yes","Yes"]
[null,null,"6606 Series","Key Features\nSpeed: Up to 4,300/hr\nPaper/Envelope Presence Sensors\nGraphics-based 10.4\" color touchscreen\nHigh-capacity output stacker\nInserts top/middle/bottom address documents\nUp to 50 programmable jobs\nThe versatile 6606 Series adapts to most any folding and inserting application. Models are available with 2-7 stations, offering the flexibility to meet your specific needs. A variety of input configurations includes a high-capacity document feeder for up to 725 sheets, 1 or 2 high-capacity production feeders, standard and special feeders, and short feed trays. The 6606 Series is capable of folding and inserting top, middle and bottom-address documents into top-flap envelopes.\n\nStandard features include a large reversible full-color touchscreen control panel with a graphical interface, automatic paper and envelope presence sensors with indicators on the control panel, a vertical output stacker which can hold up to 500 filled envelopes, in addition to a large top-loading envelope hopper with a capacity of up to 500 envelopes. The 6606 Series includes an energy-saving feature which automatically puts the inserter into standby mode after 1 hour of being idle. Users can also store up to 50 programmable jobs.\n\nVarious levels of Barcode Recognition (BCR) and Optical Mark Recognition (OMR) are available and feature CIS scanning technology, which can scan codes printed in any location on a document. Optical Character Recognition (OCR) is also available, which uses page numbering in 1/1 or N-of-M format to ensure each set is complete before being inserted into an envelope.\n\nAdditional options include a thin booklet feeder for up to 325 inserts, high-capacity output conveyor and envelope hopper for up to 1,000 envelopes each, side exit tray, cabinet and 402 Series Joggers.",null,null,"https://www.formax.com/solutions/inserters/6606-series","https://www.youtube.com/watch?v=NkyWDxAyKL8","https://www.formax.com/sites/default/files/files/products/6606-Series.pdf","Yes","Yes"]
[null,null,"7202 Series","Key Features\nInserts into flat envelopes\nSpeed: Up to 5,000/hr\n22\" Touchscreen interface\nModular 1 to 11 feeders\nUnlimited programmable jobs\nFormax 7202 Series Inserters combine user-friendly innovation with flexibility and productivity. A key feature is the 22” color touchscreen interface, which guides users through job set-up, and includes context-sensitive help on every screen. Unlimited programmable jobs lead to even greater productivity.\n\nThe 7202 Series has the power to process up to 5,000 envelopes per hour, including  flats up to 10” x 13”, folds up to 8 sheets at once, and produces up to 200,000 finished pieces per month. The modular design can be configured with up to 11 feed stations, with high-capacity feeders, and a standard capacity of up to 2,000 sheets. Versatile Feeders have been redesigned for easier loading on-the-fly, and offer the ability to insert a variety of media.\n\nA variety of code reading options are available, including single and double CIS scanners to read both sides of an insert, allowing for face-up or face-down feeding. Single and Multi-Code Reading Licenses are also available to read 1-Track and 2-Track OMR, 1D Barcode, and 2D Data Matrix.\n\nThe top-loading envelope hopper holds up to 800 #10 envelopes or 500 flats, in landscape orientation. Inserting into landscape flats offers higher processing speeds, fewer jams, and lower envelope costs. The 7202 Series inserts sets of up to 50 sheets into flats, and booklets up to 6mm thick. Standard features include a high-capacity 4-foot outfeed conveyor, which can be used in-line or at a 90° angle, an accumulator/divert deck which holds up to 300 sheets, and custom cabinets for sturdy, movable storage.\n\nAdditional options include High-Capacity Versatile Feeders (with or without intelligence), an envelope sorter/diverter and two styles of catch tray.\n\nWith a range of standard features, high capacity and intelligent design, the 7202 Series Inserters are set to take productivity to new levels.",null,null,"https://www.formax.com/solutions/inserters/7202-series",null,"https://www.formax.com/sites/default/files/files/products/7202%20Series%20Spec.pdf","Yes","Yes"]
[null,null,"7500 Series","Key Features\nInserts into flat envelopes\nSpeed: Up to 6,000/hr\nWidescreen touchscreen interface\nModular up to 11 feeders\nUnlimited programmable jobs\nTower Feeder with twin code readers\nFormax 7500 Series Inserters offer the flexibility and power to process a wide variety of inserting jobs. The modular design includes up to 11 feed stations, high-capacity feeders, and a widescreen touchscreen interface. A robust folding system folds up to 8 sheets at a time, with the power to process up to 6,000 envelopes per hour, and up to 300,000 finished pieces per month.\n\nThe top-loading envelope hopper holds up to 800 #10 envelopes or 500 flats, in landscape orientation. Inserting into landscape flats offers higher processing speeds, fewer jams, and lower envelope costs. The 7500 Series inserts sets of up to 72 pages, up to 10mm thick. Standard features include a high-capacity 4-foot outfeed conveyor, which can be used in-line or at a 90° angle, an accumulator/divert deck which holds up to 300 sheets, and custom cabinets for sturdy, movable storage.\n\nThe 7500 Series color touchscreen interface is the new standard for all PC-driven inserters. With graphics based on a photo-image of the inserter, it also provides the ability to edit documents while creating jobs. This new interface, combined with unlimited programmable jobs, makes creating and running inserting jobs easier than ever before.\n\nAll configurations include a Tower Feeder, which uses twin scanners to read codes either face-up or face-down. The 7500 Series has the ability to read 1 and 2-track OMR, 1D barcodes, and 2D Data Matrix, with codes located anywhere on the page. In addition, infrared and electromechanical double document detectors ensure the correct documents get into each envelope. Optional high-capacity feeders are available with or without intelligence, and can insert various media, including glossy booklets, DVDs and small inserts up to 6mm thick.\n \nWith a variety of standard features, high capacity and intelligent design, the 7500 Series Inserters are ready to take on any challenge.",null,null,"https://www.formax.com/solutions/inserters/7500-series",null,"https://www.formax.com/sites/default/files/files/products/7500%20Series%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"7104 Series","Key Features\nInserts into flat envelopes\nSpeed: Up to 5,500/hr\n22\" Touchscreen interface\nModular up to 17 feeders\nUnlimited programmable jobs\nThe Formax 7104 Series Inserters take flexibility and productivity to new heights. With 3 configurations, and an optional Productivity Package, this system can meet the challenge. The modular design offers up to 8 modules with up to 17 feed stations, with high-capacity feeders, and a standard capacity of up to 1,500 sheets. Each system is available with these standard feeder combinations: one 1,000-sheet feeder, one 500-sheet and one 1,000-sheet feeder, or three 500-sheet feeders. The top-loading envelope hopper holds up to 800 #10 envelopes.\n\nA 22” color touchscreen interface guides operators through job programming and functions, and with unlimited programmable jobs, it’s even easier to run recurring or frequently processed applications. The 7104 Series has optional Intelligent Feeders with the ability to read 1 and 2-track OMR, 1D Barcodes and 2D Data Matrix, with codes located anywhere on the document, front or back. Mechanical Double Document Detectors ensure the correct documents get into each envelope, allowing for the automatic insertion of multiple-page documents, which eliminates the tedious task of manually collating and inserting.\n\nThe 7104 Series processes up to 4,500 envelopes per hour (up to 5,500/hour with the optional Productivity Package), producing up to 180,000 finished pieces per month. The robust folding system folds up to 8 sheets at a time. Feeders can also be linked with a Cascade Mode to maximize output by connecting feeders filled with the same document. When one feeder empties, the next automatically starts feeding. Optional Insert Feeders are top loading making it easy to reload on-the-fly, and provide the ability to insert a variety of media, including glossy booklets.\n\nStandard features include a high-speed/capacity Accumulator and Divert Deck, ergonomically-designed Custom Cabinets on casters for convenient moveable storage, and a High-Capacity 4-foot Output Conveyor which can be used straight-on or at a 90 degree angle to the system.",null,null,"https://www.formax.com/solutions/inserters/7104-series",null,"https://www.formax.com/sites/default/files/files/products/7104%20Series_0.pdf","Yes","Yes"]
[null,"Folders"]
[null,null,"FD 300","Key Features\nClearly-marked fold settings\nPush-button operation\nSpeed: up to 7,400/hr\nFolds 11\" and 14\" paper\nHopper capacity: 200 sheets\nLCD control panel\nAutoBatch\nThe FD 300 Office Desktop Folder provides an economical solution for low-volume folding projects.\nThis compact folder processes 11\" and 14\" paper at speeds up to 7,400 sheets per hour, and is pre-marked for four popular folds: C, Z, Half and Double Parallel.\n\nUser-friendly features include an LCD control panel with 3-digit resettable counter, AutoBatch for processing sets of documents, and an output conveyor with easily-adjustable stacker wheels for neat sequential stacking of folded pieces.\n\nClearly marked fold settings and out-of-the-box operation make this folder ideal for churches, schools and small offices that demand quick and easy set-up with minimal adjustment.",null,null,"https://www.formax.com/solutions/folders/fd-300","https://www.youtube.com/watch?v=2TXxwmJ6uXQ","https://www.formax.com/sites/default/files/files/products/FD%20300%20Spec%20Sheet_1.pdf","Yes","Yes"]
[{"$nulls":7},"https://www.youtube.com/watch?v=eL3qDBaBIjo"]
[null,null,"FD 314","Key Features\nClearly-marked fold settings\nPush-button operation\nSpeed: up to 7,700/hr\nLCD control panel\nFolds 11\" and 14\" paper\nHopper capacity: 250 sheets\nAutoBatch\nThe FD 314 Office Desktop Folder provides an economical solution for low-volume folding projects. It combines a compact footprint with push-button controls, so it's simple to use, right out of the box! Fold plates are clearly marked for four common folds - letter, zig-zag, half and double parallel - and can be easily adjusted for custom folds. With a three-tire drop-in feed system, it processes 11” and 14” paper at speeds up to 7,700 sheets per hour, and offers a hopper capacity of up to 250 sheets.\n\nThe LCD control panel includes a resettable 3-digit counter, and AutoBatch for processing a set number of sheets with a pause between sets. The built-in output conveyor features adjustable stacker wheels for neat, sequential stacking of folded pieces.\n\nUser-friendly fold settings and straighforward operation make this folder ideal for churches, schools, and offices that demand quick and easy set-up with minimal adjustment.",null,null,"https://www.formax.com/solutions/folders/fd-314","https://www.youtube.com/watch?v=vlzjfDEduY0","https://www.formax.com/sites/default/files/files/products/FD%20314%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"FD 322","Key Features\nDrop-in top-feed system\nSpeed: up to 11,000/hour\nFolds up to 11\" x 17\"\nRemovable fold plates\nStandard and custom folds\nThe FD 322 Document Folder offers an unmatched level of performance and affordability. Designed with ease of operation in mind, it utilizes a drop-in feed system, eliminating the need to fan paper. Simply square the paper stack and load it into the feed tray. The FD 322 can handle 11”, 14” and 17” paper sizes, and is pre-marked for three standard folds: Letter, Zig-Zag, Half. The fold plates are easily adjusted for three custom folds: Gate, Fold Out, Double Parallel.\n\nRemovable top and bottom fold plates make this folder ideal for churches, schools, businesses or departments that demand quick and easy set-up and operation. Variable speed control allows for processing up to 11,000 sheets per hour. An extended outfeed conveyor allows operators to run most applications without having to unload the output before the infeed is empty.\n\nAs with all Formax folders, the FD 322 is constructed with a heavy-duty steel frame and molded, high-impact side covers for durability. The three-tire friction feed accurately pulls paper info the folder, while the skew adjustment allows for moving the feed table left or right, to produce crisp, accurate folds.\n\nThe compact size and user-friendly operation make the FD 322 an ideal solution for churches, schools, and offices that demand quick and easy setup and operation.",null,null,"https://www.formax.com/solutions/folders/fd-322","https://www.youtube.com/watch?v=kUu2lCfojFc","https://www.formax.com/sites/default/files/files/products/FD%20322%20Spec%20Sheet_0.pdf","Yes","Yes"]
[null,null,"FD 342","Key Features\nUser-friendly controls\nTelescoping output stacker\nSpeed: up to 15,500/hour\nFolds up to 12\" x 18\"\nAdjustable stacker wheels\nThe FD 342 Document Folder is a fast, dependable and easy-to-use solution for virtually all folding applications.  Six popular folds are clearly marked on the fold plates for quick set-up and operation, simply slide the fold stop to the desired fold and go.  Additional fold adjustments can be made with the fine tuning knobs at the end of each fold plate for precision folding.\n\nNo need to stand and watch over this folder: operators can load up to 500 sheets in the hopper, select their fold, press start and walk away to attend to other important tasks.  The FD 342 will fold the 500 sheets in no time at all and hold the folded pieces on its patented Telescoping Conveyor System until they are retrieved.\n\nThe patented Multi-Sheet Feeder is an optional feature that allows up to 4 sheets stapled or unstapled to be folded at one time through the dedicated feed system with its own side guides and skew adjustment system.\n\nThe FD 342 is capable of processing paper up to 18” (457mm) in length and up to 12.25” (311mm) in width giving it the flexibility to handle a variety of paper sizes.  With its customizable jobs, operators can fold in virtually any configuration that requires only two folds. Cross folding adds to the FD 342’s flexibility allowing for additional folds in a second pass.\n\nThe simplicity and value of the FD 342 make it an ideal solution for any church, school or small business that is cost conscious but requires the easy operation, versatility and dependability of a more expensive folder.",null,null,"https://www.formax.com/solutions/folders/fd-342","https://www.youtube.com/watch?v=kc6PHYYBUek","https://www.formax.com/sites/default/files/files/products/FD342.pdf","Yes","Yes"]
[null,null,"FD 346 Touchscreen Desktop Office Folder","Key Features\nColor touchscreen, graphics-based\nTelescoping output stacker\nSpeed: up to 15,500/hour\nFolds up to 12\" x 18\"\nAdjustable stacker wheels\nThe FD 346 Document Folder is a fast, dependable and easy-to-use solution for virtually all folding applications.  Its color touchscreen control panel features internationally-recognized symbols in place of text, making it easy for anyone to use. Six popular folds are clearly marked on the fold plates for quick set-up and operation, simply slide the fold stop to the desired fold and go.  Additional adjustments can be made with the fine tuning knobs at the end of each fold plate for precision folding.\n\nNo need to stand and watch over this folder: operators can load up to 500 sheets in the hopper, select their fold, press start and walk away to attend to other important tasks.  The FD 346 will fold the 500 sheets in no time at all and hold the folded pieces on its patented telescoping conveyor system until they are retrieved.\n\nThe optional Multi-Sheet Feeder allows up to 4 stapled or unstapled sheets to be folded at one time through a dedicated feed system with its own side guides and skew adjustment system.\n\nThe FD 346 is capable of processing paper up to 18” in length and up to 12” in width giving it the flexibility to handle a variety of paper sizes.  With its customizable jobs, operators can fold in virtually any configuration that requires only two folds. Cross folding adds to the FD 346’s flexibility allowing for additional folds in a second pass.\n\nThe innovative touchscreen, simple set-up and operation make the FD 346 an ideal solution for any church, school or small business that is cost conscious but requires the easy operation, versatility and dependability of a more expensive folder.",null,null,"https://www.formax.com/solutions/folders/fd-346","https://www.youtube.com/watch?v=u6L2dvp4E4w","https://www.formax.com/sites/default/files/files/products/FD%20346%20Spec%20Sheet.pdf"]
[null,null,"FD 382","Key Features\nAutomatic settings\n2.8\" LCD display\nTelescoping output stacker\nSpeed: up to 20,100/hour\nAdjustable stacker wheels\nThe Automatic FD 382 Document Folder offers any business, church, school or print for pay center quick, easy set-up, and the versatility to complete a variety of fold jobs in minutes. Jobs are completed exceptionally fast with the FD 382, folding up to 20,100 pieces per hour! Fully automated fold plates provide one touch setup of the 18 pre-programmed fold settings or for choosing one of the 25 custom folds that can be stored into memory. In addition, the new 2.8” (71mm) backlit LCD display and control panel makes the FD 382 extremely easy to use with a step by step user interface that is second to none.\n\nOperators can load up to 500 sheets in the hopper, select their fold, press start and walk away to attend to other important tasks. The FD 382 will fold the 500 sheets in as fast as 2 minutes and hold the folded pieces on its patented Telescoping Conveyor System.\n\nThe patented Multi-Sheet Feeder is an optional feature that allows up to 4 sheets stapled or unstapled to be folded at one time through the dedicated feed system with its own side guides and skew adjustment system.\n\nThe large 2.8” (71mm) backlit LCD display and user friendly control panel allows for untrained operators to walk up and start folding with little to no instruction. The FD 382 advanced software allows for all standard fold types and paper sizes to be customized to meet your particular needs.\n\nWhen it comes to paper folding, no one does it faster or with higher quality than the Formax FD 382!",null,null,"https://www.formax.com/solutions/folders/fd-382","https://www.youtube.com/watch?v=qAYlDLj6684","https://www.formax.com/sites/default/files/files/products/FD382_0.pdf","Yes","Yes"]
[null,null,"FD 38X","Key Features\nFully automatic settings\n2.8\" LCD display\nSpeed: up to 20,100/hour\nMulti-sheet feeder\nAutoStack™ stacker wheels\nThe Fully Automatic FD 38X Document Folder is the ideal folding solution for any business, church, school or print-for-pay center that demands quick and easy set-up. Jobs are completed exceptionally fast with the FD 38X folding up to 20,100 pieces per hour! The new 2.8” (71mm) backlit LCD display and control panel makes the FD 38X extremely easy to use and provides a user interface that is second to none. Fully automated fold plates and AutoStack™ Stacker Wheels provide one touch set-up of the 18 pre-programmed fold settings or for choosing one of the 35 custom folds that can be stored into memory.\n\nThe patented Multi-Sheet Feeder allows up to 4 sheets stapled or unstapled to be folded at one time through the dedicated feed system with its own side guides and skew adjustment system.\n\nOperators can load up to 500 sheets in the hopper, select their fold, press start and walk away to attend to other important tasks. The FD 38X will fold the 500 sheets in as fast as 2 minutes and hold the folded pieces on its patented Telescoping Conveyor System.\n\nThe large 2.8” (71mm) backlit LCD display and user friendly control panel allows for untrained operators to walk up and start folding with little to no instruction. The FD 38X advanced software allows for all standard fold types and paper sizes to be customized to meet your particular needs.\n\nThe FD 38X can also be used with the optional Formax V-Stack36 Vertical Stacker, which stacks up to 22\" of folded documents, making them easier to unload for further processing.\n\nWhen it comes to paper folding, no one does it faster or with higher quality than the Formax FD 38X!",null,null,"https://www.formax.com/solutions/folders/fd-38x","https://www.youtube.com/watch?v=iWl316jPJJM","https://www.formax.com/sites/default/files/files/products/FD38X.pdf","Yes","Yes"]
[null,null,"Atlas Air-Feed Document Folder","Key Features\nVariable speed 27,000/hr\nSix pre-set folds in common paper sizes\nBelt-driven outfeed stacker\nDurable composite fold rollers\nCompact rugged design\nPerf/Score attachment included\nThe ATLAS Air-Feed Document Folder combines high-volume output with user-friendly features in a rugged, small footprint. With variable speed control, it can process up to 27,000 sheets per hour. Six standard folds are pre-set in letter, legal and ledger paper sizes, making it easy for operators to setup and run jobs. Fully-enclosed fold plates feature dials to select fold plate position and LED displays accurate to 0.1mm. The fold rollers are made of a durable composite material designed to easily grip high-gloss paper, and are housed in a single patented pull-out cassette.\n\nThe powerful air suction feed table handles a wide variety of coated or non-coated stock, up to 25.5” in length, and aligns the sheets prior to folding. It also features a suction chamber to control curled or statically charged paper.\n\nStandard features include a modular perforator/scorer which can also be used as a roller bypass, allowing cover stock to be folded and output flat. The belt-driven outfeed stacker is located on the same side as the infeed, allowing operators to easily operate the Atlas from a single position. Double document and jam detection, batch counting, anti-static brushes, skew and micro adjustments complete the user-friendly package.\n\nThe Atlas Air-Feed Folder is ideal for those with big folding jobs and limited space.",null,null,"https://www.formax.com/solutions/folders/Atlas","https://www.youtube.com/watch?v=eZUeTjnar5E","https://www.formax.com/sites/default/files/files/products/Atlas%20Spec%20Sheet_0.pdf","Yes","Yes"]
[null,null,"Atlas-AS Air-Feed Document Folder","Key Features\nVariable speed 27,500/hr\nUnlimited job memory\nFull-color touchscreen control panel\nBelt-driven outfeed stacker\nDurable composite fold rollers\nCompact rugged design\nPerf/Score attachment included\nThe ATLAS-AS Air-Feed Document Folder combines high-volume output with user-friendly features in a rugged, small footprint. With variable speed control, it can process up to 27,500 sheets per hour. Its 7” full-color touchscreen control panel allows operators to set up jobs easily and to program an unlimited number of jobs into memory. Fully-enclosed fold plates feature dials to select fold plate position and LED displays accurate to 0.1mm. The fold rollers are made of a durable composite material designed to easily grip high-gloss paper, and are housed in a single patented pull-out cassette.\n\nThe powerful air suction feed table handles a wide variety of coated or non-coated stock, up to 26.5” in length, and aligns the sheets prior to folding. It also features a suction chamber to control curled or statically charged paper.\n\nStandard features include a modular perforator/scorer which can also be used as a roller bypass, allowing cover stock to be folded and output flat. The belt-driven outfeed stacker is located on the same side as the infeed, allowing operators to easily operate the Atlas from a single position. Double document and jam detection, batch counting, anti-static brushes, skew and micro adjustments complete the user-friendly package.\n\nThe Atlas-AS Air-Feed Folder is ideal for those with big folding jobs and limited space.",null,null,"https://www.formax.com/solutions/folders/Atlas-AS","https://www.youtube.com/watch?v=eZUeTjnar5E","https://www.formax.com/sites/default/files/files/products/Atlas-AS%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"FD 3200 Air Suction Folder","Key Features\nAir suction technology\nFolds up to 15,600/hour\nFully automated\nCompact and quiet\nDouble feed detection\nThe FD 3200 Air-Suction Document Folder offers high performance folding in a compact tabletop unit, ideal for digitally printed documents on heavy and coated stock. The air-suction feed technology reduces static electricity and minimizes feed marks common in traditional friction feed systems. The FD 3200 utilizes internal fans to produce air and suction for quiet operation in a smaller footprint.\n\nWith a speed of up to 15,600 sheets per hour, and a feed tray capacity of up to 625 sheets, the FD 3200 quickly powers through a range of applications, all at the touch of a button, while Optical Double Feed Detection ensures document integrity. To accommodate a variety of paper weights and sizes, fan speed and air flow can be adjusted independently using the interactive control panel and external adjustment knobs.\n\nUser-friendly features include automatic paper size detection and fold plate settings, control panel with LCD display, six programmed fold settings, and the ability to store up to 20 custom folds. The FD 3200 includes a cross folding guide, a four-digit counter with batch counting capability, four fold rollers for accuracy, and a variety of document security features. An optional Side Air Kit is available to enhance feeding of heavier stock and larger sheets of paper.\n\nFully automated and insulated for quiet operation, the FD 3200 is ideal for the office environment.",null,null,"https://www.formax.com/solutions/folders/fd-3200-air-suction-folder","https://www.youtube.com/watch?time_continue=103&v=60en_uUn324","https://www.formax.com/sites/default/files/files/products/FD%203200%20Spec%20Sheet.pdf","Yes","Yes"]
[null,"Mailing Software"]
[null,null,"MailDoc™ Software Suite","Key Features\nGenerate OMR, 1D & 2D BCR marks\nSave on printing & postage\nEasy set-up and operation\nSimplex to duplex printing\nFormax MailDoc™ is a powerful, easy-to-use software suite that generates Optical Mark Recognition (OMR), 1D and 2D Barcode Recognition (BCR) marks directly on documents for intelligent inserting of varying multi-page documents such as invoices and statements.\n\nMailDoc reduces printing and postage costs by sorting your unprinted documents and collating those that are intended for the same recipient so they are sent in the same envelope. Convert traditional simplex printed documents to duplex printing with MailDoc to reduce paper costs and provide additional postage savings.\n\nIn addition, MailDoc allows you to fully utilize a Formax Inserter equipped with OMR or BCR through enhanced security of sequence check marks, target marketing with selective feeding and diverting of sets based on selected criteria. Adding electronic overlays with company logos, messages or borders can enhance your printed document image while eliminating the need to inventory pre-printed forms.\n\nThe optional Postal Module further increases savings by running addresses through CASS, PAVE list management software with the use of NCOA for list certification.",null,null,"https://www.formax.com/solutions/mailing-solutions/maildoc-software-suite","N/A","https://www.formax.com/sites/default/files/files/products/MailDoc%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"Bulk Mailer Desktop Mailing Software","Key Features\nPAVE, CASS certified\nStandardizes addresses\nReal-Time NCOALink®\nIM Barcode compliant\nAddress printer support\nCopy/paste from Excel\nMake your mailing operation much more productive with Bulk Mailer — prepare USPS® compliant mailings faster and more easily. Achieve increased mail deliverability and the lowest postage rates all while avoiding the aggravation of deciphering complex postal regulations. Bulk Mailer includes a sophisticated new interface and the option to upgrade to a Microsoft® SQL Server database for faster performance with the largest address data files.\n\nNow any size mailing operation can reap the benefits of increased address quality and maximum postage discounts. The three editions of Bulk Mailer, Standard, Business, and Professional, deliver the right set of features needed by your organization. Bulk Mailer Business offers the most flexibility and advanced features, while those with small lists may be satisfied with the Standard edition.\n\nFeatures:\n\nPAVE™ Certified - Includes advanced support for First-Class Mail®, Periodicals, Standard Mail®, and all reports and postage statements\nCASS Certified™ - Address Correction cleans, standardizes, uses the DPV® product to confirm deliverability then adds ZIP + 4® codes and generates USPS® Form 3553\nReal-Time NCOALink® service - Via the Internet, update addresses of those who have moved BEFORE you mail\nIntelligent Mail® Barcode Compliant - Bulk Mailer meets the requirements for the next generation of USPS® barcode technology which is used to sort and track letters and flats.\nExtraordinary Data Exchange - Easy and powerful import capabilities - plus you can even copy and paste to/from Microsoft® Excel®\nDuplication Search - A variety of de-duplication options ensure the best results\nJob Builder - This time-saver comes with the Professional Edition\nAddress Printer Support - Model specific features are built-in, giving you the most from your high-speed address printer\nOptional Add-Ons - Choose among Package Services sorts, Mixed-Weights sorts, Palletization, Geocode, International data sets and more",null,null,"https://www.formax.com/solutions/mailing-software/bulk-mailer-desktop-mailing-software","N/A","https://www.formax.com/sites/default/files/files/products/Bulk_Mailer_Brochure%20Complete-w.pdf","Yes","Yes"]
[null,"Tabbing Systems"]
[null,null,"FD 262 Single-Head Tabber","Key Features\nUp to 12,000 pieces/hr\nFeeder holds up to 200 tri-folds\nUses a variety of tab stocks\nIntegrated bottom feed\n5-digit LCD counter\nTab density adjustment\nThe Formax FD 262 Single-Head Tabber makes quick work of applying tabs to folded mailpieces, and is designed to meet all USPS requirements for mailing and automation discounts. Using “crash tab” technology, the open edge of a mailpiece contacts an adhesive tab and travels through a set of rollers where the tab is tightly folded and sealed, creating a mail-ready piece.\n\nThe FD 262 tabs up to 12,000 pieces per hour (8 1/2” tri-folds), and handles media up to 17” wide, up to 5/32” thick. Its advanced design includes an integrated bottom feeder allowing for continuous operation, and a built-in waste take-up spool to reduce down time. The user-friendly controls include a 5-digit resettable LCD counter and a tab sensitivity control to adjust for tab stock density.\n\nVarious tab stocks can be used, including translucent, paper, and clear in sizes up to 1 1/2” in diameter. To meet USPS requirements, the mailpiece can be fed through in different directions, to apply tabs in various locations. The optional FD 282-30 3-foot Drop-Stacking Conveyor offers adjustable speed from 0 - 124 fpm, and stacks tabbed pieces in a neat, sequential order for easy removal.\n \nWith ever-changing postal regulations, having the dependable, efficient FD 262 Tabbing System can make your mailings compliant with very little effort.",null,null,"https://www.formax.com/solutions/tabbers/fd-262","https://www.youtube.com/watch?v=DnG8PE24AFM","https://www.formax.com/sites/default/files/files/products/FD%20262%20Spec%20Sheet_0.pdf","Yes","Yes"]
[null,null,"FD 282 Double-Head Edge Tabber","Key Features\nTabs up to 25,000 pieces/hr\nIn-line design\nUses a variety of tab stocks\nDigital counter with LCD display\nApplies tabs on opposite sites, simultaneously\nThe FD 282 Double-Head Edge Tabbing System features revolutionary advances in tabber design. It can apply tabs on opposite sides of the mailpiece at the same time, or on top and side simultaneously, maximizing productivity and eliminating the need to feed pieces multiple times. The key is the FD 282’s combination of tabbing heads: the fixed head applies tabs along an open edge, while the repositionable head can switch from side tabbing to front (leading-edge) tabbing. The flexible head can also affix flat tabs, small labels or up to 3 USPS roll stamps in one pass.\n\nIts central control panel features a digital LCD display, including lifetime and job resettable counters, which makes setup and operation user friendly. In addition, operators can program up to 4 jobs into memory for recurring jobs with different media sizes, tab specifications and tabbing positions. The FD 282 processes up to 25,000 pieces per hour (single tab), 15,000/hour (double tab) or 10,000/hour (triple tab), in sizes up to 11” x  15”, up to 1/4” thick.\n\nFor flexibility, the FD 282 is available as a stand-alone, compatible with a variety of feeders and output devices. It’s also available as the FD 282SF with a Medium-Duty Synchronized Feeder, or the FD 282HF with a Heavy-Duty Friction Feeder. Options include an output conveyor, and tabletop and floor stands.\n\nThe FD 282 provides a dependable and flexible solution to keep your mailings in compliance with changing USPS tabbing regulations.",null,null,"https://www.formax.com/solutions/tabbers/fd-282","https://www.youtube.com/watch?v=-aEmXORjR9c","https://www.formax.com/sites/default/files/files/products/FD%20282%20Spec%20Sheet_0.pdf","Yes","Yes"]
[null,"Envelope Opener"]
[null,null,"FD 452 Envelope Opener","Key Features\nSpeed: Up to 300 pieces/min\nOpens #10s to flats\nNo pre-sorting necessary\nNo scraps or sharp edges\nResettable LCD counter\nWhy waste time opening mail by hand? Maximize productivity with the Formax FD 452 Envelope Opener.\n\nThe FD 452 is quick to set up and simple to use. Load mail, press start and that's it! The innovative cutting mechanism slits one side of the envelope so the contents are left undamaged, with no messy paper scraps to clean up. Users can then safely extract envelope contents without the risk of sharp edges.\n\nUsing the FD 452, you can open a variety of envelope sizes at once, from #10 to flats, without pre-sorting. A unique Push Arm provides constant pressure to feed envelopes quickly and accurately. With a speed of up to 300 envelopes per minute and a catch tray capacity of up to 80 #10 envelopes, your mail will be ready in no time. The resettable LCD counter easily tracks processed mail pieces.",null,null,"https://www.formax.com/solutions/mailing-solutions/fd-452",null,"https://www.formax.com/sites/default/files/files/products/FD452.pdf","Yes","Yes"]
[null,"Envelope Sealer"]
[null,null,"FD 430 Envelope Sealer","Key Features\nClose & seal in one pass\nUp to 18,000 envelopes per hour\nPrecision moistening roller\nSeals standard or nested envelopes\nLarge outfeed tray\nThe Formax FD 430 Envelope Sealer closes and seals envelopes in a single pass. Simply place a stack of envelopes in the infeed tray, choose a processing speed with the adjustable control knob and in seconds, envelopes are sealed and ready for the mail.\n\nUsers can seal envelopes up to 9.75” wide, up to 16 mm thick, at speeds up to 18,000 envelopes per hour. Standard features include an adjustable envelope separator to ensure accurate feeding, a large outfeed tray, heavy-duty metal construction and a precision moistening roller. The flap closing bar allows users to load envelopes in a standard stack or nested with flaps open for even greater efficiency.\n\nForget the days of hand-sealing envelopes, and let the Formax FD 430 seal your mail in the blink of an eye.",null,null,"https://www.formax.com/solutions/mailing-solutions/fd-430-envelope-sealer","https://www.youtube.com/watch?v=UIldOfBViyc","https://www.formax.com/sites/default/files/files/products/FD%20430%20Spec%20Sheet_0.pdf","Yes","Yes"]
[null,"Cut-Sheet Cutter"]
[null,null,"FD 574 Cut-Sheet Cutter","Key Features\nUser-friendly control panel\n6 pre-programmed sizes\n100 memory options\nTop-loading feed system\nThe FD 574 Cut-Sheet Cutter is uniquely designed to process forms generated from a digital printer, up to 44 forms per minute. It automatically feeds the forms and cuts, slits*, or perforates* in the desired position, using transport rollers for accuracy and controls for fine-tuning.\n\nWith a speed of up to 2,640 sheets per hour, and cutting accuracy of +/- 0.5, it delivers precise and razor sharp edges on every finished piece, from checks and coupons, to tickets, membership cards and more. Pre-programmed for six popular paper sizes, it also has up to 100 programmable jobs. Options include a slitter, perforator, and belt conveyor stacker.\n\n* Optional",null,null,"https://www.formax.com/solutions/mailing-solutions/fd-574",null,"https://www.formax.com/sites/default/files/files/products/FD574.pdf","Yes","Yes"]
[null,"Cut-Sheet Bursters"]
[null,null,"FD 4170 Cut-Sheet Burster","Key Features\nVariable speed\nUp to 400 sheets 20#\n4-digit LCD counter\nProgrammable job settings\nThe FD 4170 Cut-Sheet Burster is the ideal finishing solution when multiple forms are printed on one page. Direct from a laser printer to the FD 4170, pre-perforated forms are automatically burst at perforation and stacked sequentially at speeds of up to 140 sheets per minute. No more cut sheet bursting by hand! Features include 5-level speed control, LCD counter, pro-programmed settings for 11\", 14\" and 17\" paper, adjustable side guides, and last job memory.",null,null,"https://www.formax.com/solutions/cut-sheet-bursters/fd-4170",null,"https://www.formax.com/sites/default/files/files/products/FD4170.pdf","Yes","Yes"]
[null,null,"FD 4400 Cut-Sheet Burster","Key Features\nSpeed: up to 30,000/hour\nUp to 500 sheets 20#\nAir-feed system\nContinuous loading\nThe FD 4400 High Volume Cut-Sheet Burster is specifically designed to process Check21 IRDs and other documents printed on perforated cut-sheet forms. The FD 4400 sets the benchmark as the only burster capable of processing up to 30,000 forms per hour and up to one million forms (input) per month. The bottom-feed air system allows operators to continually load forms to maximize efficiency and throughput.",null,null,"https://www.formax.com/solutions/cut-sheet-bursters/fd-4400",null,"https://www.formax.com/sites/default/files/files/products/FD4400.pdf","Yes","Yes"]
[null,"Joggers"]
[null,null,"FD 402P1 Single-Bin Paper Jogger","Key Features\nAligns & reduces static\nVariable speed\nPaper up to 11\" x 17\"\nUp to 800 sheets 20#\nThe FD 402P1 Single-Bin Paper Jogger provides quick and easy alignment for a wide variety of paper sizes up to 11\" x 17\". Jogging forms helps to separate them and reduce static electricity for accurate feeding through pressure sealers, folders, inserters and other paper handling equipment.\n\nIts solid state switch controls on/off and vibration speeds, up to 4,000 per minute. Electromagnetic design allows for continuous operation, while the slotted clean-outs allow paper dust, staples, paper clips and other debris to exit the jogging bin. The FD402P1 also features a tilted rack and a center divider to properly jog small paper stacks.",null,null,"https://www.formax.com/solutions/joggers/fd-402p1-single-bin-paper-jogger",null,"https://www.formax.com/sites/default/files/files/products/402%20Series%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"FD 402P3 Three-Bin Paper Jogger","Key Features\nAligns & reduces static\nThree bins for higher volume\nVariable speed\nUp to 1,700 sheets 20#\nThe FD 402P3 Three-Bin Paper Jogger is ideal for higher volume environments and provides quick and easy alignment for a variety of paper sizes up to 8.5\" x 14\". Jogging forms helps to separate them and reduce static electricity for accurate feeding through pressure sealers, folders, inserters and other paper handling equipment.\n\nIts solid state switch controls on/off and vibration speeds, up to 4,000 per minute. Electromagnetic design allows for continuous operation, while the slotted clean-outs allow paper dust, staples, paper clips and other debris to exit the jogging bin.",null,null,"https://www.formax.com/solutions/joggers/fd-402p3-three-bin-paper-jogger",null,"https://www.formax.com/sites/default/files/files/products/FD402_0.pdf","Yes","Yes"]
[null,null,"FD 402E2 Two-Bin Envelope Jogger","Key Features\nAligns & reduces static\nVariable speed\nUp to 1,750 sheets 20#\nThe FD 402E2 Two-Bin Envelope Jogger quickly settles the contents of incoming mail prior to opening with an automated envelope opener. It's also ideal for aligning checks and statement stubs for further processing in a banking environment.\n\nIts solid state switch controls on/off and vibration speeds, up to 4,000 per minute. Electromagnetic design allows for continuous operation, while the slotted clean-outs allow paper dust, staples, paper clips and other debris to exit the jogging bin.",null,null,"https://www.formax.com/solutions/joggers/fd-402e2-two-bin-envelope-jogger",null,"https://www.formax.com/sites/default/files/files/products/FD402_1.pdf","Yes","Yes"]
[null,null,"FD 404A1 Air Jogger","Key Features\nAlign, dry & remove static\nVariable speed, air pressure\nTilting jog bin\nUp to 940 sheets 20#\nThe FD 404A1 High-Capacity Air Jogger features improved ergonomics and a contemporary color scheme, and is ideal for print shops and production houses. This upright air jogger aligns and dries printed sheets as a single process, while removing static electricity. Variable vibration speed and air pressure controls combine to reduce jogging time, allowing press sheets and digital printouts to be air-dried immediately.\n\nIts V-shaped jog bin allows for jogging a criss-cross stacked pile of papers, while the vertical to horizontal tilt feature helps keeps large paper stacks from bending. With a capacity of up to 940 sheets, standard or foot pedal operation, and all-metal construction, the FD 404A1 is an ideal piece of equipment for any print shop.",null,null,"https://www.formax.com/solutions/joggers/fd-404a1-air-jogger","https://www.youtube.com/watch?v=gNb2bdD1wek","https://www.formax.com/sites/default/files/files/products/Air%20Jogger%20Spec%20Sheet_0.pdf","Yes","Yes"]
[null,null,"FD 402TA1 Tabletop Air Jogger","Key Features\nAlign, dry & remove static\nCompact & powerful\nVariable speed, air pressure\nPaper size up to 12\" x 18\"\nUp to 940 sheets 20#\nThe FD 402TA1 Tabletop Air Jogger is an ideal solution for print shops and production houses with limited space. This compact, powerful model aligns and dries sheets in a single process while reducing static electricity. Variable vibration speed and air pressure controls combine to reduce jogging time, allowing press sheets and digital printouts to be air-dried immediately.\n\nIts V-shaped jog bin allows for jogging a criss-cross stacked pile of papers, while the vertical to horizontal tilt feature helps keeps large paper stacks from bending. It has three operating modes, and variable air pressure and speed control to process up to 940 sheets at a time in sizes up to 12” x 18”.",null,null,"https://www.formax.com/solutions/joggers/fd-402ta1-tabletop-air-jogger-0","https://www.youtube.com/watch?v=X5606yPByL0","https://www.formax.com/sites/default/files/files/products/Air%20Jogger%20Spec%20Sheet.pdf","Yes","Yes"]
[null,"Continuous Form Bursters"]
[null,null,"FD 550 Industrial Burster","Key Features\nBurst up to 200 fpm\nSafety interlocks\nOutput conveyor\nCabinet\nThis low-volume burster offers industrial quality at an economical price. The FD 550 processes bursting jobs at speeds of 0-200 feet per minute. Standard features include tractor feed, slitters, safety interlocks, a conveyor unit and a cabinet. A power drop-stacker can be added to enhance productivity.\n\nThis low-volume unit is capable of operating 5 hours a day, 5 days a week. Many of the standard features offered in the higher end models are available as options to meet any need or application.",null,null,"https://www.formax.com/solutions/low-vol-burster",null,"https://www.formax.com/sites/default/files/files/products/Ind%20Bursters_1.pdf","Yes","Yes"]
[null,null,"Medium Volume Industrial Burster","Key Features\nBurst 15-350 fpm\nTractor feed, slitters\n17\" form capability\nOutput conveyor\nThe FD 666 Medium-Volume Burster processes bursting jobs at speeds of 15-350 feet per minute, with 17\" form capability. Standard features include slitters, tractor feed, safety interlocks, cabinet and a conveyor unit. A power drop-stacker can be added to enhance productivity, in addition to a center slitter, cylinder for 2-up printing, extra-wide margin trimmers, and a 6-digit photo-cell counter.\n\nThe FD 666 is capable of operating 5 hours a day, 5 days a week, offering industrial quality at an economical price. Virtually all of the standard features offered in the higher end models are available as options to meet any need or application.\n\n",null,null,"https://www.formax.com/solutions/medium-vol-burster",null,"https://www.formax.com/sites/default/files/files/products/Ind%20Bursters_0.pdf","Yes","Yes"]
[null,null,"High Volume Industrial Bursters","Key Features\nBurst up to 500 fpm\nContinuous operation, 24/7\nSteel upper rollers\nOutput conveyor\nTwo high-volume industrial bursters are available to process large bursting jobs at speeds up to 500 feet per minute while slitting, separating and stacking the forms. Standard features include slitters, tractor feed, safety interlocks, stand and a conveyor unit. A power drop-stacker can be added to enhance productivity.\n\nThe FD 676 is the standard model, while the FD 680 adds an imprinter. Each high-volume unit is capable of continuous operation, 7 days a week.",null,null,"https://www.formax.com/solutions/high-vol-bursters",null,"https://www.formax.com/sites/default/files/files/products/Ind%20Bursters.pdf","Yes","Yes"]
[null,"Document Signer"]
[null,null,"FD 150 Document Signer","Key Features\nSpeed: up to 300/minute\nDual key locks\nFour programmable jobs\nTwo counters\nWith the FD 150 Document Signer, you can sign or endorse cut-sheet documents securely at speeds up to 300 sheets per minute. Dual key locks and two counters, one resettable and one non-resettable, come standard for security and accuracy.\n\nFour programmable job settings make it easy to complete frequently-run jobs. Features include dual key/lock controls, and both resettable and non-resettable counters for maximum audit capability. Optional tri-color and ultraviolet ink rolls add extra security.",null,null,"https://www.formax.com/solutions/mailing-solutions/fd-150",null,"https://www.formax.com/sites/default/files/files/products/FD150.pdf","Yes","Yes"]
[null,"Conveyors/Stackers"]
[null,null,"Bi-Directional Drop-Stacking Conveyors","Key Features\n4-ft and 6-ft models\nCompatible with a variety of folders and sealers\nControl panel is reversible for bi-directional transport\nInternal vacuum fans\nSpeed: up to 350 ft/min\nMade in USA\nFormax FD 4040 and FD 4060 Drop-Stacking Conveyors are commonly run in-line with various brands of inkjet addressing systems. Utilizing internal vacuum fans at the infeed, they offer high-speed transport up to 350 feet/minute. These dual high-suction fans are located under the perforated belt, and pull media down onto the conveyor.\n\nThe FD 4040 and FD 4060 each feature a patent-pending reversible control panel module which can be rotated 180 degrees for left-to-right or right-to-left transport, offering greater flexibility in workflow and equipment configuration. IEC receptacles are integrated into the control panel providing safe, convenient power for an optional infrared dryer.\n\nEach model has adjustable height legs up to 35\" from the floor, as well as adjustable drop stack height from 5\" - 11\", and each is proudly made in the USA.",null,null,"https://www.formax.com/solutions/finishing-solutions/Conveyors",null,"https://www.formax.com/sites/default/files/files/products/FD%204040%20-%20FD%204060%20Spec%20Sheet%207-15_0.pdf","Yes","Yes"]
[null,null,"V-Stack36 Vertical Stacker","Key Features\nStacks documents vertically\nCompatible with a variety of folders and sealers\nPhoto eye activation\nLED indicator\nOptional adjustable stand\nThe V-Stack36 vertical stacker is designed to work with a variety of Formax pressure sealers and tabletop folders. Unlike a traditional outfeed conveyor, it stacks forms vertically, providing a neat stack which is easier to unload for further processing.\n\nWith photo-eye activation, the V-Stack36 neatly stacks up to 22 inches of folded documents. The infeed features a six-ball-roller deck and two guide wheels to ensure forms enter the stacker smoothly, and an LED lamp which alerts operators when the stacker is near full capacity. Its vertical paper stop adjusts to accommodate document sizes and fold types up to 7” high by 12\" wide.\n\nAn interlock is available for FD 38X folders and FD 2054, FD 2096 and 2200 Series pressure sealers, which automatically stops the stacker and the source machine when the stacker is at full capacity.\n\nA height-adjustable stand with locking casters is available to align with a variety of inputs. The stand is optional for use with tabletop folders and pressure sealers, and required for use with production pressure sealers.",null,null,"https://www.formax.com/solutions/mailing-solutions/v-stack36","https://www.youtube.com/watch?v=pWu9_GxmdUg","https://www.formax.com/sites/default/files/files/products/V-Stack36_1.pdf","Yes","Yes"]
["Data Destruction","Deskside Shredders"]
[null,null,"FD 8204CC Deskside Shredder","Key Features\nAutoStart/AutoStop\nUp to 17 sheets at once\nCDs, credit cards, staples\nQuiet operation\nThe Formax FD 8204CC Deskside Shredder is as compact as a wastebasket, with enough power to handle CDs, paper clips, staples and credit cards. This rugged cross-cut model provides on-the-spot destruction of sensitive paperwork, phone messages and notes generated throughout the day. This cross-cut model can shred up to 17 sheets at a time, up to 7.5 feet per minute, with a shred size of 5/32\" x 1 3/8\". The new design is also quieter than its predecessor. The FD 8204CC is ideal for busy professionals or the small home office.",null,null,"https://www.formax.com/solutions/deskside-shredders/fd-8204cc",null,"https://www.formax.com/sites/default/files/files/products/FD-8204_0.pdf","Yes","Yes"]
[null,null,"FD 8302 Deskside Shredders","Key Features\nAutoStart/AutoStop\nAll-metal cabinet\nStrip Cut model shreds CDs\nHeat-treated steel cutters\nFormax FD 8302 Deskside Shredders are as compact as a wastebasket, yet provide enough power to handle paper clips and staples. Two models offer on-the-spot destruction of sensitive paperwork, phone messages, and notes generated throughout the day. The Strip-Cut model can also shred CDs with its dedicated CD feed opening.\n\nThe FD 8302CC Cross-Cut model can shred up to 8 sheets at once, up to 27 feet per minute, with a microcut shred size of 1/16\" x 5/8\".\n\nThe FD 8300SC Strip-Cut model can shred up to 23 sheets at once, up to 21 feet per minute, with a shred size of 5/32\".\n\nThe 8302 Series Deskside Shredders are ideal for busy professionals or the small home office.",null,null,"https://www.formax.com/solutions/data-destruction-solutions/fd-8302",null,"https://www.formax.com/sites/default/files/files/products/FD%208302%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"FD 8254CC Deskside Shredder","Key Features\nAutoStart/AutoStop\nInfeed: up to 14 sheets\nShred size .15\" x 1.18\"\nCredit cards, staples, paper clips\nSpeed: up to 17.5 fpm\nEnergy-saving standby mode\nThe FD 8254CC provides high-quality shredding performance in a deskside model. This cross-cut shredder offers on-the-spot destruction of sensitive paperwork, phone messages and notes generated throughout the day.\n\nCompact and powerful, it shreds paper into P-4/Level 3 particles, meeting HIPAA regulations, and with solid steel cutting blades, it also handles credit cards, paper clips and staples with ease. Continuous Duty Operation allows for continual shredding with no down time. The removable waste bin features a fill-level window making it simple to see when it’s time to be emptied. And when it’s not in use, power consumption is reduced with its zero-energy stand-by mode.\n\nThe FD 8254CC is ideal for busy professionals or the small home office.",null,null,"https://www.formax.com/solutions/deskside-shredders/fd-8254cc",null,"https://www.formax.com/sites/default/files/files/products/FD%208254CC%20Spec%20Sheet.pdf","Yes","Yes"]
[null,"Office Shredders"]
[null,null,"OnSite FD 8402 Office Shredders","Key Features\nAutoStart/AutoStop\nLED Control Panel\nCross-Cut or Strip-Cut\nEnergy-saving ECO Mode\nAll-metal cabinet\nOptional oiling system\nFormax OnSite FD 8402 Office Shredders offer commercial-grade components in a sleek, practical design. An easy-to-use LED control panel puts the power right at your fingertips.\n\nThe FD 8402CC Cross-Cut model can shred up to 26 sheets at once, up to 33 feet per minute, with a shred size of 5/32\" x 1 1/5\".\n\nThe FD 8402SC Strip-Cut model can shred up to 32 sheets at once, up to 30 feet per minute, with a shred size of 1/4\".\n\nIn addition, the new ECO mode saves energy by automatically switching into standby mode after 5 minutes of inactivity.\n\nThe optional EvenFlow™ Automatic Oiling System periodically lubricates the cutting blades based on motor run time, keeping the shredder in peak operating condition.",null,null,"https://www.formax.com/solutions/data-destruction-solutions/fd-8402",null,"https://www.formax.com/sites/default/files/files/products/FD%208402.pdf","Yes","Yes"]
[null,null,"OnSite FD 8502 Office Shredders","Key Features\nAutoStart/AutoStop\nLED Control Panel\nCross-Cut or Strip-Cut\n16\" feed opening\nEnergy-saving ECO Mode\nAll-metal cabinet\nOptional oiling system\nFormax FD 8502 Office Shredders are built to the highest standards for operator convenience, safety and reliability. Both cross-cut and strip-cut models feature an easy-to-use LED control panel which puts commercial-grade power right at your fingertips.\n\nThe FD 8502CC Cross-Cut model can shred 23-25 sheets at a time, up to 35 feet per minute, with a shred size of 5/32\" x 1 1/5\".\n\nThe FD 8502SC Strip-Cut model can shred up to 22 sheets at once, up to 33 feet per minute, with a shred size of 5/32\".\n\nHeat-treated steel blades, a steel cabinet, lifetime guaranteed waste bin, and a powerful AC geared-motor ensure years of reliable performance and information security in your office environment. In addition, the ECO Mode saves energy by automatically switching into standby mode after 5 minutes of inactivity.\n\nThe optional EvenFlow™ Automatic Oiling System periodically lubricates the cutting blades based on motor run time, keeping the shredder in peak operating condition.",null,null,"https://www.formax.com/solutions/data-destruction-solutions/fd-8502",null,"https://www.formax.com/sites/default/files/files/products/FD%208502.pdf","Yes","Yes"]
[null,null,"OnSite FD 8502AF AutoFeed Shredder","Key Features\nAutoFeed up to 175 sheets\nLED Control Panel\nUp to 11\" x 17\" paper\nAll-metal cabinet\n16\" feed opening\nEnergy-saving ECO Mode\nOptional oiling system\nThe Formax FD 8502AF AutoFeed Office Shredder features a dedicated AutoFeed Hopper which allows users to load up to 175 sheets, press start and walk away! No more standing in front of the shredder, hand-feeding small stacks of paper one after another.\n\nThe AutoFeeder has a capacity of up to 175 sheets, up to 11” x 17”. The Standard Hand-Feed Hopper accommodates 22-24 sheets at a time, with a 16\" wide throat.\n\nCommercial-grade features include an easy-to-use LED control panel with load indicator, heat-treated steel blades, a steel cabinet, lifetime guaranteed waste bin, and a powerful AC geared-motor ensuring years of reliable performance and information security in your office environment.  In addition, the ECO Mode saves energy by automatically switching into standby mode after 5 minutes of inactivity.",null,null,"https://www.formax.com/solutions/data-destruction-solutions/fd-8502af","https://www.youtube.com/watch?v=Y_g-1sYe-JE","https://www.formax.com/sites/default/files/files/products/FD%208502AF.pdf","Yes","Yes"]
[null,null,"OnSite FD 8602 Office Shredders","Key Features\nAutoStart/AutoStop\nLED Control Panel\nCross-Cut or Strip-Cut\n16\" feed opening\nEnergy-saving ECO Mode\nAll-metal cabinet\nOptional oiling system\nFormax OnSite FD 8602 Office Shredders feature an extra wide 16\" feed opening combined with commercial-grade components in a sleek, practical design. An easy-to-use LED control panel puts the power right at your fingertips.\n\nThe FD 8602CC Cross-Cut model can shred up to 37 sheets at a time, up to 22 feet per minute, with a shred size of 5/32\" x 1 1/5\".\n\nThe FD 8602SC Strip-Cut model can shred up to 31 sheets at once, up to 30 feet per minute, with a shred size of 1/4\".\n\nCommercial-grade components include heat-treated steel blades, a steel cabinet, lifetime guaranteed waste bin, and a powerful AC geared-motor to ensure years of reliable performance and information security in your office environment. In addition, the new ECO mode saves energy by automatically switching into standby mode after 5 minutes of inactivity.\n\nThe optional EvenFlow™ Automatic Oiling System helps to keep the FD 8602CC and FD 8602SC in peak operating condition.",null,null,"https://www.formax.com/solutions/data-destruction-solutions/fd8602",null,"https://www.formax.com/sites/default/files/files/products/FD%208602.pdf","Yes","Yes"]
[null,null,"OnSite FD 8652CC AutoOiler Shredder","Key Features\nAutoStart/AutoStop\nLED Control Panel\nCross-Cut or Strip-Cut\nEnergy-saving ECO Mode\n16\" feed opening\nAll-metal cabinet\nOiling system\nThe Formax OnSite FD 8652CC AutoOiler Shredder features fully-automatic internal oiler that periodically pumps oil onto the cutting blades for optimal performance.\n\nThe FD 8650CC is an office-size shredder with industrial strength, and shreds up to 32 sheets at one time at speeds up to 33 feet per minute. The extra wide feed opening handles documents up to 16” wide and the large waste bin holds up to 53 gallons. These specifications make it an ideal centralized office shredder.  In addition, the ECO Mode saves energy by automatically switching into standby mode after 5 minutes of inactivity.\n\nCommercial-grade features include an easy-to-use LED control panel with load indicator, heat-treated steel blades, a steel cabinet, lifetime guaranteed waste bin, and a powerful AC geared-motor ensuring years of reliable performance and information security in your office environment.",null,null,"https://www.formax.com/solutions/data-destruction-solutions/fd-8652cc",null,"https://www.formax.com/sites/default/files/files/products/FD%208652.pdf","Yes","Yes"]
[null,null,"OnSite FD 8704CC Multimedia Shredder","Key Features\nShreds Flash Drives, CD, DVDs, mini DV\nShreds CDs, DVDs, mini DV\nSeparate infeed for media\nLED Control Panel\nEnergy-saving ECO Mode\nAuto Start/Stop, Reverse\nOptional oiling system\nThe OnSite FD 8704CC Multimedia Office Shredder offers commercial-grade quality and unmatched features in a compact design ideal for the office environment. \n\nIt features two dedicated feed openings: one to accept up to 45 sheets of paper at once, and a second feed opening specially designed to shred multiple CDs, DVDs, and DV tapes at one time. Paper can be shred at a speed of up to 12 feet per minute, with a shred size of 5/32\" x 1 5/8\". The FD 8704CC has a waste bin capacity of up to 33 gallons.\n\nStandard features include heat-treated steel blades, an easy-to-use LED control panel, lifetime guaranteed waste bin, and a powerful AC geared-motor.  In addition, the new ECO mode saves energy by automatically switching into standby mode after 5 minutes of inactivity.\n\nThe optional EvenFlow™ Automatic Oiling System helps to keep the FD 8704CC in peak operating condition.",null,null,"https://www.formax.com/solutions/data-destruction-solutions/fd-8704cc",null,"https://www.formax.com/sites/default/files/files/products/FD%208704.pdf","Yes","Yes"]
[null,"Industrial Shredders"]
[null,null,"FD 8806CC / 8806SC Industrial Shredders","Key Features\nHigh-capacity industrial\nConveyor fed\nCross cut / Strip cut\nLED Control Panel\nShred entire files & more\nAutomatic Oiling System\nThe Formax FD 8806CC Cross Cut and 8806SC Strip Cut are among the most advanced high volume industrial shredders available. These high-capacity conveyor-fed shredders combine fully-automated features with the rugged, industrial strength needed for high volume centralized shredding.\n\nStandard features include an LED control panel with load indicator which provides immediate feedback to the operator, maximizing efficiency and minimizing jams. The continuous-duty motor, all-metal gearing and heat-treated solid steel cutting blades provide the power to shred up to 90 sheets (CC) or 110 sheets (SC) in one pass, as well as entire files, stacks of computer forms, cardboard, CDs and magnetic discs.\n\nUser-friendly features include Auto Start/Stop, Auto Reverse, and Auto Cleaning, rugged plastic waste bin on casters, a large safety stop bar, and key lock. The EvenFlow™ Automatic Oiling System is another standard feature, which lubricates the all-steel cutting blades, helping to keep the FD 8806CC and 8806SC in peak operating condition.",null,null,"https://www.formax.com/solutions/industrial-shredders/fd-8806","https://www.youtube.com/watch?v=VpDATK1K19M","https://www.formax.com/sites/default/files/files/products/FD%208806CC-SC%20Spec%20Sheet_0.pdf","Yes","Yes"]
[null,null,"FD 8850CC Industrial Shredder","Key Features\nShreds a variety of media\nHigh-capacity\nTwo separate infeeds\nShreds crumpled paper\nAutomatic Oiling System\nThe Formax FD 8850CC Industrial Shredder offers automated features and rugged construction for high volume centralized shredding of a variety of media.\n\nTwo separate infeeds offer the ability to shred a variety of media. The upper input hopper has a rotating bin to accommodate batches of crumpled paper. Simply dump your waste bin into the hopper, even while the shredder is running. The standard input handles paper, stacks of continuous computer paper, credit cards, CDs/DVDs, computer disks, and USB flash drives. In addition, a convenient shelf pulls out to allow for easier feeding.\n\nStandard features include an LED control panel and user-friendly features such as Auto Start/Stop and Auto Reverse to clear paper jams. Its mobile waste bin on casters and reusable bag make emptying the shredder a breeze. With an AC-geared motor and chain drive, it has the power to shred up to 80 sheets of paper at once, into Level 3 shred particles 1/8” x 2”.\n\nThe EvenFlow™ Automatic Oiling System lubricates the cutting blades, helping to keep the shredder in peak operating condition.\n\nThe FD 8850CC provides security and versatility in a compact powerful package.",null,null,"https://www.formax.com/solutions/data-destruction-solutions/fd-8850cc","https://www.youtube.com/watch?v=oJ65vYzfeqg","https://www.formax.com/sites/default/files/files/products/FD%208850CC%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"FD 8906CC Industrial Shredder","Key Features\nHigh-capacity\nUp to 650 sheets at once\nLED Control Panel\nShreds entire files & more\nAutomatic Oiling System\nOptional output conveyor\nThe Formax FD 8906CC Industrial Shredder offers high capacity for shredding large volumes of material, and can serve the needs of an entire organization. It's powerful enough to shred just about anything including entire files, stacks of computer forms, cardboard, tapes, CDs and magnetic disks.\n\nThe FD 8906CC Cross-Cut model can shred up to 650 sheets at once, up to 35 feet per minute, with a shred size of 5/16\" x 1 1/2\" - 3\". Features include an LED Control Panel with digital load indicator, Auto Start/Stop, Auto Reverse and Auto Cleaning, and front waste bin access, to allow for placement against a wall.\n\nThe newly-redesigned waste bin has two side-by-side compartments. This makes the waste bin much easier to empty with two smaller canvas bags instead of one large bag. The waste bin is also easier to slide in and out of the shredder, thanks to high-quality guide rollers on both sides of the internal frame. The original single-compartment waste bin is still available as an option.\n\nThe EvenFlowTM Automatic Oiling System is a standard feature which lubricates the all-steel cutting blades, helping to keep the shredder in peak operating condition.\n\nIn addition, an optional Ouput Conveyor Belt System is available for the FD 8906CC which transports material out of the shredder and into an external waste bin, increasing capacity and decreasing down time between emptying and replacing the waste bin.",null,null,"https://www.formax.com/solutions/industrial-shredders/fd-8906cc","https://www.youtube.com/watch?v=eMH_viL8bJY","https://www.formax.com/sites/default/files/files/products/FD%208906CC%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"FD 8906B Industrial Shredder","Key Features\nHigh-capacity\nBaler compacts shredded material\nUp to 650 sheets at once\nLED Control Panel\nShreds entire files & more\nAutomatic Oiling System\nThe Formax FD 8906B Industrial Shredder and Baler is a high-capacity conveyor-fed unit designed for large volume shredding in a central location and offers fully-automated features including Auto Start/Stop, Auto Reverse and Auto Cleaning for ease of use.\n\nThe FD 8906B combines the power and features of the FD 8906CC with an Output Baler for convenient disposal of shredded material. The Baler continually compacts shredded material into a bale, which is then ejected into a plastic bag for easy disposal.\n\nThe FD 8906B can shred stacks of computer forms, cardboard, tapes, ribbons, CDs, magnetic disks, and entire files up to 650 sheets, at a speed of up to 35 fpm.\n\nStandard features include an LED Control Panel with load indicator, heat-treated solid-steel cutting blades, a powerful AC geared-motor, and a variety of safety features. Shredding blades can also be customized to meet your specific needs.\n\nThe standard EvenFlow™ automatic oiling system with 25 heavy-duty copper nozzles lubricates the cutting blades, helping to keep the FD 8906B in peak operating condition.",null,null,"https://www.formax.com/solutions/industrial-shredders/fd-8906b","https://www.youtube.com/watch?v=eMH_viL8bJY","https://www.formax.com/sites/default/files/files/products/FD%208906B%20Spec%20Sheet.pdf","Yes","Yes"]
[null,"High Security Shredders"]
[null,null,"FD 8300HS High Security Deskside Shredder","Key Features\nNSA Level 6 High Security\nAutoStart/Stop/Reverse\nLED Control Panel\nShred size: 1/32\" x 3/16\"\nAll-metal cabinet\nThe Formax FD 8300HS High Security Deskside Shredder offers Level 6 Security in a compact, rugged design that fits right under a desk to shred “Top Secret” or classified documents. An easy-to-use LED control panel puts the power right at your fingertips, and commercial-grade components ensure durability.\n\nThis cross-cut model can shred up to 8 sheets at once, up to 23 feet per minute, with a shred size of 1/32” x 3/16”. It has been evaluated by the NSA and meets the requirements of NSA/CSS specification 02-01 for Level 6 high security cross-cut shredders. In addition, the ECO Mode saves energy by automatically switching into standby mode after 5 minutes of inactivity.\n\nCommercial-grade features include heat-treated steel blades, a steel cabinet, lifetime guaranteed waste bin, and a powerful AC geared-motor. The optional EvenFlow™ Automatic Internal Oiling System helps to keep the FD 8300HS in peak operation.",null,null,"https://www.formax.com/solutions/data-destruction-solutions/fd-8300hs",null,"https://www.formax.com/sites/default/files/files/products/FD8300HS_0.pdf","Yes","Yes"]
[null,null,"FD 8400HS-1 High Security Office Shredder","Key Features\nNSA Level 6 High Security\nAutoStart/Stop/Reverse\nLED Control Panel\nShred size: 1/32\" x 3/16\"\nAll-metal cabinet\nEvenFlow Automatic Oiling System\nEnergy-saving ECO Mode\nFormax FD 8400HS-1 High Security Office Shredders offer Level 6 security with commercial-grade components in a sleek, practical design. An easy-to-use LED control panel puts the power right at your fingertips.\n\nThe FD 8400HS-1 shreds up to 7 sheets at once, up to 23 feet per minute, with a shred size of 1/32\" x 3/16\".\n\nThe FD 8400HS-1 has been evaluated by the NSA and meets the requirements of NSA/CSS specification 02-01 for Level 6 high security cross cut shredders.\n\nThe EvenFlow™ Automatic Oiling System is standard on the FD 8400HS-1, and periodically lubricates the cutting blades based on motor run time, keeping the shredder in peak operating condition. In addition, the new ECO mode saves energy by automatically switching into standby mode after 5 minutes of inactivity.",null,null,"https://www.formax.com/solutions/data-destruction-solutions/fd8400hs-1",null,"https://www.formax.com/sites/default/files/files/products/FD8400HS-1.pdf","Yes","Yes"]
[null,null,"FD 8500HS High Security Office Shredder","Key Features\nNSA Level 6 High Security\nAutoStart/Stop/Reverse\nLED Control Panel\nShred size: 1/32\" x 3/16\"\n16\" feed opening\nAll-metal cabinet\nEnergy-saving ECO Mode\nOptional oiling system\nFormax FD 8500HS High Security Office Shredders offer Level 6 Security with a 16\" feed opening combined with commercial-grade components in a sleek, practical design. An easy-to-use LED control panel puts the power right at your fingertips.\n\nThe FD 8500HS Cross-Cut model can shred up to 5 sheets at a time, up to 35 feet per minute, with a shred size of 1/32\" x 3/16\".\n\nThe FD 8500HS has been evaluated by the NSA and meets the requirements of NSA/CSS specification 02-01 for Level 6 high security cross cut shredders. In addition, the new ECO mode saves energy by automatically switching into standby mode after 5 minutes of inactivity.\n\nThe optional EvenFlow™ Automatic Oiling System periodically lubricates the cutting blades based on motor run time, keeping the shredder in peak operating condition.",null,null,"https://www.formax.com/solutions/data-destruction-solutions/fd-8500hs",null,"https://www.formax.com/sites/default/files/files/products/FD8500HS.pdf","Yes","Yes"]
[null,null,"FD 8650HS High Security Office Shredder","Key Features\nNSA Level 6 High Security\nAutomatic Oiling System\nExtra-wide 16\" feed opening\nShred size: 1/32\" x 3/16\"\nLED Control Panel\nEnergy-saving ECO Mode\nFormax FD 8650HS High Security Office Shredders offers Level 6 Security, with an automatic oiler that oils the cutting blades periodically for optimal performance.\n\nThe FD 8650HS is an office size shredder with industrial strength, and shreds up to 15 sheets at once, up to 24 feet per minute, with a shred size of 1/32” x 3/16”. Evaluated by the NSA, it meets the requirements of NSA/CSS specification 02-01 for Level 6 high security cross cut shredders. The extra wide feed opening handles documents up to 16” wide and the large waste bin holds up to 53 gallons.  In addition, the ECO Mode saves energy by automatically switching into standby mode after 5 minutes of inactivity.\n\nCommercial-grade features include an easy-to-use LED control panel with load indicator, heat-treated steel blades, a steel cabinet, lifetime guaranteed waste bin, and a powerful AC geared-motor ensuring years of reliable performance and information security in your office environment.",null,null,"https://www.formax.com/solutions/data-destruction-solutions/fd-8650hs","https://www.youtube.com/watch?time_continue=1&v=JMUk3w-F2zI","https://www.formax.com/sites/default/files/files/products/FD8650HS_0.pdf","Yes","Yes"]
[null,null,"FD 8712HS High Security Optical Media Shredder","Key Features\nNSA/CSS specs for optical media destruction\nShreds CD-R, CD-RW, CD-ROM and DVD\nAutomatic Oiling System\nShreds up to 1,068/hour\nLED Control Panel\nEnergy-saving ECO Mode\nThe FD 8712HS High Security Optical Media Shredder meets the requirements of NSA/CSS Specification for Optical Media Destruction Devices.\n\nThis shredder is the perfect solution for top secret and classified destruction of Optical Media including CD-ROM, CD-R, CD-RW and DVDs. The cutting system shreds up to 1,068 disks per hour into 1/16\" x 5/32\" particles.\n\nStandard features include an all-metal cabinet with casters, steel gearing, lifetime guaranteed waste bin, and an easy-to-use control panel with digital load indicator. In addition, the ECO Mode saves energy by automatically switching into standby mode after 5 minutes of inactivity.\n\nThe EvenFlow™ Automatic Internal Oiling System is an available option, which lubricates the cutting blades automatically during use to keep them in peak operating condition.",null,null,"https://www.formax.com/solutions/data-destruction-solutions/fd-8712hs",null,"https://www.formax.com/sites/default/files/files/products/FD%208712HS%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"FD 8730HS High Security Paper / Optical Media Shredder","Key Features\nNSA Level P-7 High Security\nSeparate feed/waste bins\nShreds paper, CDs, DVDs\nAutomatic Oiling System\nLED Control Panel\nEnergy-saving ECO Mode\nThe FD 8730HS High Security Paper & Optical Media Shredder is a combination High Security Shredder for the destruction of Paper and Optical Media that meets the requirements of NSA/CSS Specification 02-01 for High Security Cross-Cut Paper Shredders as well as NSA/CSS Specification 04-02 for Optical Media Destruction Devices.\n\nThe FD8730HS is the perfect solution for top secret and classified shredding of Paper and Optical Media including all types of CDs, DVDs and credit cards. The CD cutting system shreds up to 2,000 CDs per hour into 1/16\" x 5/32\" particles and the Paper cutting system shreds up to 15 sheets at once, up to 23 feet per minute, producing 1/32\" x 3/16\" particles.\n\nThe FD 8730HS includes the EvenFlow™ Automatic Internal Oiling System that lubricates the cutting heads automatically during use. Other features include an all-metal cabinet with casters, steel gearing, lifetime guaranteed waste bins, and an easy-to-use control panel with digital load indicator. In addition, the ECO Mode saves energy by automatically switching into standby mode after 5 minutes of inactivity.",null,null,"https://www.formax.com/solutions/data-destruction-solutions/fd-8730hs","https://www.youtube.com/watch?v=UMrRHphCVjQ","https://www.formax.com/sites/default/files/files/products/FD8730HS_0.pdf","Yes","Yes"]
[null,"Hard Drive Punch"]
[null,null,"FD 87HD Hard Drive Punch","Key Features\nPunctures hard drives\nHandles 2.5\" and 3.5\" drives\nTransparent safety shield\nNickel-plated steel punch\nLED-illuminated chamber\nConvenient waste bin\nDiscarding a hard drive is not as simple as tossing it in the trash. And even if you erase the drive by magnetically degaussing, are you sure the data is secure?\n\nThe Formax FD 87HD Hard Drive Punch provides that added level of security by punching a hole through discarded hard drives, causing visible damage and making the stored data virtually unreadable.\n\nSimply load a hard drive into the feed chute, close the safety shield, and with the push of a button, the high-quality steel punch punctures the hard drive, which then slides into a convenient waste bin for storage until disposal or recycling.\n\nThe FD 87HD punching die is made of hardened, nickel-plated steel for durability, and handles the two most common hard drive sizes, 2.5” and 3.5”, without any additional adjustments. LEDs illuminate the chamber during the punching process, visible through the transparent safety shield.\n\nThe LED control panel displays the status and offers jam protection with auto reverse and automatic stop. In addition, sensors stop the motor automatically if the door is open or waste bin is full. The powerful geared motor is housed in an all-metal cabinet with casters for mobility and is designed for low operational noise.\n\nFor that added measure of security, trust a Formax FD 87HD Hard Drive Punch to be sure your digital data doesn’t end up in the wrong hands.",null,null,"https://www.formax.com/solutions/data-destruction-solutions/fd-87hd","https://www.youtube.com/watch?v=vkCvWcHQo88","https://www.formax.com/sites/default/files/files/products/FD87HD.pdf","Yes","Yes"]
[null,"Casino Shredder"]
[null,null,"FD 87 Casino Shredder","Key Features\nShreds cards, dice, chips, tokens\nDedicated shredding chamber\nTransparent safety shield\nSolid-steel cutting blades\nLED Control Panel\nRugged, convenient waste bin\nCommercial-grade power for highly-sensitive casino game pieces\n\nIn the casino and gaming industry, security is a top priority, both on the gaming floor and behind the scenes. Reduce the risk of fraud with the FD 87 Casino Shredder. This specially-designed unit combines user-friendly features with the industrial strength needed to ensure retired gaming pieces stay out of the wrong hands.\n\nSolid-steel cutting blades and a heavy-duty motor shred entire decks of playing cards, multiple dice, casino chips, coins and gaming tokens. Simply open the enclosed shredding chamber, drop in the items and close the latch. Press Start on the LED Control Panel and watch through the clear plexi window as the blades shred each piece. Shredded particles are then collected in the rugged molded plastic waste bin for secure disposal.\n\nThe Formax FD 87 Casino Shredder is ideal for behind-the-scenes security in gaming facilities of all sizes.",null,null,"https://www.formax.com/solutions/data-destruction/fd-87-casino-shredder","https://www.youtube.com/watch?v=KVw0lBh_lls","https://www.formax.com/sites/default/files/files/products/FD%2087%20Casino%20Spec%20Sheet.pdf","Yes","Yes"]
["Digital Print & Finishing","Digital Color Printers"]
[null,null,"ColorMax7 Digital Color Printer","Key Features\nHigh-speed inkjet printer\nFull CMYK color\nFull bleed 8.5\" x 17\"\nHigh-capacity ink tanks\nThe ColorMax7 Digital Color Printer uses the latest in inkjet technology to produce full-color output at three times the speed of traditional shuttle head printers, at one third the per-page cost. Its Memjet® print head has 70,400 ink nozzles and no moving parts, which offers higher speeds, lower ink and maintenance costs and less noise.\n\nThe ColorMax7 produces full-color CMYK output, up to 16.8 million colors, on a variety of paper stocks and sizes, with full-bleed capability on media up to 8.5” wide. It can print 1600 x 1600 dpi at 6 inches per second, and 1600 x 800 dpi at 12 inches per second.\n\nWith its thermal inkjet technology, it doesn’t require heat or contact to create an image, so it can safely be used with pre-printed envelopes and windowed envelopes without damaging the window or marring the original image. High-capacity ink tanks and fully-automated print head cleaning ensure optimum print quality throughout print runs.",null,null,"https://www.formax.com/solutions/mailing-solutions/colormax7-digital-color-printer","https://www.youtube.com/watch?v=tANeTIox3Xc","https://www.formax.com/sites/default/files/files/products/ColorMax7%20Spec%20Sheet_0.pdf","Yes","Yes"]
[null,null,"ColorMaxLP Digital Color Label Printer","Key Features\nHigh-speed inkjet label printer\nFull CMYK color\nFull bleed up to 8.5\" wide\nSpeed up to 60 ft/min\nHigh-capacity ink tanks\nUp to 1600 dpi\nGloss, semi-gloss, matte\nThe ColorMaxLP Digital Color Label Printer prints brilliant color labels at up to 60 feet per minute. Using the latest Memjet® inkjet technology, it produces full-color CMYK output, reproducing up to 16.8 million colors, on a variety of label stocks and styles, with full-bleed capability on media up to 8.5” wide.\n\nThe Memjet® print head has 70,400 ink nozzles and no moving parts, which offers higher speeds, lower ink and maintenance costs, and can print up to 1600 x 1600 dpi at 12 inches per second / 60 feet per minute. Featuring a “warm start,” the ColorMaxLP begins printing in under 10 seconds, and its high-capacity 250ml ink tanks allow for longer uninterrupted print runs. Three output modes -- roll-to-roll, roll-to-cut, and print & hold -- allow users to choose the most convenient option for their particular job.\n\nStandard features include an integrated roll unwinder which is enclosed to protect against dust, LCD control panel, built-in automatic cutter, Bartender label design software and easy-access service bays for ink cartridge replacement.\n\nOptions include an automatic roll-to-roll rewinder, Wasatch SoftRIP color matching software, a variable data printing module, and a convenient adjustable-height cabinet.\n\nThe ColorMaxLP is the ideal solution for high-quality, low-cost short to mid-run label printing applications.",null,null,"https://www.formax.com/solutions/digital-color-printers/ColorMaxLP","https://www.youtube.com/watch?v=WZKWh0QQVsA","https://www.formax.com/sites/default/files/files/products/ColorMaxLP%20Spec.pdf","Yes","Yes"]
[null,null,"ColorMaxT5 Digital Color Multimedia Printer","Key Features\nDurable toner-based prints\nPrints CMYK, CMYK+white\nPrint envelopes, various other media\nLED print heads\nColor-on color, white-on color media\nHigh-capacity toner cartridges\nColor LCD control panel\nThe ColorMaxT5 Digital Color Multimedia Printer produces outstanding professional-quality output, up to 50 pages per minute, with the ability to print CMYK plus white toner in a single pass.  Five-color printing takes envelopes, marketing collateral, and more to a whole new level: print color-on-color or white-on-color and watch the colors pop off the page. Revolutionary multi-level LED print heads control the amount of toner applied to each 1200-dpi dot, preserving fine image detail for even printing across the entire document.\n\nDry-toner based printing is durable enough for envelopes to withstand the elements, and with its straight feed path, high-capacity feeder and output conveyor, the ColorMaxT5 is ideal for printing envelopes of all sizes. It easily handles 360gsm extra-thick card stock, polyester, magnetic media, transparency films and much more, in sizes ranging from 3” x 5” index cards to 13” x 52” banners.\n\nHigh-capacity toner cartridges produce up to 38,000 pages, keeping projects up and running for longer periods without costly down-time. Replacing consumables is easy with the front-access compartment. Its high-resolution color LCD control panel features an alphanumeric keypad, and displays real-time information on print jobs and toner levels. Duplex printing is standard, allowing users to feed and print two-sided documents in one pass.\n\nThe powerful 2GB of memory and 1 Gigabit network provide a platform designed to support a variety of features and services, now and in the future.\n\nNo more reliance on outside printing vendors, which can be costly, and time-consuming. With the ColorMaxT5, users can produce brilliant color-on-color or white-on-color jobs on-demand, on-site.",null,null,"https://www.formax.com/solutions/digital-color-printers/ColorMaxT5","https://www.youtube.com/watch?v=Na4-QxPQg80","https://www.formax.com/sites/default/files/files/products/ColormaxT5%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"ColorMaxT4 Digital Color Multimedia Printer","Key Features\nDurable toner-based print\nPrint envelopes, various other media\nLED print heads\nStraight feed path\nHigh-capacity toner cartridges\nColor LCD control panel\nThe ColorMaxT4 Digital Color Multimedia Printer produces outstanding professional-quality output, up to 50 pages per minute. Revolutionary multi-level LED print heads control the amount of toner applied to each 1200-dpi dot, preserving fine image detail for even printing across the entire document.\n\nDry-toner based printing is durable enough for envelopes to withstand the elements, and with its straight feed path, high-capacity feeder and output conveyor, the ColorMaxT4 is ideal for printing envelopes of all sizes. It easily handles 360gsm extra-thick card stock, polyester, magnetic media, transparency films and much more, in sizes ranging from 3” x 5” index cards to 13” x 52” banners.\n\nHigh-capacity toner cartridges produce up to 38,000 pages, keeping projects up and running for longer periods without costly down-time. Replacing consumables is easy with the front-access compartment. Its high-resolution color LCD control panel features an alphanumeric keypad, and displays real-time information on print jobs and toner levels. Duplex printing is standard, allowing users to feed and print two-sided documents in one pass.\n\nThe powerful 2GB of memory and 1 Gigabit network provide a platform designed to support a variety of features and services, now and in the future.\n\nNo more reliance on outside printing vendors, which can be costly, and time-consuming. With the ColorMaxT4, users can produce brilliant color-on-color or white-on-color jobs on-demand, on-site.",null,null,"https://www.formax.com/solutions/digital-color-printers/ColorMaxT4","https://www.youtube.com/watch?v=Na4-QxPQg80","https://www.formax.com/sites/default/files/files/products/ColormaxT4%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"ColorMaxT6 Digital Color Multimedia Printer","Key Features\nDurable toner-based prints\nPrints CMYK, CMYK+White or Clear\nPrint envelopes, various other media\nLED print heads\nColor-on color, white-on color media\nHigh-capacity toner cartridges\nColor LCD control panel\nThe ColorMaxT6 Digital Color Multimedia Printer produces outstanding CMYK output using revolutionary multi-level LED print heads to control the amount of toner applied to each 1200-dpi dot, for fine detail across the entire document. High-capacity toner cartridges produce up to 38,000 pages, using dry toner which is durable, and ideal for envelopes to withstand the elements.\n\nThe ColorMaxT6 has the ability to print CMYK plus White or Clear toner in a single pass. Using white toner allows users to print color-on-color and white-on-color, producing text and images that virtually pop right off the page. Clear gloss toner produces watermarks and artistic embellishments that simply can’t be ignored. It only takes a few minutes to switch the fifth station from White to Clear gloss toner, and back again.\n\nDesigned with a straight feed path, envelope feeder and output conveyor, the ColorMaxT6 provides Clean Sheet print technology, making it ideal for printing envelopes of all sizes. Printing at up to 50 pages per minute, it can handle a variety of stock, up to 360gsm, in sizes ranging from 3” x 5” index cards to 13” x 52” banners. This flexibility provides the ability to create envelopes, banners, mock-ups, stationery, invitations, brochures, and more.\n\nThe high-resolution color LCD control panel features an alphanumeric keypad, and displays real-time information on print jobs and toner levels. Other user-friendly features include a front-access compartment for replacing toner, and duplex printing, which allows users to feed and print two-sided documents in one pass.\n\nStandard configuration includes the printer, two 530-sheet trays, an envelope feeder and output conveyor, and a stand with casters for mobility. Options include a long paper tray for banner printing, and a 160GB hard disk kit.\n\nThe ColorMaxT6 produces brilliant full-color envelopes and more, making it ideal for print shops, mail houses, advertising agencies, businesses and schools.",null,null,"https://www.formax.com/solutions/digital-color-printers/colormaxt6","N/A","https://www.formax.com/sites/default/files/files/products/ColorMaxT6%20Spec%20Sheet.pdf","Yes","Yes"]
[null,"Color Management Software"]
[null,null,"cmColor RIP and Color Match Software","Key Features\nUse with ColorMax7 Printer\nHarlequin® RIP engine\nSpot color matching\nProfessional output\nFormax cmColor RIP and Color Match Software combines tools for color management, spot color matching, hot folders and production job presets, with the powerful Harlequin® RIP engine to provide a seamless workflow solution. Achieve outstanding overall image quality, with predictable and repeatable color standardization.\n\nUsers can edit spot color and adapt to existing specifications. ICC color profiles are built into the program to ensure high-quality color output on a wide range of media, offering more print consistency than using standard printer drivers.\n\ncmColor Software is specially designed for use with the ColorMax7 Digital Color Printer, providing a seamless workflow solution to enhance quality, manage jobs, and deliver professional color output, time after time. This software-printer combination is ideal for businesses and commercial printers who produce full-bleed color envelopes, marketing materials, invitations and much more.",null,null,"https://www.formax.com/solutions/digital-print-finishing-solutions/cmcolor",null,"https://www.formax.com/sites/default/files/files/products/cmColor%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"Wasatch SoftRIP Software","Key Features\nCompatible with ColorMax7 and ColorMaxLP\nSimple setup\nPrecision color tools\nPlug-and-play imaging configurations\nOptional Variable Data Printing\nWasatch SoftRIP Color Matching Software combines simple setup, intuitive operation and sophisticated features that  save time, money and media. It's compatible with both the ColorMax7 and ColorMaxLP Digital Color Printers.\n\nPlug-and-play imaging configurations help users with setup, while intricate color controls provide unparalleled quality color output. Its exclusive Precision Stochastic Screens Halftone Method offers excellent color reproduction with perfectly smooth gradients.\n\nSoftRIP has the capacity to manage any print environment, because it allows users to drive up to four printers simultaneously, streamlining complex production runs. The Master Queues Manager helps control the real-time status of print jobs. The money-saving Smart Nesting feature creates efficient page print layouts by combining RIP’ed files with new jobs to conserve media using Tightest Fit, Super Easy-Cut or a best-of-both option, which balances media and time savings with an innovative turn-and-trim layout.\n\nVariable Data Printing (VDP) is a convenient option which streamlines the production of customized print runs including envelopes, postcards, labels and more. Print preview, batch processing and variable data templates create media- and time-saving print layouts.",null,null,"https://www.formax.com/solutions/digital-print-finishing-solutions/wasatch-softrip",null,"https://www.formax.com/sites/default/files/files/products/Wasatch%20SoftRIP%20Spec%20Sheet.pdf","Yes","Yes"]
[null,"Cut-True Cutters"]
[null,null,"Cut-True 13M Tabletop Manual Guillotine Cutter","Key Features\nSimple to use\nCuts stacks up to 5/8\" H\nLED cutting line for accuracy\nVarious safety features\nThe Cut-True 13M Tabletop Manual Paper Cutter is rugged and compact with a hardened steel blade and LED Laser Line for precision cutting with minimal effort. Simply load a stack of paper, up to 14.5” wide, secure with the clamp, and pull down on the lever arm; it’s that easy.\n\nThe back gauge and calibrated scales allow operators to make fine adjustments, while the Laser Line shows exactly where the blade will cut, making crisp accurate cuts every time.\n\nIn addition to accuracy, the Cut-True 13M has a range of safety features including front and rear transparent covers, blade lock, external blade depth adjustment, and easy-to-use blade change safety tool.\n\nThe Cut-True 13M cuts stacks up to 5/8” high and is ideal for small print shops and others who want to produce professional-quality brochures, invitations and more.",null,null,"https://www.formax.com/solutions/cut-true-cutters/cut-true-13m",null,"https://www.formax.com/sites/default/files/files/products/Cut-True%2013M%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"Cut-True 15M Manual Guillotine Cutter","Key Features\nQuick and accurate\nCuts stacks up to 2.36\" H\nLED cutting line\nVarious safety features\nThe Cut-True 15M Manual Paper Cutter features a hardened steel blade to easily slice through paper stacks up to 2.36” high. Its Guillotine blade and LED Laser Line combine to offer precision cutting with minimal effort. Simply load a stack of paper, up to 16.9” wide, secure with the geared clamp, and pull down on the lever arm; it’s that easy.\n\nUsing the spindle-guided back gauge and calibrated scales, operators can make fine adjustments, while the Laser Line shows exactly where to cut.\n\nIn addition to accuracy, the Cut-True 15M has a range of safety features including front and rear transparent covers, blade lock, external blade depth adjustment, easy blade change access from the front of the cutter, and a wooden paper push for safe alignment. This compact model also includes a rugged metal stand and feet for tabletop use.\n\nThe Cut-True 15M is ideal for transforming brochures, invitations and more, with crisp, accurate cuts.",null,null,"https://www.formax.com/solutions/cut-true-cutters/cut-true-15m","https://www.youtube.com/watch?v=3Bwf_ChiNAY","https://www.formax.com/sites/default/files/files/products/Cut-True%2015M%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"Cut-True 16M Manual Guillotine Cutter","Key Features\nQuick and accurate\nCuts stacks up to 3.15\" H\nLED cutting line\nVarious safety features\nThe Cut-True 16M Manual Paper Cutter combines accuracy with ease-of-use in cutting paper up to 18.7” wide. With its hardened-steel Guillotine blade, and lever-activated blade arm, it has the capacity to cut through paper stacks up to 3.15” with razor-sharp precision.\n\nUsing the LED Laser Line, spindle-guided back gauge and calibrated scales, operators can make fine adjustments, and know exactly where to cut.\n\nIn addition to accuracy, the Cut-True 16M ranks high in safety features including front and rear transparent covers, blade lock, external blade depth adjustment, easy blade change access from the front of the cutter, and a wooden paper push for safe alignment. It also includes a rugged metal stand for a comfortable working height, and feet for tabletop use.\n\nThe Cut-True 16M is ideal for transforming brochures, invitations and more, with crisp, professional cutting, and makes a great addition to print shops and in-plant finishing.",null,null,"https://www.formax.com/solutions/cut-true-cutters/cut-true-16m","https://www.youtube.com/watch?v=3Bwf_ChiNAY","https://www.formax.com/sites/default/files/files/products/Cut-True%2016M%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"Cut-True 22S Semi-Automatic Guillotine Cutter","Key Features\nQuick and accurate\nElectronic two-button operation\nCuts stacks up to 1.77\" H\nLED cutting line\nVarious safety features\nThe Cut-True 22S Semi-Automatic Electric Cutter offers precision cutting for paper stacks up to 16.9” wide. This semi-automatic cutter requires very little effort, thanks to its electronically-controlled two-button operation. Simply load a stack of paper, up to 1.77” high, secure with the geared clamp, and press the buttons to engage the hardened-steel Guillotine blade.\n\nAccurate cutting is easy with its spindle-guided back gauge with LED digital readout and calibrated scales. Using these and the LED Laser Line, operators can make fine adjustments, and see exactly where the blade will cut.\n\nThe 22S doesn’t sacrifce safety for accuracy. In fact, it features an electronically-controlled front safety cover, transparent rear cover, safety lock with key, blade lock, external blade depth adjustment, easy blade change access from the front of the cutter, and a wooden paper push for safe alignment. The rugged metal stand is included, providing a stable work surface, as well as feet for tabletop use.\n\nThe Cut-True 22S is ideal for transforming brochures, invitations and more, with crisp, accurate cuts, and makes a welcome addition to print shops and in-plant finishing operations.",null,null,"https://www.formax.com/solutions/cut-true-cutters/cut-true-22s","https://www.youtube.com/watch?v=3Bwf_ChiNAY","https://www.formax.com/sites/default/files/files/products/Cut-True%2022S%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"Cut-True 27S Semi-Automatic Guillotine Cutter","Key Features\nSemi-automatic cutting\nElectronic two-button operation\nAutomatic paper clamp\nCuts stacks up to 3.15\" H\nLED cutting line\nVarious safety features\nRugged metal stand with convenient storage shelf\nThe Cut-True 27S Semi-Automatic Electric Paper Cutter offers precision cutting for paper stacks up to 18.9” wide. User-friendly features include dual-button electronic operation, automatic paper clamp, and LED digital readout. Simply load a stack of paper, up to 3.15” high and press the clamp and blade buttons to engage the hardened-steel Guillotine blade.  These features, combined with the bright red LED Cutting Line, allow operators to make fine adjustments and see exactly where the blade will cut.\n\nAccuracy meets safety in the Cut-True 27S, with front and rear transparent safety guards, blade lock, safety lock with key, external blade depth adjustment, automatic blade return from any position, easy-to-use blade change safety tool, and a wooden paper push for safe alignment. The rugged metal stand is also included, providing a stable work surface, and a convenient shelf for additional storage.\n\nThe Cut-True 27S Electric Cutter is ideal for transforming brochures, invitations and more, with crisp, accurate cuts, and makes a welcome addition to print shops and in-plant finishing operations.",null,null,"https://www.formax.com/solutions/cut-true-cutters/cut-true-27s","https://www.youtube.com/watch?v=Rzv8FHdbpYc","https://www.formax.com/sites/default/files/files/products/Cut-True%2027S%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"Cut-True 29A Automatic Electric Guillotine Cutter","Key Features\nTouchscreen control panel\nElectronic two-button operation\nAutomatic paper clamp\nCuts stacks up to 3.15\" H\nLED cutting line\nInfrared Safety Curtain\nUp to 100 programmable jobs\nThe Formax Cut-True 29A Electric Guillotine Paper Cutter offers precision cutting for paper stacks up to 20.5” wide. User-friendly, intuitive features include a touchscreen control panel, automatically-adjusting back gauge and the capacity to program up to 100 jobs/100 cuts. An infrared light beam safety curtain provides safety and convenience as it shuts down operation if the light plane is interrupted.\n\nOperation is simple: utilize the touchscreen control panel to program and select job settings, then load a stack of paper, up to 3.15” high. Set the back gauge using the touchscreen. The bright LED Cutting Line allows operators to see exactly where the blade will cut and make fine adjustments. Electronically-controlled two-hand operation engages the hardened steel blade for crisp, accurate cuts, every time.\n\nCutting accuracy is 0.1mm on paper stacks up to 80mm. The Cut-True 29A also features a special anti-friction surface with optional wide side tables, making it easier for operators to maneuver large paper stock. A false clamp is included to minimize the risk of marking sensitive paper stock or perfect bound books. In addition, the clamp can be removed to decrease the minimum cut length, and is easily stored within the machine.\n\nStandard safety features include a lock with key, blade lock, external blade depth adjustment, automatic blade return from any position, easy-to-use blade change safety tool, and a wooden paper push for safe alignment.\n\nThe Cut-True 29A is ideal for transforming large sheets into brochures, invitations and more, with crisp, accurate cuts, and is a welcome addition to print shops and in-plant finishing operations.",null,null,"https://www.formax.com/solutions/cut-true-cutters/cut-true-29a","https://www.youtube.com/watch?v=7XGlp-SEREg","https://www.formax.com/sites/default/files/files/products/Cut-True%2029A%20Spec%20Sheet.pdf","Yes","Yes"]
[{"$nulls":7},"https://www.youtube.com/embed/V3N0qBepOjQ?width=640&height=480&iframe=true"]
[{"$nulls":7},"https://www.youtube.com/embed/sOOLMJhtX6Q?width=640&height=480&iframe=true"]
[{"$nulls":7},"https://www.youtube.com/embed/eO8mEfHnByk?width=640&height=480&iframe=true"]
[{"$nulls":7},"https://www.youtube.com/embed/Gx5npDyXraM?width=640&height=480&iframe=true"]
[null,null,"Cut-True 29H Hydraulic Guillotine Cutter","Key Features\nHydraulic cutting action\nTouchscreen control panel\nElectronic two-button operation\nUp to 100 programmable jobs\nCuts stacks up to 3.15\" H\nLED cutting line\nVarious safety features\nThe Formax Cut-True 29H Hydraulic Guillotine Paper Cutter offers precision cutting for paper stacks up to 20.5” wide. User-friendly, intuitive features include a touchscreen control panel, automatically-adjusting back gauge and the capacity to program up to 100 jobs/100 cuts. An infrared light beam safety curtain provides safety and convenience as it shuts down operation if the light plane is interrupted.\n\nOperation is simple: utilize the touchscreen to program and select job settings, then load a stack of paper, up to 3.15” high. Set the back gauge using the touchscreen, then use the foot pedal pre-clamp to check the paper position. The bright LED Cutting Line allows operators to see exactly where the blade will cut and make fine adjustments. Electronically-controlled two-hand operation engages the hardened steel blade for crisp, accurate cuts, every time.\n\nCutting accuracy is 0.1mm on paper stacks up to 80mm. The Cut-True 29H also features a special anti-friction surface with optional wide side tables, making it easier for operators to maneuver large paper stock. The hydraulic clamp pressure is adjustable to give the best clamp possible for different paper weights and stack heights. A false clamp is included to minimize the risk of marking sensitive paper stock or perfect bound books. In addition, the clamp can be removed to decrease the minimum cut length, and stored within the machine. The Cut-True 29H also features an internal light to illuminate the cutting area.\n\nStandard safety features include a lock with key, blade lock, external blade depth adjustment, automatic blade return from any position, easy-to-use blade change safety tool, and a wooden paper push for safe alignment.\n\nThe Cut-True 29H is ideal for transforming large sheets into brochures, invitations and more, with crisp, accurate cuts, and is a welcome addition to print shops and in-plant finishing operations.",null,null,"https://www.formax.com/solutions/cut-true-cutters/cut-true-29h","https://www.youtube.com/watch?v=7XGlp-SEREg","https://www.formax.com/sites/default/files/files/products/Cut-True%2029H%20Spec%20Sheet.pdf","Yes","Yes"]
[{"$nulls":7},"https://www.youtube.com/embed/dcQ5VdjBAP4?width=640&height=480&iframe=true"]
[{"$nulls":7},"https://www.youtube.com/embed/sOOLMJhtX6Q?width=640&height=480&iframe=true"]
[{"$nulls":7},"https://www.youtube.com/embed/eO8mEfHnByk?width=640&height=480&iframe=true"]
[{"$nulls":7},"https://www.youtube.com/embed/Gx5npDyXraM?width=640&height=480&iframe=true"]
[null,null,"Cut-True 31A Electric Guillotine Cutter","Key Features\n7\" Color Touchscreen\nElectronic two-button operation\nAutomatic paper clamp\nCuts stacks up to 28\" wide\nLED cutting line\nInfrared Safety Curtain\nUp to 100 programmable jobs\nExtra large side tables\nThe Cut-True 31A Electric Guillotine Paper Cutter offers precision cutting for paper stacks up to 28” wide, up to 4” high. User-friendly, intuitive features include a 7” color touchscreen control panel, automatically-adjusting back gauge and the capacity to program up to 100 jobs/100 cuts. An infrared light beam safety curtain provides safety and convenience as it shuts down operation if the light plane is interrupted.\n\nOperation is simple with the full-color touchscreen for programming and selecting jobs. The foot-pedal pre-clamp and bright LED Cutting Line work together allowing operators to see exactly where the blade will cut and to make fine adjustments. Electronically-controlled two-hand operation engages the hardened steel blade for crisp, accurate cuts, every time. Cutting accuracy is 0.1mm on maximum paper stacks.\n\nThe Cut-True 31A features extra-large side tables, making it easier for operators to maneuver large paper stock. A false clamp is included to minimize the risk of marking sensitive paper stock or perfect bound books. The false clamp can be removed to decrease the minimum cut length to 1.18”, and stored within the machine when not in use. The Cut-True 31A also features an internal light to illuminate the cutting area.\n\nStandard safety features include dual-button operation and an infrared safety curtain, a lock with key, blade lock, automatic blade return from any position, an easy-to-use blade change safety tool, and a wooden paper push for safe alignment.\n\nThe Cut-True 31A is ideal for transforming large sheets into brochures, invitations and more, with crisp, accurate cuts, and is a welcome addition to print shops and in-plant finishing operations.",null,null,"https://www.formax.com/solutions/cut-true-cutters/cut-true-31a","https://www.youtube.com/watch?v=x94HjbUi5dQ","https://www.formax.com/sites/default/files/files/products/Cut-True%2031A%20Spec%20Sheet_0.pdf","Yes","Yes"]
[null,null,"Cut-True 31H Hydraulic Guillotine Cutter","Key Features\n7\" Color Touchscreen\nHydraulically controlled\nLow-friction air-assist ball deck\nCuts stacks up to 28\" wide\nLED cutting line\nInfrared Safety Curtain\nUp to 100 programmable jobs\nExtra large side tables\nThe Formax Cut-True 31H Hydraulic Guillotine Paper Cutter features a hydraulic blade and clamp drive for true two-shift operation, and rugged heavy-duty construction for precision cutting of paper stacks up to 28” wide and up to 4” high. User-friendly features include a color touchscreen control panel, automatically-adjusting back gauge, an internal light to illuminate the cutting area, and the capacity to program up to 100 jobs/100 cuts.\n\nOperation is simple using the color touchscreen for programming and selecting jobs. The foot-pedal pre-clamp and bright LED Cutting Line work together allowing operators to see exactly where the blade will cut and to make fine adjustments. Electronically-controlled two-hand operation engages the hardened steel blade for crisp, accurate cuts, every time. Cutting accuracy is 0.1mm on maximum paper stacks.\n\nThe Cut-True 31H features an anti-friction ball deck with air-assist and extra-large side tables, making it easier for operators to maneuver large paper stock. The hydraulic clamp pressure is easily adjusted using the pressure gauge knob, to provide the best clamp possible for different paper weights and stack heights. A removable false clamp is included to minimize the risk of marking sensitive paper stock or perfect bound books. It can be easily removed to decrease the minimum cut length to 1.18”, and stored within the machine when not in use.\n\nStandard safety features include dual-button operation and an infrared safety curtain which immediately stops operation if the light plane is interrupted. The Cut-True 31H also includes a lock with key, blade lock, automatic blade return from any position, a blade change safety tool, and a wooden paper push for safe alignment.\n\nThe Cut-True 31H is ideal for transforming large sheets into brochures, invitations, business cards, and more, with crisp, accurate cuts, and is a welcome addition to digital print shops and in-plant finishing operations.",null,null,"https://www.formax.com/solutions/cut-true-cutters/cut-true-31h","https://www.youtube.com/watch?v=x94HjbUi5dQ","https://www.formax.com/sites/default/files/files/products/Cut-True%2031H%20Spec%20Sheet_0.pdf","Yes","Yes"]
[null,"Card Cutters"]
[null,null,"FD 120 Card Cutter","Key Features\nCuts and slits cards, photos\nLCD Display\n6 programmable jobs\nThe FD 120 Card Cutter is ideal for processing color business cards, postcards, greeting cards and photos, right from your desktop. The FD 120 automatically cuts and slits documents and stacks them in sequential order at speeds of up to 130 business cards per minute.\n\nFeatures include an easy-to-use control panel with LCD display, 6 pre-programmed jobs, 6 programmable jobs, and the ability to cut letter and legal size paper, up to 300gsm. Optional interchangeable slit/score/perforation cassettes offer even greater productivity.",null,null,"https://www.formax.com/solutions/card-cutters/fd-120-card-cutter","https://www.youtube.com/watch?v=hwVUNDI5Z4c","https://www.formax.com/sites/default/files/files/products/FD%20120%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"FD 125 Card Cutter","Key Features\nCuts sheets up to 13\" x 19\"\nLCD Display\nFull-bleed capability\n7 programmable jobs\nThe FD 125 Card Cutter is ideal for on-demand processing of full-bleed color business cards, postcards, greeting cards and photos. With its capacity to cut a wide range of paper sizes in weights up to 300 gsm, users can create professional quality cards right from the desktop. The FD 125 features an easy-to-use control panel with LCD display, and cuts sheets from letter size up to 13” x 19”.\n\nThe FD 125 automatically cuts and slits documents and stacks them in sequential order at speeds of up to 240 business cards per minute. Users can utilize the 7 pre-programmed jobs or 6 programmable jobs to save time and effort. The unit includes a stand which doubles as an easily-accessible waste bin compartment. Options include a 15” conveyor for neat and sequential output, and interchangeable cutting cassettes for even greater productivity.",null,null,"https://www.formax.com/solutions/card-cutters/fd-125-card-cutter","https://www.youtube.com/watch?time_continue=133&v=1J-YbWAaiJE","https://www.formax.com/sites/default/files/files/products/FD125.pdf","Yes","Yes"]
[null,"Creasers/Perforators"]
[null,null,"FD 215S Semi-Automatic Creaser","Key Features\nPrevents cracking in toner-based digital printouts\nSemi-automatic operation\nAll-metal construction\nThe FD 215S Semi-Automatic Paper Creaser offers easy setup with push-button or hands-free foot pedal operation. Creasing prevents tearing and cracking in toner-based digital printouts, providing a clean professional look, and making it easier for folding devices to fold with accuracy.\n\nThe FD 215S features all-metal construction, easily adjustable paper stops, and is ideal for small print shops or businesses. Common applications include greeting cards, postcards, brochures, invitations, CD covers, and more.",null,null,"https://www.formax.com/solutions/creasers/fd-215s","https://www.youtube.com/watch?v=XoZ-S9qnPnY","https://www.formax.com/sites/default/files/files/products/FD215S.pdf","Yes","Yes"]
[null,null,"FD 90 Rotary Perforator / Creaser","Key Features\nSimple set-up & operation\nUp to 5 parallel perfs/creases in one pass\nUp to 6,800 per hour\nTelescoping infeed/outfeed\nReliable friction feeding\nSheets up to 13.8\" x 19\"\nThe FD 90 Rotary Perforator/Creaser is specially designed for finishing printed sheets, up to 13.8” x 19”. Its three-tire friction feeding system reliably feeds up to 6,800 sheets per hour, and can create up to 5 parallel perforations and/or creases in a single pass. Perforating allows for easy separation of multiple printouts, tear-offs, postcards or tickets on a single sheet, while creasing allows for easy folding and reduces unsightly cracking in digital printouts.\n\nOperation is easy: simply load printed sheets on the extendable infeed table, adjust the side guides and press the power button. Sheets are fed and perforated and/or creased automatically then stacked neatly on the telescoping outfeed table. The FD 90 can easily accommodate paper weights from 55 - 180gsm.\n\nStandard set-up includes two perforating wheels, one creasing wheel and paper guides. Options include additional perforating sets, microperforating sets (17 tpi), creasing sets and guide strips to accommodate 55 - 60gsm paper.\n\nThe FD 90 is ideal for small print shops, on-demand and in-plant finishing applications including postcards, invitations, tear-offs, brochures, billing statements and more.",null,null,"https://www.formax.com/solutions/creasers/FD-90-Perforator-Creaser","https://www.youtube.com/watch?v=Vtn3hG-vjJY","https://www.formax.com/sites/default/files/files/products/FD%2090%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"Atlas C100 High-Speed Automatic Creaser","Key Features\nFully automatic\n7\" color touchscreen\nUp to 8,500 sheets per hour\nUp to 16 creases per sheet\nBottom-suction air feed table\nSheets up to 27.5\" x 12.9\"\nIn today’s digital print environment, it’s not enough to simply print a piece; it must be finished properly for a clean, professional look. The Atlas C100 Auto-Feeding Creaser is a fully-automatic, user-friendly solution to solve the problem of cracking in toner-based digital prints. Utilizing a unique creasing matrix, it compresses paper fibers instead of cutting them, virtually eliminating cracks on a creased or folded edge.\n\nUsing the graphics-based 7” touchscreen control panel, operators can easily set-up and save jobs in just minutes or use one of the six pre-programmed settings. The C100 automatically calculates the crease positions based on paper size and sets them accordingly. The powerful bottom-suction air-feed system allows for continuous loading of sheets, which increases productivity while maintaining accuracy, even with heavier stocks.\n\nThis fully-automatic air-feed creaser offers variable speed control to accommodate a wide variety of sheet sizes and thicknesses. With the ability to produce up to 16 creases per sheet, it can process up to 8,500 sheets (8.5” x 11”) or up to 11,000 sheets (6.5” x 8.5”) per hour. Perforating capabilities are also standard, with a wide range of perf wheels to suit many different applications.\n\nWith rugged metal construction and a compact footprint, the Atlas C100 is an ideal addition to small print shops and production facilities with limited space that want to expand their digital print finishing capabilities.",null,null,"https://www.formax.com/solutions/creasers/atlas-c100","https://www.youtube.com/watch?v=flruW3fTDAY","https://www.formax.com/sites/default/files/files/products/Atlas%20Creasers%20Spec%20Sheet.pdf","Yes","Yes"]
[null,null,"Atlas C200 High-Speed Automatic Creaser","Key Features\nFully automatic\n7\" color touchscreen\nUp to 8,500 sheets per hour\nUp to 16 creases per sheet\nBottom-suction air feed table\nSheets up to 27.5\" x 19.6\"\nIn today’s digital print environment, it’s not enough to simply print a piece; it must be finished properly for a clean, professional look. The Atlas C200 Auto-Feeding Creaser is a fully-automatic, user-friendly solution to solve the problem of cracking in toner-based digital prints. Utilizing a unique creasing matrix, it compresses paper fibers instead of cutting them, virtually eliminating cracks on a creased or folded edge.\n\nUsing the graphics-based 7” touchscreen control panel, operators can easily set-up and save jobs in just minutes or use one of the six pre-programmed settings. The C200 automatically calculates the crease positions based on paper size and sets them accordingly. The powerful bottom-suction air-feed system allows for continuous loading of sheets, which increases productivity while maintaining accuracy, even with heavier stocks.\n\nThis fully-automatic air-feed creaser offers variable speed control to accommodate a wide variety of sheet sizes and thicknesses. With the ability to produce up to 16 creases per sheet, it can process up to 8,500 sheets (8.5” x 11”) or up to 11,000 sheets (6.5” x 8.5”) per hour. The C200 can accommodate sheets up to 27.5\" x 19.6\". Perforating capabilities are also standard, with a wide range of perf wheels to suit many different applications.\n\nWith rugged metal construction and a compact footprint, the Atlas C200 is an ideal addition to small print shops and production facilities with limited space that want to expand their digital print finishing capabilities.",null,null,"https://www.formax.com/solutions/creasers/atlas-c200","https://www.youtube.com/watch?v=flruW3fTDAY","https://www.formax.com/sites/default/files/files/products/Atlas%20Creasers%20Spec%20Sheet_0.pdf","Yes","Yes"]
[null,null,"Atlas C300 High-Speed Automatic Creaser/Folder","Key Features\nFully automatic\nCrease & fold in a single pass\nDynamic creasing matrix\n7\" color touchscreen\nUp to 6,000 sheets per hour\nBottom-suction air feed table\nSheets up to 27.5\" x 15.1\"\nFloating knife folding technology\nIn today’s digital print environment, it’s not enough to simply print a piece; it must be finished properly for a clean, professional look. The Atlas C300 Auto-Feeding Creaser/Folder is a fully-automatic, user-friendly solution to solve the problem of cracking in toner-based digital prints. Utilizing a unique creasing matrix, it compresses paper fibers instead of cutting them, virtually eliminating cracks on a creased or folded edge.\n\nThe Atlas C300 produces high-speed creasing and folding in a single pass. Sheets pass through the dynamic creasing matrix and the patented floating knife folding mechanism, which minimize marking of the digital printout. Speed is maintained, regardless of the number of creases: up to 9 sheets with 9 creases each can be produced in less than 9 seconds.\n\nUsing the graphics-based 7” touchscreen control panel, operators can easily set-up and save jobs in just minutes or use one of the six pre-programmed settings. The C300 automatically calculates the crease positions based on paper size and sets them accordingly. The powerful bottom-suction air-feed system allows for continuous loading of sheets, which increases productivity while maintaining accuracy, even with heavier stocks.\n\nThis fully-automatic air-feed creaser offers variable speed control to accommodate a wide variety of sheet sizes and thicknesses. With the ability to produce up to 16 creases per sheet, it can process up to 6,000 sheets per hour. The C300 can accommodate sheets up to 27.5\" x 15.1\". Perforating capabilities are also standard, with a wide range of perf wheels to suit many different applications.\n\nThe C300 can be used as a stand-alone creaser, or as a perforator when creasing and folding are not required. With rugged metal construction and a compact footprint, the Atlas C300 is an ideal addition to small print shops and production facilities with limited space that want to expand their digital print finishing capabilities.",null,null,"https://www.formax.com/solutions/creasers/atlas-c300","https://www.youtube.com/watch?v=DOH3IG_7roQ","https://www.formax.com/sites/default/files/files/products/Atlas%20Creasers%20Spec%20Sheet_1.pdf","Yes","Yes"]
[null,"Booklet Makers/Finishers"]
[null,null,"FD 180 Automatic Booklet Maker","Key Features\nLCD control panel\nPush-button operation\nUp to 500 booklets per hour\nThe FD 180 Automatic Tabletop Booklet Maker is a compact and efficient addition to any office, church, school, small print shop or in-plant operation. Quick and easy setup leads to professional-quality booklets, at the touch of a button.\n\nChoose one of six pre-set sheet sizes or program up to 6 custom sizes into memory. The LCD Control Panel and push-button controls make this desktop unit easy to use. Staple and fold up to 15 sheets of 20# bond with two automatic staplers in a choice of five stapling positions. Automatic operation and a time-delay feature give you the ability to create up to 500 booklets per hour.",null,null,"https://www.formax.com/solutions/booklet-makers/fd-180",null,"https://www.formax.com/sites/default/files/files/products/FD180.pdf","Yes","Yes"]
[null,null,"Square IT Squareback Booklet Finisher","Key Features\nCreates square binding on stapled booklets\nHandles booklets up to 96 pages\nSimple, quiet operation\nCompact and rugged with a small footprint\nOperates as a stand-alone or in-line\nThe Formax Square IT squareback booklet finisher gives your stapled booklets a professional, perfect-bound look, with the security of a stapled binding. Squareback booklets lie flat, making them easier to front-trim on a guillotine cutter. Square bindings also offer the option of printing on the spine, plus they’re easier to package and store.\n\nThe Square IT finishes booklets up to 9 1/2” x 12 3/4”, in sizes up to 24 sheets of 80gsm paper. With the easy-to-use control panel, operators can choose from four thickness options, which provide the ideal squareback binding based on the number of pages.\n\nThis versatile, compact machine can be used either as a hand-feed unit or in-line with a wide range of traditional and digital finishing devices. An optional adjustable stand is also available .\n\nTake your booklets to the next level with the Square IT squareback booklet finisher.",null,null,"https://www.formax.com/solutions/booklet-makers/square-it-finisher","https://www.youtube.com/watch?v=0uCglnaT0ao","https://www.formax.com/sites/default/files/files/products/Square%20IT.pdf","Yes","Yes"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]

{"sheet":"MBM Corp","index":6,"n_rows":185,"n_cols":12,"rows_kept":185,"cut":false,"hidden":false,"merged":[]}
["Category","Sub-Category (if applicable)","Product Name","Product Description","Specifications","Serial #","Vendor Site URL","Video Content URL(s)","Downloadable Content URL(s)","Pictures Saved?","Migrated?","Alternative Site URL"]
["Shredders","Deskside Shredders"]
[null,null,"DESTROYIT® 2270","Two separate cutting heads with separate feed openings—one for paper and one for CDs / DVDs. Removable shred bin contains separate compartments for easy material separation and disposal. Window in shred bin shows fill level. Transparent safety shield in the feed opening. Automatic power cut-off when bin is removed from cabinet. Double protection against overheating. Automatic start and stop controlled by photo cell. Multifunction control switch with pilot light. High quality, hardened steel cutting shafts take staples, paper clips, credit cards, and CDs / DVDs. Lifetime warranty on the cutting shafts. Quiet and powerful single phase motor. Fully enclosed gear box housing. High quality wooden cabinet.\n\nShred volume, gallons: 5 (paper), 3/4 (plastic) \nFeed opening, inches: 8 3/4 \nElectrical requirements, volts: 115 \nMaximum horsepower: 1/5 \nDimensions (D x W x H), inches: 8 3/4 x 13 1/2 x 21 \nShipping weight, pounds: 32","2270 STRIP-CUT\nSecurity level P-2\nStrip width 4 mm (3/16 inch)\nSheet capacity 10-12*\nShred speed, ft./min. 12\nShred capabilities (non-paper)Shreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $399\n\n2270 CROSS-CUT\nSecurity level P-4\nParticle size 3 x 25 mm (1/8 x 1 inches)\nSheet capacity 5-6*\nShred speed, ft./min. 12\nShred capabilities (non-paper)Shreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $499\n\n*Certified using 8 1/2\" x 11\" 20 pound bond and recommended power supply.",null,"https://www.mbmcorp.com/Paper-Shredders/Deskside-Shredders/DESTROYIT-2270-102.html","https://www.youtube.com/watch?v=3-8xAiTClXM",null,"Yes","Yes"]
[null,null,"DESTROYIT® 2360","Comprehensive SPS™ safety package: Easy Switch control element uses illuminated color codes and symbols to indicate operational status and functions as an emergency stop switch; patented, electronically controlled, transparent safety shield in the feed opening; automatic power cut-off when cabinet is opened or shred bin is full; automatic reverse and power cut-off when overfed; double protection against overheating; Zero Energy Consumption sleep mode cuts off power supply after 30 minutes of inactivity.\n\nAutomatic start and stop controlled by photo cell. High quality, hardened steel cutting shafts take staples, paper clips, and credit cards (strip- and cross-cut models). Super micro-cut model meets all NSA/CSS specifications and is DOD approved. Lifetime warranty on the cutting shafts (strip- and cross-cut models). 1 year warranty on super micro-cut cutting shafts. Quiet and powerful single phase motor. Fully enclosed gear box housing. High quality wooden cabinet mounted on casters. Convenient, environmentally friendly shred bin does not require disposable shred bags.\n\nShred volume, gallons: 9 \nFeed opening, inches: 9 1/2 \nElectrical requirements, volts: 115 \nMaximum horsepower: 1/2 \nDimensions (D x W x H), inches: 11 3/4 x 15 1/2 x 28 3/4 \nShipping weight, pounds: 53","2360 STRIP-CUT\nSecurity level P-2\nStrip width 4 mm (3/16 inch)\nSheet capacity 12-14*\nShred speed, ft./min. 27\nShred capabilities (non-paper)Shreds paper clips and staples effortlesslyShreds credit cards effortlessly\nList Price US $899\n\n2360 CROSS-CUT\nSecurity level P-4\nParticle size 4 x 40 mm (3/16 x 1 1/2 inches)\nSheet capacity 11-13*\nShred speed, ft./min. 14\nShred capabilities (non-paper)Shreds paper clips and staples effortlesslyShreds credit cards effortlessly\nList Price US $1,039\n\n2360 CROSS-CUT\nSecurity level P-5\nParticle size 2 x 15 mm (3/32 x 5/8 inches)\nSheet capacity 6-8*\nShred speed, ft./min. 14\nShred capabilities (non-paper)Shreds paper clips and staples effortlesslyShreds credit cards effortlessly\nList Price US $1,039\n\n*Certified using 8 1/2\" x 11\" 20 pound bond and recommended power supply.",null,"https://www.mbmcorp.com/Paper-Shredders/Deskside-Shredders/DESTROYIT-2360-103.html","https://www.youtube.com/watch?v=UiZ69zvh6gg",null,"Yes","Yes"]
[null,null,"DESTROYIT® 2465","SPS™ – (Safety Protection System) package: patented, electronically controlled, transparent safety flap in the feed opening as additional safety element; EASY- SWITCH – intelligent control element indicating the operational status of the shredder with varying color codes and back-lit symbols; automatic reverse and power cut-off (avoids paper jams); automatic stop if the shred bin is full; electronic door protection via a magnetic proximity switch; double motor protection against over-heating; ZERO ENERGY standby mode: Complete, automatic disconnection from power supply after 30 minutes. Photo cell controlled automatic start and stop. With SSC™ – smart shred control: a smiley on the EASY-SWITCH element indicates the used sheet capacity during shredding process to avoid paper jams. High-quality, paper clip proof cutting shafts from special hardened steel with lifetime guarantee. Quiet, powerful and energy-efficient single phase motor. Fully closed gear box housing and durable gears. High-quality wooden cabinet, mobile on castors. Convenient environmentally-friendly shred bin (no disposable shred bags required).\n\nShred volume, gallons: 9 \nFeed opening, inches: 9 1/2 \nElectrical requirements, volts: 115 \nMaximum horsepower: 3/4 \nProduct Dimensions (D x W x H), inches: 11.5 x 15.5 x 25\nShipping weight, pounds: 58","DESTROYIT® 2465 STRIP-CUT\nSecurity level P-2\nStrip width 4 mm (3/16 inch)\nSheet capacity 19-22*\nShred speed, ft./min. 27\nShred capabilities (non-paper)Shreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US 1,249\n\nDESTROYIT® 2465 CROSS-CUT\nSecurity level P-5\nStrip width 2 x 15 mm (3/32\" x 5/8\")\nSheet capacity 9 - 11*\nShred speed, ft./min. 27\nShred capabilities (non-paper)Shreds paper clips and staples effortlesslyShreds credit cards effortlessly\nList Price US 1,449\n\nDESTROYIT® 2465 CROSS-CUT\nSecurity level P-4\nStrip width 4 x 40 mm (3/16\" x 1 1/2\")\nSheet capacity 13 - 15*\nShred speed, ft./min. 27\nShred capabilities (non-paper)Shreds paper clips and staples effortlesslyShreds credit cards effortlessly\nList Price US 1,449\n\n*Certified using 8 1/2\" x 11\" 20 pound bond and recommended power supply.",null,"https://www.mbmcorp.com/Paper-Shredders/Deskside-Shredders/DESTROYIT-2465-422.html",null,null,"Yes","Yes"]
[null,"Centralized Office Shredders"]
[null,null,"DESTROYIT® 2503","Comprehensive SPS™ safety package: Easy Switch control element uses illuminated color codes and symbols to indicate operational status and functions as an emergency stop switch; patented, electronically controlled, transparent safety shield in the feed opening; automatic power cut-off when cabinet is opened or shred bin is full; automatic reverse and power cut-off when overfed; double protection against overheating; Zero Energy Consumption sleep mode cuts off power supply after 30 minutes of inactivity.\n\nAutomatic start and stop controlled by photo cell. High quality, hardened steel cutting shafts take staples, paper clips, and credit cards (strip-cut model takes CDs / DVDs). Lifetime warranty on the cutting shafts. Quiet and powerful single phase motor. Fully enclosed gear box housing. High quality wooden cabinet mounted on casters. Convenient, environmentally friendly shred bin does not require disposable shred bags.\n\nShred volume, gallons: 20 \nFeed opening, inches: 10 1/4 \nElectrical requirements, volts: 115 \nMaximum horsepower: 3/4 \nDimensions (D x W x H), inches: 14 3/4 x 19 3/4 x 34 1/4 \nShipping weight, pounds: 78","2503 STRIP-CUT\nSecurity level\tP-2\nStrip width\t4 mm (3/16 inch)\nSheet capacity\t19-21*\nShred speed, ft./min.\t24\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $1,679\n\n2503 CROSS-CUT\nSecurity level\tP-4\nParticle size\t4 x 40 mm (3/16 x 1 1/2 inches)\nSheet capacity\t12-14*\nShred speed, ft./min.\t24\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlessly\nList Price US $1,879\n\n2503 CROSS-CUT\nSecurity level\tP-5\nParticle size\t2 x 15 mm (3/32 x 5/8 inches)\nSheet capacity\t8-10*\nShred speed, ft./min.\t24\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlessly\nList Price US $1,879\n\n*Certified using 8 1/2\" x 11\" 20 pound bond and recommended power supply.",null,"https://www.mbmcorp.com/Paper-Shredders/Centralized-Office-Shredders/DESTROYIT-2503-117.html","https://www.youtube.com/watch?v=CgLmcAuLml0",null,"Yes","Yes"]
[null,null,"DESTROYIT® 2604","Comprehensive SPS™ safety package: Easy Switch control element uses illuminated color codes and symbols to indicate operational status and functions as an emergency stop switch; patented, electronically controlled, transparent safety shield in the feed opening; automatic power cut-off when cabinet is opened or shred bin is full; automatic reverse and power cut-off when overfed; double protection against overheating; Zero Energy Consumption sleep mode cuts off power supply after 30 minutes of inactivity.\n\nAutomatic start and stop controlled by photo cell. Patented Electronic Capacity Control (ECC) indicator prevents jams by monitoring sheet capacity levels during operation. Automatic oil injection ensures optimal performance at all times (cross-cut and high security models). High quality, hardened steel cutting shafts take staples, paper clips, credit cards, and CDs / DVDs (strip- and cross-cut models). High security models meet all NSA/CSS specifications and are DOD approved. Lifetime warranty on the cutting shafts (strip- and cross-cut models). 1 year warranty on high security cutting shafts. Quiet and powerful single phase motor rated for continuous operation. Sturdy Twin Drive System with fully enclosed gear box housing. High quality wooden cabinet mounted on casters. Convenient, environmentally friendly shred bin does not require disposable shred bags.\n\nShred volume, gallons: 26 \nFeed opening, inches: 10 1/4 \nElectrical requirements, volts: 115 \nMaximum horsepower: 1 \nDimensions (D x W x H), inches: 18 1/2 x 19 1/2 x 36 1/2 \nShipping weight, pounds: 123","2604 STRIP-CUT\nSecurity level\tP-2\nStrip width\t4 mm (3/16 inch)\nSheet capacity\t27-30*\nShred speed, ft./min.\t18\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $2,199\n\n2604 CROSS-CUT\nSecurity level\tP-4\nParticle size\t4 x 40 mm (3/16 x 1 1/2 inches)\nSheet capacity\t23-25*\nShred speed, ft./min.\t18\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $2,549\n\n2604 CROSS-CUT\nSecurity level\tP-5\nParticle size\t2 x 15 mm (3/32 x 5/8 inches)\nSheet capacity\t14-16*\nShred speed, ft./min.\t18\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $2,549\n\n2604 SMC HIGH SECURITY\nSecurity level\tP-7\nParticle size\t.8 x 5 mm (1/32 x 3/16 inches)\nSheet capacity\t6-8*\nShred speed, ft./min.\t28\nList Price US $2,699\n\n*Certified using 8 1/2\" x 11\" 20 pound bond and recommended power supply.",null,"https://www.mbmcorp.com/Paper-Shredders/Centralized-Office-Shredders/DESTROYIT-2604-118.html","https://www.youtube.com/watch?v=gqdkJFCTCdg",null,"Yes","Yes"]
[null,null,"DESTROYIT® 3104","Comprehensive SPS™ safety package: Easy Switch control element uses illuminated color codes and symbols to indicate operational status and functions as an emergency stop switch; patented, electronically controlled, transparent safety shield in the feed opening; automatic power cut-off when cabinet is opened or shred bin is full; automatic reverse and power cut-off when overfed; double protection against overheating; Zero Energy Consumption sleep mode cuts off power supply after 30 minutes of inactivity.\n\nAutomatic start and stop controlled by photo cell. Patented Electronic Capacity Control (ECC) indicator prevents jams by monitoring sheet capacity levels during operation. High quality, hardened steel cutting shafts take staples, paper clips, and credit cards (strip-cut and 4 x 40 cross-cut models take CDs / DVDs). Lifetime warranty on the cutting shafts. Quiet and powerful single phase motor rated for continuous operation. Sturdy Twin Drive System with fully enclosed gear box housing. High quality wooden cabinet mounted on casters. Convenient, environmentally friendly shred bin does not require disposable shred bags.\n\nShred volume, gallons: 32 \nFeed opening, inches: 12 \nElectrical requirements, volts: 115 \nMaximum horsepower: 1 \nDimensions (D x W x H), inches: 18 1/2 x 21 x 36 1/2 \nShipping weight, pounds: 132","3104 STRIP-CUT\nSecurity level\tP-2\nStrip width\t4 mm (3/16 inch)\nSheet capacity\t27-30*\nShred speed, ft./min.\t18\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $2,599\n\n3104 CROSS-CUT\nSecurity level\tP-4\nParticle size\t4 x 40 mm (3/16 x 1 1/2 inches)\nSheet capacity\t22-25*\nShred speed, ft./min.\t18\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $2,999\n\n3104 CROSS-CUT\nSecurity level\tP-5\nParticle size\t2 x 15 mm (3/32 x 5/8 inches)\nSheet capacity\t14-17*\nShred speed, ft./min.\t18\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlessly\nList Price US $2,999\n\n*Certified using 8 1/2\" x 11\" 20 pound bond and recommended power supply.",null,"https://www.mbmcorp.com/Paper-Shredders/Centralized-Office-Shredders/DESTROYIT-3104-119.html","https://www.youtube.com/watch?v=4lOKZHESERE",null,"Yes","Yes"]
[null,null,"DESTROYIT® 3105","Comprehensive SPS™ safety package: Easy Switch control element uses illuminated color codes and symbols to indicate operational status and functions as an emergency stop switch; patented, electronically controlled, transparent safety shield in the feed opening; automatic power cut-off when cabinet is opened or shred bin is full; automatic reverse and power cut-off when overfed; double protection against overheating; Zero Energy Consumption sleep mode cuts off power supply after 30 minutes of inactivity.\n\nAutomatic start and stop controlled by photo cell. Patented Electronic Capacity Control (ECC) indicator prevents jams by monitoring sheet capacity levels during operation. Automatic oil injection ensures optimal performance at all times. High quality, hardened steel cutting shafts take staples, paper clips, credit cards, and CDs / DVDs. Lifetime warranty on the cutting shafts. Quiet and powerful single phase motor rated for continuous operation. Sturdy chain drive with fully enclosed gear box housing. High quality wooden cabinet mounted on casters. Convenient, environmentally friendly shred bin does not require disposable shred bags.\n\nShred volume, gallons: 37 \nFeed opening, inches: 12 \nElectrical requirements, volts: 115 (20 amp. dedicated line required) \nMaximum horsepower: 2 1/8 \nDimensions (D x W x H), inches: 23 x 22 x 40 \nShipping weight, pounds: 324","3105 CROSS-CUT\nSecurity level\tP-4\nParticle size\t4 x 40 mm (3/16 x 1 1/2 inches)\nSheet capacity\t37-39*\nShred speed, ft./min.\t30\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $6,799\n3105 CROSS-CUT\nSecurity level\tP-5\nParticle size\t2 x 15 mm (3/32 x 5/8 inches)\nSheet capacity\t24-26*\nShred speed, ft./min.\t30\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $6,799",null,"https://www.mbmcorp.com/Paper-Shredders/Centralized-Office-Shredders/DESTROYIT-3105-120.html","https://www.youtube.com/watch?v=6R1bSSnjh14",null,"Yes","Yes"]
[null,null,"DESTROYIT® 3804","Comprehensive SPS™ safety package: Easy Switch control element uses illuminated color codes and symbols to indicate operational status and functions as an emergency stop switch; patented, electronically controlled, transparent safety shield in the feed opening; automatic power cut-off when cabinet is opened or shred bin is full; automatic reverse and power cut-off when overfed; double protection against overheating; Zero Energy Consumption sleep mode cuts off power supply after 30 minutes of inactivity.\n\nAutomatic start and stop controlled by photo cell. Patented Electronic Capacity Control (ECC) indicator prevents jams by monitoring sheet capacity levels during operation. High quality, hardened steel cutting shafts take staples, paper clips, and credit cards (strip-cut and 4 x 40 cross-cut models take CDs / DVDs). Lifetime warranty on the cutting shafts. Quiet and powerful single phase motor rated for continuous operation. Sturdy Twin Drive System with fully enclosed gear box housing. High quality wooden cabinet mounted on casters. Convenient, environmentally friendly shred bin does not require disposable shred bags.\n\nShred volume, gallons: 44 \nFeed opening, inches: 16 \nElectrical requirements, volts: 115 \nMaximum horsepower: 1 \nDimensions (D x W x H), inches: 23 1/4 x 25 1/4 x 38 1/4 \nShipping weight, pounds: 232 (strip-cut), 233 (cross-cut)","3804 STRIP-CUT\nSecurity level\tP-2\nStrip width\t6 mm (1/4 inch)\nSheet capacity\t29-31*\nShred speed, ft./min.\t20\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $3,349\n\n3804 CROSS-CUT\nSecurity level\tP-4\nParticle size\t4 x 40 mm (3/16 x 1 1/2 inches)\nSheet capacity\t24-26*\nShred speed, ft./min.\t20\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $3,749\n\n3804 CROSS-CUT\nSecurity level\tP-5\nParticle size\t2 x 15 mm (3/32 x 5/8 inches)\nSheet capacity\t12-14*\nShred speed, ft./min.\t20\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlessly\nList Price US $3,749\n\n*Certified using 8 1/2\" x 11\" 20 pound bond and recommended power supply.",null,"https://www.mbmcorp.com/Paper-Shredders/Centralized-Office-Shredders/DESTROYIT-3804-121.html",null,null,"Yes","Yes"]
[null,null,"DESTROYIT® 4002","Comprehensive SPS™ safety package: Easy Switch control element uses illuminated color codes and symbols to indicate operational status and functions as an emergency stop switch; patented, electronically controlled, transparent safety shield in the feed opening; automatic power cut-off when cabinet is opened or shred bin is full; automatic reverse and power cut-off when overfed; double protection against overheating; Zero Energy Consumption sleep mode cuts off power supply after 30 minutes of inactivity.\n\nAutomatic start and stop controlled by photo cell. Patented Electronic Capacity Control (ECC) indicator prevents jams by monitoring sheet capacity levels during operation. Automatic oil injection ensures optimal performance at all times (cross-cut models). High quality, hardened steel cutting shafts take staples, paper clips, credit cards, and CDs / DVDs. Lifetime warranty on the cutting shafts. Quiet and powerful single phase motor rated for continuous operation. Sturdy Twin Drive System with fully enclosed gear box housing. High quality wooden cabinet mounted on casters. Convenient, environmentally friendly shred bin does not require disposable shred bags.\n\nShred volume, gallons: 44\nFeed opening, inches: 16\nElectrical requirements, volts: 115\nMaximum horsepower: 1 3/4\nDimensions (D x W x H), inches: 23 1/4 x 25 1/4 x 38 1/4\nShipping weight, pounds: 239 (strip-cut), 240 (cross-cut)","4002 STRIP-CUT\nSecurity level\tP-2\nStrip width\t6 mm (1/4 inch)\nSheet capacity\t32-35*\nShred speed, ft./min.\t30\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $3,749\n4002 CROSS-CUT\nSecurity level\tP-4\nParticle size\t4 x 40 mm (3/16 x 1 1/2 inches)\nSheet capacity\t24-26*\nShred speed, ft./min.\t25\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $4,299\n4002 CROSS-CUT\nSecurity level\tP-5\nParticle size\t2 x 15 mm (3/32 x 5/8 inches)\nSheet capacity\t14-16*\nShred speed, ft./min.\t25\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $4,299*Certified using 8 1/2\" x 11\" 20 pound bond and recommended power supply.",null,"https://www.mbmcorp.com/Paper-Shredders/Centralized-Office-Shredders/DESTROYIT-4002-122.html","https://www.youtube.com/watch?v=r7YG3N4u8xk",null,"Yes","Yes"]
[null,null,"DESTROYIT® 4005","Comprehensive SPS™ safety package: Easy Switch control element uses illuminated color codes and symbols to indicate operational status and functions as an emergency stop switch; patented, electronically controlled, transparent safety shield in the feed opening; automatic power cut-off when cabinet is opened or shred bin is full; automatic reverse and power cut-off when overfed; double protection against overheating; Zero Energy Consumption sleep mode cuts off power supply after 30 minutes of inactivity.\n\nAutomatic start and stop controlled by photo cell. Patented Electronic Capacity Control (ECC) indicator prevents jams by monitoring sheet capacity levels during operation. Automatic oil injection ensures optimal performance at all times. High quality, hardened steel cutting shafts take staples, paper clips, credit cards, and CDs / DVDs (strip- and cross-cut models). High security models meet all NSA/CSS specifications and are DOD approved. Lifetime warranty on the cutting shafts (strip- and cross-cut models). 1 year warranty on high security cutting shafts. Quiet and powerful single phase motor rated for continuous operation. Sturdy chain drive with fully enclosed gear box housing. High quality wooden cabinet mounted on casters. Convenient, environmentally friendly shred bin does not require disposable shred bags.\n\nShred volume, gallons: 44 \nFeed opening, inches: 16 \nElectrical requirements, volts: 115 (20 amp. dedicated line required) \nMaximum horsepower: 2 1/8 \nDimensions (D x W x H), inches: 23 1/4 x 25 1/4 x 39 3/4 \nShipping weight, pounds: 343 (strip-cut), 378 (cross-cut), 390 (high security)","4005 STRIP-CUT\nSecurity level\tP-2\nStrip width\t6 mm (1/4 inch)\nSheet capacity\t50-52*\nShred speed, ft./min.\t40\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $6,949\n\n4005 CROSS-CUT\nSecurity level\tP-4\nParticle size\t4 x 40 mm (3/16 x 1 1/2 inches)\nSheet capacity\t37-39*\nShred speed, ft./min.\t30\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $7,999\n\n4005 CROSS-CUT\nSecurity level\tP-5\nParticle size\t2 x 15 mm (3/32 x 5/8 inches)\nSheet capacity\t24-26*\nShred speed, ft./min.\t30\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $7,999\n\nDESTROYIT 4005 SMC\nSecurity level\tP-7\nParticle size\t.8 x 5 mm (1/32 x 3/16 inches)\nSheet capacity\t10-12*\nShred speed, ft./min.\t44\nList Price US $5,499\n\n*Certified using 8 1/2\" x 11\" 20 pound bond and recommended power supply.",null,"https://www.mbmcorp.com/Paper-Shredders/Centralized-Office-Shredders/DESTROYIT-4005-123.html","https://www.youtube.com/watch?v=MKmRNNIsPtw",null,"Yes","Yes"]
[null,"High Capacity Shredders"]
[null,null,"DESTROYIT® 4605","Small footprint—ideal for limited space applications. Top loading feed hopper for bulky materials such as crumpled paper from wastebaskets. Main switch and emergency stop button. Automatic power cut-off when hopper or cabinet is opened or shred bag is full. Automatic reverse and power cut-off when overfed. Thermal switch prevents overheating. Special rotating paddles for positive feeding of bulky materials. Standard feed opening for flat paper with automatic start and stop controlled by photo cell. Fold-out feed table. Soft-touch control keys with optical indicators to show operational status. Soft metal resistant, hardened steel cutting shafts take CDs / DVDs and hardbound documents. High powered 3 phase motor rated for continuous operation. Fully enclosed gear box housing. Mounted on heavy duty casters. Front opening cabinet door and mobile shred bin for easy replacement of shred bags.\n\nShred volume, gallons: 61 \nFeed opening, inches: 18 \nElectrical requirements, volts: 220, 3 phase \nMaximum horsepower: 7 1/3 \nDimensions (D x W x H), inches: 30 x 29 x 67 \nShipping weight, pounds: 715","4605 CROSS-CUT\nSecurity level\tP-3\nParticle size\t4 x 60 mm (3/16 x 2 3/8 inches)\nSheet capacity\t50-60*\nShred speed, ft./min.\t40\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $14,699\n\n4605 CROSS-CUT\nSecurity level\tP-5\nParticle size\t2 x 15 mm (3/32 x 5/8 inches)\nSheet capacity\t32-37*\nShred speed, ft./min.\t40\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $14,699\n\n*Certified using 8 1/2\" x 11\" 20 pound bond and recommended power supply.",null,"https://www.mbmcorp.com/Paper-Shredders/High-Capacity-Shredders/DESTROYIT-4605-136.html","https://www.youtube.com/watch?v=IDOF9KvOY78",null,"Yes","Not Yet"]
[null,null,"DESTROYIT® 4107","Powered conveyor belt feed system. Convenient centralized oiler for lubrication of the cutting shafts. Safety lock and key, main switch, and emergency stop button. Automatic power cut-off when cabinet is opened or shred bag is full. Automatic reverse and power cut-off when overfed. Thermal switch prevents overheating. Removable side tables provide large work space. Push button control panel with optical indicators to show operational status. Soft metal resistant, hardened steel cutting shafts take CDs / DVDs and hardbound documents. High powered 3 phase motor rated for continuous operation. Fully enclosed gear box housing. Mounted on heavy duty casters. Rear opening cabinet door and mobile shred bag suspension frame for easy replacement of shred bags.\n\nShred volume, gallons: 79 \nFeed opening, inches: 16 \nElectrical requirements, volts: 220, 3 phase \nMaximum horsepower: 10 (strip-cut), 8 (cross-cut) \nDimensions (D x W x H), inches: 67 x 48 3/4 x 56 3/4 (27 W minus side tables) \nShipping weight, pounds: 952 (12 and 9 mm strip-cut), 994 (6 mm strip-cut), 983 (cross-cut)","4107 STRIP-CUT\nSecurity level\tP-2\nStrip width\t12 mm (1/2 inch)\nSheet capacity\t120-140*\nShred speed, ft./min.\t60\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $13,999\n4107 STRIP-CUT\nSecurity level\tP-2\nStrip width\t9 mm (3/8 inch)\nSheet capacity\t105-125*\nShred speed, ft./min.\t60\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $13,999\n4107 STRIP-CUT\nSecurity level\tP-2\nStrip width\t6 mm (1/4 inch)\nSheet capacity\t75-95*\nShred speed, ft./min.\t60\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $13,999\n4107 CROSS-CUT\nSecurity level\tP-3\nParticle size\t6 x 50 mm (1/4 x 2 inches)\nSheet capacity\t65-82*\nShred speed, ft./min.\t53\nShred capabilities (non-paper)\tShreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US $15,999",null,"https://www.mbmcorp.com/Paper-Shredders/High-Capacity-Shredders/DESTROYIT-4107-137.html","https://www.youtube.com/watch?v=kWmov1iiq30",null,"Yes","Yes"]
[null,null,"DESTROYIT® 5009","Extra large feed table with powered conveyor belt feed system. Convenient centralized oiler for lubrication of the cutting shafts. Electronically controlled safety guard. Safety lock and key, main switch, and emergency stop button. Automatic power cut-off when cabinet is opened or shred bag is full. Automatic reverse and power cut-off when overfed. Thermal switch prevents overheating. Push button control panel with optical indicators to show operational status. 2 automatic speed modes: POWER for bulk feeding large quantities of paper and SPEED for high speed shredding of lesser amounts. Soft metal resistant, hardened steel cutting shafts take CDs / DVDs, hardbound documents, and 3-ring binders. Dual 3 phase motors (24 maximum horsepower) rated for continuous operation. Fully enclosed gear box housing. Mounted on heavy duty casters. Rear opening cabinet door and mobile shred bin with bag mounting frame for easy replacement of shred bags. Optional accessories: modular exit conveyor belt system and additional shred bins.\n\nShred volume, gallons: 79 \nFeed opening, inches: 20 \nElectrical requirements, volts: 220, 3 phase (50 amp. dedicated line required) \nMaximum horsepower: 24 \nDimensions (D x W x H), inches: 85 1/2 x 40 3/4 x 67 1/2 (121 D with modular exit conveyor belt system) \nShipping weight, pounds: 3,080","5009 CROSS-CUT\nSecurity level        P-2\nParticle size        8 x 40-80 mm (11/32 x 1 1/2–3 inches)\nSheet capacity        600-700*\nShred speed, ft./min.        24-46 (2 automatic speed modes)\nShred capabilities (non-paper)        Shreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US P-2: $37,999\n\n5009 CROSS-CUT\nSecurity level        P-3\nParticle size        6 x 50 mm (1/4 x 2 inches)\nSheet capacity        300-400*\nShred speed, ft./min.        24-45 (2 automatic speed modes)\nShred capabilities (non-paper)        Shreds paper clips and staples effortlesslyShreds credit cards effortlesslyShreds CDs and DVDs effortlessly\nList Price US P-3: $41,999\n\n*Certified using 8 1/2\" x 11\" 20 pound bond and recommended power supply.",null,"https://www.mbmcorp.com/Paper-Shredders/High-Capacity-Shredders/DESTROYIT-5009-138.html","https://www.youtube.com/watch?v=MJ_715Vgjtw",null,"Yes","Yes"]
[null,"High Security Shredders"]
[null,null,"2445 SMC HIGH SECURITY","Comprehensive SPS™ safety package: Easy Switch control element uses illuminated color icons and symbols to indicate operational status and functions as an emergency stop switch; patented, electronically controlled, transparent safety shield in the feed opening; automatic power cut-off when cabinet is opened or shred bin is full; automatic reverse and power cut-off when overfed; double protection against overheating; Zero Energy Consumption sleep mode cuts off power supply after 30 minutes of inactivity.\n\nAutomatic start and stop controlled by photo cell. High quality, hardened steel cutting shafts. Meets all NSA/CSS specifications and is DOD approved. 1 year warranty on the cutting shafts. Quiet and powerful single phase motor. Fully enclosed gear box housing. High quality wooden cabinet mounted on casters. Convenient, environmentally friendly shred bin does not require disposable shred bags.\n\nShred volume, gallons: 9 \nFeed opening, inches: 9 1/2 \nElectrical requirements, volts: 115 \nMaximum horsepower: 1/2 \nDimensions (D x W x H), inches: 11 3/4 x 15 1/2 x 28 3/4 \nShipping weight, pounds: 53","2445 SMC HIGH SECURITY\nSecurity level\tP-7\nParticle size\t.8 x 5 mm\nSheet capacity\t5-7*\nShred speed, ft./min.\t14\nCall for Pricing\n\n*Certified using 8 1/2\" x 11\" 20 pound bond and recommended power supply.",null,"https://www.mbmcorp.com/Paper-Shredders/High-Security-Shredders/2445-SMC-HIGH-SECURITY-401.html",null,null,"Yes","Yes"]
[null,null,"2604 SMC HIGH SECURITY","Comprehensive SPS™ safety package: Easy Switch control element uses illuminated color codes and symbols to indicate operational status and functions as an emergency stop switch; patented, electronically controlled, transparent safety shield in the feed opening; automatic power cut-off when cabinet is opened or shred bin is full; automatic reverse and power cut-off when overfed; double protection against overheating; Zero Energy Consumption sleep mode cuts off power supply after 30 minutes of inactivity.\n\nAutomatic start and stop controlled by photo cell. Patented Electronic Capacity Control (ECC) indicator prevents jams by monitoring sheet capacity levels during operation. Automatic oil injection ensures optimal performance at all times. High quality, hardened steel cutting shafts. Meets all NSA/CSS specifications and is DOD approved. 1 year warranty on the cutting shafts. Quiet and powerful single phase motor rated for continuous operation. Sturdy Twin Drive System with fully enclosed gear box housing. High quality wooden cabinet mounted on casters. Convenient, environmentally friendly shred bin does not require disposable shred bags.\n\nShred volume, gallons: 26 \nFeed opening, inches: 10 1/4 \nElectrical requirements, volts: 115 \nMaximum horsepower: 1 \nDimensions (D x W x H), inches: 18 1/2 x 19 1/2 x 36 1/2 \nShipping weight, pounds: 123","2604 SMC HIGH SECURITY\nSecurity level\tP-7\nParticle size\t.8 x 5 mm (1/32 x 3/16 inches)\nSheet capacity\t6-8*\nShred speed, ft./min.\t28\nList Price US $2,699\n\n*Certified using 8 1/2\" x 11\" 20 pound bond and recommended power supply.",null,"https://www.mbmcorp.com/Paper-Shredders/High-Security-Shredders/2604-SMC-HIGH-SECURITY-142.html","https://www.youtube.com/watch?v=gqdkJFCTCdg",null,"Yes","Yes"]
[null,null,"4005 SMC HIGH SECURITY","Comprehensive SPS™ safety package: Easy Switch control element uses illuminated color codes and symbols to indicate operational status and functions as an emergency stop switch; patented, electronically controlled, transparent safety shield in the feed opening; automatic power cut-off when cabinet is opened or shred bin is full; automatic reverse and power cut-off when overfed; double protection against overheating; Zero Energy Consumption sleep mode cuts off power supply after 30 minutes of inactivity.\n\nAutomatic start and stop controlled by photo cell. Patented Electronic Capacity Control (ECC) indicator prevents jams by monitoring sheet capacity levels during operation. Automatic oil injection ensures optimal performance at all times. High quality, hardened steel cutting shafts. Meets all NSA/CSS specifications and is DOD approved. 1 year warranty on the cutting shafts. Quiet and powerful single phase motor rated for continuous operation. Sturdy chain drive with fully enclosed gear box housing. High quality wooden cabinet mounted on casters. Convenient, environmentally friendly shred bin does not require disposable shred bags.\n\nShred volume, gallons: 44 \nFeed opening, inches: 16 \nElectrical requirements, volts: 115 (20 amp. dedicated line required) \nMaximum horsepower: 2 1/8 \nDimensions (D x W x H), inches: 23 1/4 x 25 1/4 x 39 3/4 \nShipping weight, pounds: 390","4005 SMC\nSecurity level\tP-7\nParticle size\t.8 x 5 mm (1/32 x 3/16 inches)\nSheet capacity\t10-12*\nShred speed, ft./min.\t44\nList Price US $5,499\n\n*Certified using 8 1/2\" x 11\" 20 pound bond and recommended power supply.",null,"https://www.mbmcorp.com/Paper-Shredders/High-Security-Shredders/4005-SMC-HIGH-SECURITY-144.html","https://www.youtube.com/watch?v=MKmRNNIsPtw",null,"Yes","Yes"]
[null,"Special Solutions"]
[null,null,"DESTROYIT 0101 HDP HARD DRIVE PUNCH","Comprehensive SPS safety package: Easy Switch control element uses illuminated color codes and symbols to indicate operational status and functions as an emergency stop switch; electronically controlled, transparent safety shield in the feed opening; automatic stop after punching; automatic power cut-off when cabinet is opened or collection bin is full; double protection against overheating.\n\nPunches a hole completely through the hard drive, making it unreadable. Suitable for 2 1⁄2 and 3 1⁄2 inch drives (single feed). Handy slide lever for easy selection of hard drive size. Adjustable feed chute made of high quality steel. LEDs illuminate feed chute during punching process. Punching die made of hardened, nickel-plated steel. Automatic reverse on punching die prevents jams. Slider mechanism for unloading punching compartment—destroyed drives drop into a sturdy collection bin to await proper disposal. Quiet and powerful single phase motor rated for continuous operation. Sturdy Twin Drive System with fully enclosed gear box housing. High quality wooden cabinet mounted on casters. Anti-static collection bin made of impact-resistant plastic. 1 year warranty on all parts, excluding wearables.\n\n\nDimensions (D x W x H), inches: 18 1/2 x 19 1/2 x 33 1/2 \nShipping weight, pounds: 208","DESTROYIT 0101 HDP\nSecurity level:\tH-3\nHard drive sizes, inches:\t2 1/2 or 3 1/2\nPunching cycle, seconds:\t15\nCollection bin volume:\tweight sensor\nElectrical requirements, volts:\t115\nMaximum horsepower:\t1\nList Price US $5,499.00",null,"https://www.mbmcorp.com/Paper-Shredders/Special-Solutions/DESTROYIT-0101-HDP-HARD-DRIVE-PUNCH-151.html",null,null,"Yes","Yes"]
[null,null,"DESTROYIT DEGAUSSER / HDP","Comprehensive SPS safety package (HDP unit): Easy Switch control element uses illuminated color codes and symbols to indicate operational status and functions as an emergency stop switch; electronically controlled, transparent safety shield in the feed opening; automatic stop after punching; automatic power cut-off when cabinet is opened or collection bin is full; double protection against overheating.\n\nHDP unit: Punches a hole completely through the hard drive, making it unreadable. Suitable for 2 1⁄2 and 3 1⁄2 inch drives (single feed). Handy slide lever for easy selection of hard drive size. Adjustable feed chute made of high quality steel. LEDs illuminate feed chute during punching process. Punching die made of hardened, nickel-plated steel. Automatic reverse on punching die prevents jams. Slider mechanism for unloading punching compartment— destroyed drives drop into a sturdy collection bin to await proper disposal. Quiet and powerful single phase motor rated for continuous operation. Sturdy Twin Drive System with fully enclosed gear box housing.\n\nDegausser unit: Erases hard drives (laptop, desktop, and network up to 1 1⁄2 inches high) and high coercivity tape media, including all formats of LTO, Super DLT I and II, AIT, 3590 Series, 8 mm and more. Fast, 60 second cycle time. High field strength and encompassing magnetic field ensure data is completely erased and non-recoverable, regardless of operating system or interface. Digital status indicator and field strength verification. No moving parts allow for extremely quiet operation. Rated for continuous operation (no cooling necessary).\n\nHigh quality wooden cabinet mounted on casters. Anti-static collection bin made of impact-resistant plastic. 1 year warranty on all parts, excluding wearables.\n\nSecurity level: H-3 (HDP unit) \nHard drive sizes, inches: 2 1/2 or 3 1/2 \nErasing area (H x W x D), inches: 1 1/2 x 4 1/4 x 6 \nDegaussing cycle, seconds: 60 \nDegaussing system: capacitive discharge \nDegausser magnetic field: 8,700 Oe / .87 Tesla \nPunching cycle, seconds: 15 \nCollection bin volume: weight sensor (automatic cut-off when collection bin is full) \nElectrical requirements, volts: 115 \nMaximum horsepower (HDP): 1 \nDimensions (D x W x H), inches: 18 1/2 x 19 1/2 x 33 1/2 \nShipping weight, pounds: 247",null,null,"https://www.mbmcorp.com/Paper-Shredders/Special-Solutions/DESTROYIT-DEGAUSSER-HDP-152.html",null,null,"Yes","Yes"]
[null,null,"HARD DRIVE DEGAUSSER","Erases hard drives (laptop, desktop, and network up to 1 1⁄2 inches high) and high coercivity tape media, including all formats of LTO, Super DLT I and II, AIT, 3590 Series, 8 mm and more. Fast, 60 second cycle time. High field strength and encompassing magnetic field ensure data is completely erased and non-recoverable, regardless of operating system or interface. Digital status indicator and field strength verification. No moving parts allow for extremely quiet operation. Rated for continuous operation (no cooling necessary). 1 year warranty.\n\nHard drive sizes, inches: 2 1/2 or 3 1/2 \nErasing area (H x W x D), inches: 1 1/2 x 4 1/4 x 6 \nDegaussing cycle, seconds: 60 \nDegaussing system: capacitive discharge \nDegausser magnetic field: 8,700 Oe / .87 Tesla \nPunching cycle, seconds: 15 \nElectrical requirements, volts: 115 \nDimensions (D x W x H), inches: 13 1/4 x 6 x 17 1/4 \nShipping weight, pounds: 40",null,null,"https://www.mbmcorp.com/Paper-Shredders/Special-Solutions/HARD-DRIVE-DEGAUSSER-153.html",null,null,"Yes","Yes"]
[null,null,"DESTROYIT HARD DRIVE SHREDDER","Specially designed for office environments. Destroys up to 8 standard size hard drives per minute. Produces a 38 mm particle width. Integrated HEPA filter. Automatic reverse feature prevents jams. Safety feed chute keeps the operator's hands away from the cutting chamber and prevents particle \"fly-back.\" Automatic power cut-off when collection bin is full or when cabinet door is opened. Quiet operation. Mounted on heavy duty casters. 1 year warranty on all parts, excluding wearables.\n\nSecurity level: 0-5 \nParticle size: 38 mm (1 1/2 inches) x random \nMaximum drive thickness, inches: 1 \nFeed opening, inches: 5.2 x 1.5 \nPerformance (approx.), pieces per hour: 500 \nShred volume, pounds: 20 \nElectrical requirements, volts: 120 (20 amp. dedicated line required) \nMaximum horsepower: 1 \nDimensions (D x W x H), inches: 21 x 45 x 46 \nShipping weight, pounds: 875",null,null,"https://www.mbmcorp.com/Paper-Shredders/Special-Solutions/DESTROYIT-HARD-DRIVE-SHREDDER-155.html",null,null,"Yes","Yes"]
[null,"Shredder Accessories"]
[null,null,"AUTO OILER FOR CENTRALIZED MODELS","The cutting shafts are automatically lubricated while shredding, ensuring optimal performance for Destroyit® 3104 & Destroyit® 3804 cross-cut models.","Optional for 3104 & 3804 models (installed)\n\nList Price US $999.00",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Accessories/AUTO-OILER-FOR-CENTRALIZED-MODELS-172.html",null,null,"Yes","Yes"]
[null,null,"AUTO OILER FOR HIGH CAPACITY MODELS","The cutting shafts are automatically lubricated while shredding, ensuring optimal performance for Destroyit® 4107 and Destroyit® 5009 cross-cut models.","High Capacity models\n\nList Price US $1,149.00",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Accessories/AUTO-OILER-FOR-HIGH-CAPACITY-MODELS-173.html",null,null,"Yes","Yes"]
[null,null,"COLLECTION CONSOLE","Lockable collection console for the collection and storage of medium to large amounts of confidential documents for in-house shredding.","Self-locking cabinet door with tamper proof lock guard. Internal paper deflector prevents phishing. Multiple consoles can be accessed with a single key. High quality wooden cabinet. Convenient, environmentally friendly collection bin does not require disposable shred bags.\n\nCollection bin volume, gallons: 17 \nDimensions (D x W x H), inches: 16 x 21 1/2 x 36 \nShipping weight, pounds: 60\n\nList Price US $229.00",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Accessories/COLLECTION-CONSOLE-174.html",null,null,"Yes","Yes"]
[null,null,"MODULAR CONVEYOR BELT SYSTEM","Optional accessory transports shredded material to an external container.","Eliminates need to change shred bags. Easy to install—simply roll into place, close door, and lock. Electric belt drive is controlled by the shredder electronics. Electrically secured locking system. Mounted on heavy duty casters.\n\nSpeed, ft./min.: 35\nFeed opening (W x H), inches: 13 3/4 x 4\nDimensions (D x W x H), inches: 74 x 27 1/4 x 45 3/4\nShipping weight, pounds: 359\n\nRestricted product for Destroyit® 5009 High Capacity\n\nList Price US $5,999.00",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Accessories/MODULAR-CONVEYOR-BELT-SYSTEM-175.html",null,null,"Yes","Yes"]
[null,null,"SHRED COLLECTION CART FOR 5009","79 gallon shred bin is mounted on heavy duty casters for easy mobility. Shredder stops automatically when door is opened.","5009\n\nList Price US $1,599.00",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Accessories/SHRED-COLLECTION-CART-FOR-5009-176.html",null,null,"Yes","Yes"]
[null,null,"COLLECTION CART","Lockable, 95 gallon mobile cart for the collection and storage of large amounts of confidential documents for in-house shredding.","Dual locking system (internal and external hasp) ensures complete security. Deflector in feed slot prevents tampering. Multiple carts can be accessed with a single key. 12 inch rubber wheels and heavy duty axle for ease of movement, even when filled to capacity. Super strong, high density plastic construction. Environmentally friendly—does not require disposable shred bags. 5 year warranty on internal locking system\n\nVolume, gallons: 95 \nDimensions (D x W x H), inches: 34 x 24 x 44 1/4 \nShipping weight, pounds: 56\n\nList Price US $229.00",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Accessories/COLLECTION-CART-177.html",null,null,"Yes","Yes"]
[null,"Shredder Supplies"]
[null,null,"901 SHRED BAGS","Quantity: 1 case \nThickness: .002 mm \nCapacity: 56 gallons \nDimensions (W x H): 54\" x 48\" \nShipping weight: 37 lbs.","4000ss, 4002, 4202\n\nList Price US $159.00",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Supplies/901-SHRED-BAGS-157.html",null,null,"Yes","Not Yet"]
[null,null,"902 SHRED BAGS","Quantity: 1 case \nThickness: .002 mm \nCapacity: 25 gallons \nDimensions (W x H): 30\" x 38\" \nShipping weight: 18 lbs. ","2501, 2600, 2601, 3801\n\nList Price US $135.00",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Supplies/902-SHRED-BAGS-158.html",null,null,"Yes","Not Yet"]
[null,null,"907 SHRED BAGS","Quantity: 1 case \nThickness: .001 mm \nCapacity: 7 gallons \nDimensions (W x H): 23\" x 24\" \nShipping weight: 10 lbs. ","1000, 2000, 2100, 2200, 2201, 2230, 2240, 2245, 2250, 2260, 2265, 2270, 2350, 2400, 2401, 3000\n\nList Price US $99.00",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Supplies/907-SHRED-BAGS-159.html",null,null,"Yes","Not Yet"]
[null,null,"908 SHRED BAGS","Quantity: 1 case \nThickness: .001 mm \nCapacity: 12 gallons \nDimensions (W x H): 24\" x 30\" \nShipping weight: 13 lbs.","2360, 2401L, 2402, 2403, 2404\n\nList Price US $95.00",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Supplies/908-SHRED-BAGS-160.html",null,null,"Yes","Not Yet"]
[null,null,"914 SHRED BAGS","Quantity: 1 case \nThickness: .002 mm \nCapacity: 60 gallons \nDimensions (W x H): 36\" x 75\" \nShipping weight: 40 lbs. ","4104, 4105 strip-cut\n\nList Price US $219.00",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Supplies/914-SHRED-BAGS-161.html",null,null,"Yes","Not Yet"]
[null,null,"915 SHRED BAGS","Quantity: 1 case \nThickness: .004 mm \nCapacity: 65 gallons \nDimensions (W x H): 52\" x 58\" \nShipping weight: 38 lbs. ","4105 cross-cut, 4106\n\nList Price US $219.00",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Supplies/915-SHRED-BAGS-162.html",null,null,"Yes","Not Yet"]
[null,null,"917 SHRED BAGS","Quantity: 1 case \nThickness: .002 mm \nCapacity: 31 gallons \nDimensions (W x H): 35\" x 38\" \nShipping weight: 21 lbs.","3800, 3802, 4001, 4203\n\nList Price US $139.00",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Supplies/917-SHRED-BAGS-163.html",null,null,"Yes","Not Yet"]
[null,null,"918 SHRED BAGS","Quantity: 1 case \nThickness: .002 mm \nCapacity: 44 gallons \nDimensions (W x H): 40\" x 48\" \nShipping weight: 28 lbs. ","3105, 3803, 3804, 4000, 4003, 4004, 4005, 4011, 4012\n\nList Price US $149.00",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Supplies/918-SHRED-BAGS-164.html",null,null,"Yes","Not Yet"]
[null,null,"919 EXTRA LARGE SHRED BAGS","Quantity: 1 case \nThickness: .002 mm \nCapacity: 88 gallons \nDimensions (W x H): 54\" x 75\" \nShipping weight: 58 lbs. ","4000ss\n\nList Price US $249.00",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Supplies/919-EXTRA-LARGE-SHRED-BAGS-165.html",null,null,"Yes","Not Yet"]
[null,null,"920 SHRED BAGS","Quantity: 1 case \nThickness: .002 mm \nCapacity: 40 gallons \nDimensions (W x H): 33\" x 47\" \nShipping weight: 23 lbs. ","2502, 2503, 2602, 2603, 2604, 3102, 3103, 3104\n\nList Price US $149.00",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Supplies/920-SHRED-BAGS-166.html",null,null,"Yes","Not Yet"]
[null,null,"921 SHRED BAGS","Quantity: 1 case \nThickness: .002 mm \nCapacity: 61 gallons \nDimensions (W x H): 47\" x 52\" \nShipping weight: 24 lbs. ","4605\n\nList Price US $249.00\n",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Supplies/921-SHRED-BAGS-167.html",null,null,"Yes","Not Yet"]
[null,null,"922 SHRED BAGS","922 SHRED BAGS\nQuantity: 1 case \nThickness: .002 mm \nCapacity: 79 gallons \nDimensions (W x H): 44\" x 64\" \nShipping weight: 52 lbs. ","4107, 4109\n\nList Price US $259.00\n",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Supplies/922-SHRED-BAGS-168.html",null,null,"Yes","Not Yet"]
[null,null,"923 SHRED BAGS (OLD STYLE)","Quantity: 1 case \nThickness: .004 mm \nCapacity: 75 gallons \nDimensions (W x H): 42\" x 56\" \nShipping weight: 28 lbs. ","5009\n\nList Price US $209.00\n",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Supplies/923-SHRED-BAGS-OLD-STYLE-169.html",null,null,"Yes","Not Yet"]
[null,null,"924 SHRED BAGS (NEW STYLE)","Quantity: 1 case \nThickness: .004 mm \nCapacity: 79 gallons \nDimensions (W x H): 40\" x 58\" \nShipping weight: 36 lbs. ","5009\n\nList Price US $229.00\n",null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Supplies/924-SHRED-BAGS-NEW-STYLE-170.html",null,null,"Yes","Not Yet"]
[null,null,"DESTROYIT® SPECIAL FORMULA SHREDDER OIL","MBM® shredder oil is a specially blended, high cling, non-detergent oil formulated for use in Destroyit® shredders. It is recommended that shredding wheels be oiled for every 30 minutes of operation for cross-cut shredders and for every hour of operation for strip-cut models.\n\nLIST PRICE (US)\n• 4 bottles, 1 pint each $59 \n• 8 bottles, 1 pint each $89\n• 6 bottles, 1 quart each $109\n• 4 bottles, 1 gallon each $189\n\nLIST PRICE (CAN)\n• 4 bottles, 1 pint each $79 \n• 6 bottles, 1 quart each $149 \n• 4 bottles, 1 gallon each $259 ",null,null,"https://www.mbmcorp.com/Paper-Shredders/Shredder-Supplies/DESTROYIT-SPECIAL-FORMULA-SHREDDER-OIL-171.html",null,null,"Yes","Not Yet"]
["Finishing","Triumph™ Cutters"]
[null,null,"TRIUMPH™ 4300","SCS™ safety features: hinged, transparent safety guard on front table with locking device for the blade lever (a cut can only be executed if the safety guard is completely closed); transparent safety cover on rear table; blade changing device covers cutting edge of blade; blade depth adjustment from outside of machine; blade and cutting stick can be changed without removing covers; safety blade lever with patented overload protection.\n\nPatented, lever-activated, fast-action clamp. Lockable back gauge. Precision side guide with measurement scale (mm / inches). High quality, German steel blade. All-metal construction. Optional stand, or cabinet with storage shelves. UL and C UL approved.\n\nDimensions (D x W x H), inches: 22 1/2 x 28 x 18 1/2 (47 1/2 H with stand, 46 3/4 H with cabinet)\nShipping weight, pounds: 95 (121 with stand, 190 with cabinet)","TRIUMPH 4300\nCutting width, inches 16 7/8\nCutting height, inches 3/4\nNarrow cut, inches 1 1/2\nLength behind blade, inches13 3/8\nList Price US $999",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Cutters/TRIUMPH-4300-215.html","https://www.youtube.com/watch?v=oEm4bR0Hj2M",null,"Yes","Yes"]
[null,null,"TRIUMPH™ 4305","SCS™ safety features: hinged, transparent safety guard on front table (locks automatically while cutting); transparent safety cover on rear table; safety catch (locks blade lever in up position); blade changing device covers cutting edge of blade; blade depth adjustment from outside of machine; blade and cutting stick can be changed without removing covers.\n\nSpindle-guided back gauge with calibrated crank and measurement scale. Patented, lever-activated, fast-action clamp. Precision side guide with measurement scale (mm / inches). High quality, German steel blade. Solid steel blade carrier and adjustable blade guides. All-metal construction. Optional stand (shown above), or cabinet with storage shelves. UL and C UL approved.\n\nDimensions (D x W x H), inches: 34 5/8 x 34 5/8 x 15 3/4 (45 1/4 H with stand, 44 H with cabinet)\nShipping weight, pounds: 115 (141 with stand, 210 with cabinet)","TRIUMPH 4305\nCutting width, inches 16 7/8\nCutting height, inches 1 1/2\nNarrow cut, inches 1 5/16\nLength behind blade, inches17\nList Price US $1,799",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Cutters/TRIUMPH-4305-216.html","https://www.youtube.com/watch?v=oEm4bR0Hj2M",null,"Yes","Yes"]
[null,null,"TRIUMPH™ 4705","SCS™ safety features: hinged, transparent safety guard on front table (locks automatically while cutting); transparent safety cover on rear table; safety catch (locks blade lever in up position); blade changing device covers cutting edge of blade; blade depth adjustment from outside of machine; blade and cutting stick can be changed without removing covers. \n\nSpindle-guided back gauge with calibrated crank. Manual spindle clamp is guided on both sides to apply even pressure along entire cutting width. Front table measurement scale (mm / inches). High quality, German steel blade. Solid steel blade carrier and adjustable blade guides. All-metal construction. Optional stand (shown above). UL and C UL approved.\n\nDimensions (D x W x H), inches: 35 x 39 x 23 (50 H with stand)\nShipping weight, pounds: 297 (320 with stand)","TRIUMPH 4705\nCutting width, inches 18 3/4\nCutting height, inches 2 3/4\nNarrow cut, inches 1 3/16\nLength behind blade, inches18\nList Price US $3,299",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Cutters/TRIUMPH-4705-217.html","https://www.youtube.com/watch?v=oEm4bR0Hj2M",null,"Yes","Yes"]
[null,null,"TRIUMPH™ 4315","Comprehensive SCS™ safety package: patented EASY CUT electronic blade activation bars for true two-hand operation; transparent, electronically controlled front safety guard; transparent safety cover on rear table; main switch and safety lock with key; 24 volt controls (low voltage); patented IDEAL safety drive; automatic blade return from every position; disc brake for instant blade stop; blade changing device covers cutting edge of blade; blade depth adjustment from outside of machine; blade and cutting stick can be changed without removing covers.\n\nElectric blade drive. Spindle-guided back gauge with calibrated crank. Front table digital display (cm or inches) for precise back gauge positioning. Bright, LED optical cutting line. Patented lever-activated, fast-action clamp. Precision side guide. High quality, German steel blade. Solid steel blade carrier and adjustable blade guides. All-metal construction. Optional stand (shown above), or cabinet with storage shelves. UL and C UL approved.\n\nElectrical requirements: 115 V, 60 Hz\nMotor output, horsepower: 0.6\nDimensions (D x W x H), inches: 34 1/4 x 25 x 14 (42 3/4 H with stand, 42 1/2 H with cabinet)\nShipping weight, pounds: 191 (217 with stand, 286 with cabinet)","TRIUMPH 4315\nCutting width, inches 16 7/8\nCutting height, inches 1 1/2\nNarrow cut, inches 1 3/8\nLength behind blade, inches17\nList Price US $4,199",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Cutters/TRIUMPH-4315-218.html","https://www.youtube.com/watch?v=Rl6O3E_CjBk",null,"Yes","Yes"]
[null,null,"TRIUMPH™ 4350","Comprehensive SCS™ safety package: patented EASY CUT electronic blade activation bars for true two-hand operation; transparent, electronically controlled front safety guard; transparent safety cover on rear table; main switch and safety lock with key; 24 volt controls (low voltage); patented IDEAL safety drive; automatic blade and clamp return from every position; disc brake for instant blade stop; blade changing device covers cutting edge of blade; blade depth adjustment from outside of machine; blade and cutting stick can be changed without removing covers.\n\nElectric blade and clamp drive. Spindle-guided back gauge with calibrated crank. Front table digital display (cm or inches) for precise back gauge positioning. Bright, LED optical cutting line. Patented automatic clamp. Precision side guide. High quality, German steel blade. Solid steel blade carrier and adjustable blade guides. All-metal construction. Optional stand (shown above), or cabinet with storage shelves. UL and C UL approved.\n\nElectrical requirements: 115 V, 60 Hz\nMotor output, horsepower: 0.6\nDimensions (D x W x H), inches: 34 1/4 x 25 x 14 (42 3/4 H with stand, 42 1/2 H with cabinet)\nShipping weight, pounds: 200 (226 with stand, 295 with cabinet)","TRIUMPH 4350\nCutting width, inches 16 7/8\nCutting height, inches 1 1/2\nNarrow cut, inches 1 3/8\nLength behind blade, inches17\nList Price US $4,999",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Cutters/TRIUMPH-4350-219.html","https://www.youtube.com/watch?v=bExfgNqyHBE",null,"Yes","Yes"]
[null,null,"TRIUMPH™ 4815","Comprehensive SCS™ safety package: patented EASY CUT electronic blade activation bars for true two-hand operation; transparent, electronically controlled front safety guard; safety cover on rear table; main switch and safety lock with key; 24 volt controls (low voltage); patented IDEAL safety drive; automatic blade return from every position; disc brake for instant blade stop; blade changing device covers cutting edge of blade; blade depth adjustment from outside of machine; blade and cutting stick can be changed without removing covers.\n\nErgonomic, 37 inch working height. Electric blade drive. Spindle-guided back gauge with calibrated crank. Front table digital display (cm or inches) for precise back gauge positioning. Bright, LED optical cutting line. Adjustable back gauge with narrow separations and plastic gliders. Manual spindle clamp is guided on both sides to apply even pressure along entire cutting width. Dual side guides on front and rear tables. High quality, German steel blade. Solid steel blade carrier and adjustable blade guides. All-metal construction. Includes stand with storage shelf, easy-access tool holder, and paper blocking tool. Optional side tables increase work surface. UL and C UL approved.\n\nElectrical requirements: 115 V, 60 Hz\nMotor output, horsepower: 1.5\nDimensions (D x W x H), inches: 41 1/2 x 30 x 55 1/2 (53 W with side tables)\nShipping weight, pounds: 531 (552 with side tables)","TRIUMPH 4815\nCutting width, inches 18 5/8\nCutting height, inches 3\nNarrow cut, inches 1\nLength behind blade, inches18\nList Price US $7,399",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Cutters/TRIUMPH-4815-221.html","https://www.youtube.com/watch?v=Rl6O3E_CjBk",null,"Yes","Yes"]
[null,null,"TRIUMPH™ 4850","Comprehensive SCS™ safety package: patented EASY CUT electronic blade activation bars for true two-hand operation; transparent, electronically controlled front safety guard; safety cover on rear table; main switch and safety lock with key; 24 volt controls (low voltage); patented IDEAL safety drive; automatic blade and clamp return from every position; disc brake for instant blade stop; blade changing device covers cutting edge of blade; blade depth adjustment from outside of machine; blade and cutting stick can be changed without removing covers.\n\nErgonomic, 37 inch working height. Electric blade and clamp drive. Spindle-guided back gauge with calibrated crank. Front table digital display (cm or inches) for precise back gauge positioning. Bright, LED optical cutting line. Adjustable back gauge with narrow separations and plastic gliders. Automatic clamp. Dual side guides on front and rear tables. High quality, German steel blade. Solid steel blade carrier and adjustable blade guides. All-metal construction. Includes stand with storage shelf, easy-access tool holder, and paper blocking tool. Optional side tables increase work surface. UL and C UL approved.\n\nElectrical requirements: 115 V, 60 Hz (20 amp dedicated line required)\nMotor output, horsepower: 2\nDimensions (D x W x H), inches: 41 1/2 x 30 x 51 (53 W with side tables)\nShipping weight, pounds: 556 (577 with side tables)","TRIUMPH 4850\nCutting width, inches 18 5/8\nCutting height, inches 3\nNarrow cut, inches 1\nLength behind blade, inches18\nList Price US $8,999",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Cutters/TRIUMPH-4850-222.html","https://www.youtube.com/watch?v=bExfgNqyHBE",null,"Yes","Yes"]
[null,null,"TRIUMPH™ 5255","Comprehensive SCS™ safety package: patented EASY CUT electronic blade activation bars for true two-hand operation; transparent, electronically controlled front safety guard; safety cover on rear table; main switch and safety lock with key; 24 volt controls (low voltage); patented IDEAL safety drive; automatic blade and clamp return from every position; disc brake for instant blade stop; blade changing device covers cutting edge of blade; blade depth adjustment from outside of machine; blade and cutting stick can be changed without removing covers.\n\nErgonomic, 37 inch working height. Electric blade and clamp drive. Electric back gauge drive with touchpad for easy programming. Digital measurement display (cm or inches) with multilingual operator guidance, accurate to 1/10 mm or 1/100 inch. Stores 99 programs with up to 99 steps in each (up to 15 repeat cuts can be integrated as a single step). Pre-programmed for standard paper sizes. Memory key for repeat cuts. Automatic SET function for reference measurement and EJECT function for pushing out paper. Self-diagnostic system with error indication on display. Electronic hand wheel with variable speed control for manual back gauge setting. Bright, LED optical cutting line. Adjustable, spindle guided back gauge with narrow separations and plastic gliders. Dual side guides on front and rear tables. High quality, German steel blade. Solid steel blade carrier and adjustable blade guides. All-metal construction. Includes stand with storage shelf, easy-access tool holder, and paper blocking tool. Optional side tables increase work surface. UL and C UL approved.\n\nElectrical requirements: 115 V, 60 Hz (20 amp dedicated line required)\nMotor output, horsepower: 2\nDimensions (D x W x H), inches: 44 x 33 7/8 x 51 (56 1/2 W with side tables)\nShipping weight, pounds: 648 (669 with side tables)","TRIUMPH 5255\nCutting width, inches 20 3/8\nCutting height, inches 3\nNarrow cut, inches 1 3/8\nLength behind blade, inches20 3/8\nList Price US $10,999",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Cutters/TRIUMPH-5255-223.html","https://www.youtube.com/watch?v=jiqE9R-0_rA",null,"Yes","Yes"]
[null,null,"TRIUMPH™ 5260","Comprehensive SCS™ safety package: patented EASY CUT electronic blade activation bars for true two-hand operation; IR light beam safety curtain on front table; safety cover on rear table; main switch and safety lock with key; 24 volt controls (low voltage); patented IDEAL safety drive; automatic blade and clamp return from every position; disc brake for instant blade stop; blade changing device covers cutting edge of blade; blade depth adjustment from outside of machine; blade and cutting stick can be changed without removing covers.\n\nErgonomic, 37 inch working height. Electric blade and clamp drive. Electric back gauge drive with touchpad for easy programming. Digital measurement display (cm or inches) with multilingual operator guidance, accurate to 1/10 mm or 1/100 inch. Stores 99 programs with up to 99 steps in each (up to 15 repeat cuts can be integrated as a single step). Pre-programmed for standard paper sizes. Memory key for repeat cuts. Automatic SET function for reference measurement and EJECT function for pushing out paper. Self-diagnostic system with error indication on display. Electronic hand wheel with variable speed control for manual back gauge setting. Bright, LED optical cutting line. 3-step, LED front table illumination. Adjustable, spindle guided back gauge with narrow separations and plastic gliders. Dual side guides on front and rear tables. High quality, German steel blade. Solid steel blade carrier and adjustable blade guides. All-metal construction. Includes stand with storage shelf, easy-access tool holder, and paper blocking tool. Optional side tables increase work surface. UL and C UL approved.\n\nElectrical requirements: 115 V, 60 Hz (20 amp dedicated line required)\nMotor output, horsepower: 2\nDimensions (D x W x H), inches: 44 x 33 7/8 x 51 (56 1/2 W with side tables)\nShipping weight, pounds: 657 (677 with side tables)","TRIUMPH 5260\nCutting width, inches 20 3/8\nCutting height, inches 3\nNarrow cut, inches 1 3/8\nLength behind blade, inches20 3/8\nList Price US $12,999",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Cutters/TRIUMPH-5260-224.html","https://www.youtube.com/watch?v=jiqE9R-0_rA",null,"Yes","Yes"]
[null,null,"TRIUMPH™ 6655","Comprehensive SCS™ safety package: patented EASY CUT electronic blade activation bars for true two-hand operation; transparent, electronically controlled front safety guard; safety cover on rear table; main switch and safety lock with key; 24 volt controls (low voltage); patented IDEAL safety drive; automatic blade and clamp return from every position; disc brake for instant blade stop; blade changing device covers cutting edge of blade; blade depth adjustment from outside of machine; blade and cutting stick can be changed without removing covers.\n\nErgonomic, 37 inch working height. Electric blade and clamp drive. Electric back gauge drive with touchpad for easy programming. Digital measurement display (cm or inches) with multilingual operator guidance, accurate to 1/10 mm or 1/100 inch. Stores 99 programs with up to 99 steps in each (up to 15 repeat cuts can be integrated as a single step). Pre-programmed for standard paper sizes. Memory key for repeat cuts. Automatic SET function for reference measurement and EJECT function for pushing out paper. Self-diagnostic system with error indication on display. Electronic hand wheel with variable speed control for manual back gauge setting. Bright, LED optical cutting line. Adjustable, spindle guided back gauge with narrow separations and plastic gliders. Dual side guides on front and rear tables. High quality, German steel blade. Solid steel blade carrier and adjustable blade guides. All-metal construction. Includes stand with storage shelf, easy-access tool holder, and paper blocking tool. Optional side tables increase work surface. UL and C UL approved.\n\nElectrical requirements: 115 V, 60 Hz (20 amp dedicated line required)\nMotor output, horsepower: 2\nDimensions (D x W x H), inches: 48 x 39 x 51 (61 1/2 W with side tables)\nShipping weight, pounds: 772 (793 with side tables)","TRIUMPH 6655\nCutting width, inches 25 1/2\nCutting height, inches 3\nNarrow cut, inches 1\nLength behind blade, inches24\nList Price US $13,199",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Cutters/TRIUMPH-6655-225.html","https://www.youtube.com/watch?v=jiqE9R-0_rA",null,"Yes","Yes"]
[null,null,"TRIUMPH™ 6660","Comprehensive SCS™ safety package: patented EASY CUT electronic blade activation bars for true two-hand operation; IR light beam safety curtain on front table; safety cover on rear table; main switch and safety lock with key; 24 volt controls (low voltage); patented IDEAL safety drive; automatic blade and clamp return from every position; disc brake for instant blade stop; blade changing device covers cutting edge of blade; blade depth adjustment from outside of machine; blade and cutting stick can be changed without removing covers.\n\nErgonomic, 37 inch working height. Electric blade and clamp drive. Electric back gauge drive with touchpad for easy programming. Digital measurement display (cm or inches) with multilingual operator guidance, accurate to 1/10 mm or 1/100 inch. Stores 99 programs with up to 99 steps in each (up to 15 repeat cuts can be integrated as a single step). Pre-programmed for standard paper sizes. Memory key for repeat cuts. Automatic SET function for reference measurement and EJECT function for pushing out paper. Self-diagnostic system with error indication on display. Electronic hand wheel with variable speed control for manual back gauge setting. Bright, LED optical cutting line. 3-step, LED front table illumination; Adjustable, spindle guided back gauge with narrow separations and plastic gliders. Dual side guides on front and rear tables. High quality, German steel blade. Solid steel blade carrier and adjustable blade guides. All-metal construction. Includes stand with storage shelf, easy-access tool holder, and paper blocking tool. Optional side tables increase work surface. UL and C UL approved.\n\nElectrical requirements: 115 V, 60 Hz (20 amp dedicated line required)\nMotor output, horsepower: 2\nDimensions (D x W x H), inches: 48 x 39 x 51 (61 1/2 W with side tables)\nShipping weight, pounds: 775 (796 with side tables)","TRIUMPH 6660\nCutting width, inches 25 1/2\nCutting height, inches 3\nNarrow cut, inches 1\nLength behind blade, inches24\nList Price US $14,999",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Cutters/TRIUMPH-6660-226.html","https://www.youtube.com/watch?v=jiqE9R-0_rA",null,"Yes","Yes"]
[null,null,"TRIUMPH™ 5560 /5560 LT","Comprehensive SCS™ safety package: patented EASY CUT electronic blade activation bars for true two-hand operation; IR light beam safety curtain on front table; safety cover on rear table; lockable main switch; 24 volt controls (low voltage); patented IDEAL safety drive; automatic blade and clamp return from every position; blade changing device covers cutting edge of blade; blade depth adjustment from outside of machine; blade and cutting stick can be changed without removing covers.\n\nHydraulic blade and clamp drive. Foot pedal for pre-clamping. Electric back gauge drive with touchpad for easy programming. Digital measurement display (cm or inches) with multilingual operator guidance, accurate to 1/10 mm or 1/100 inch. Stores 99 programs with up to 99 steps in each (up to 15 repeat cuts can be integrated as a single step). Pre-programmed for standard paper sizes. Memory key for repeat cuts. Automatic SET function for reference measurement and EJECT function for pushing out paper. Self-diagnostic system with error indication on display. Electronic hand wheel with variable speed control for manual back gauge setting. Clamp pressure is fully adjustable between 1,900 and 3,800 psi. False clamp plate. Bright, LED optical cutting line. Stainless steel work surface. High quality, German HSS blade. Precision swing cut blade movement. Aluminum blade carrier and clamp bar. Adjustable blade guides. All-metal construction. Mounted on casters. Includes easy-access tool holder and paper blocking tool. Optional side tables increase work surface. UL and C UL approved.\n\nDimensions (D x W x H), inches: 55 x 42 x 54 (64 W with side tables) \n5560 shipping weight, pounds: 970 (1,008 with side tables) \n5560 LT shipping weight, pounds: 1,014 (1,052 with side tables)","TRIUMPH 5560 /5560 LT\nCutting width, inches 21 5/8\nCutting height, inches 3 3/4 (3 5/8 with false clamp)\nNarrow cut, inches 1 1/4 (2 3/8 with false clamp)\nLength behind blade, inches22 7/16\nList Price US $16,999, LT: $19,999",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Cutters/TRIUMPH-5560-5560-LT-227.html",null,null,"Yes","Yes"]
[null,null,"TRIUMPH™ 7260","Comprehensive SCS™ safety package: patented EASY CUT electronic blade activation bars for true two-hand operation; IR light beam safety curtain on front table; safety cover on rear table; main switch and safety lock with key; 24 volt controls (low voltage); patented IDEAL safety drive; automatic blade and clamp return from every position; disc brake for instant blade stop; blade changing device covers cutting edge of blade; blade depth adjustment from outside of machine; blade and cutting stick can be changed without removing covers.\n\nHydraulic clamp drive. Foot pedal for pre-clamping. Electric back gauge drive with control module for easy programming. Digital measurement display (cm or inches) with multilingual operator guidance, accurate to 1/10 mm or 1/100 inch. Stores 99 programs with up to 99 steps in each (up to 15 repeat cuts can be integrated as a single step). Pre-programmed for standard paper sizes. Memory keys for repeat cuts (manual) and quick setting of frequently needed measurements. Automatic SET function for reference measurement and paper EJECT function with and without program mode. DELETE and INSERT mode for correcting and modifying programs. Automatic correction in case of back gauge displacement. Push buttons for fast back gauge movement (forward and reverse). Integrated calculator. Self-diagnostic system with error indication on display. Electric blade drive with solid steel carrier and adjustable guides. Electronic hand wheel with variable speed control for manual back gauge setting. Clamp pressure is fully adjustable between 550 and 4,400 psi. False clamp plate with optical indicator. Bright, LED optical cutting line. Stainless steel work surface. Standard air tables (front and rear). High quality, German HSS blade. Precision swing cut blade movement. All-metal construction. Includes easy-access tool holder and paper blocking tool. Optional side tables increase work surface. UL and C UL approved.\n\nDimensions (D x W x H), inches: 60 1/2 x 51 3/8 x 52 1/2 (63 D, 82 1/2 W with side tables) \nShipping weight, pounds: 1,534 (1,622 with side tables)","TRIUMPH 7260\nCutting width, inches 28\nCutting height, inches 3\nNarrow cut, inches 3/4 (3 1/2 with false clamp)\nLength behind blade, inches28\nList Price US $23,999",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Cutters/TRIUMPH-7260-228.html",null,null,"Yes","Yes"]
[null,null,"Scissor Hands","What is Scissor Hands?\n\nScissor Hands is a cloud-based software which instantly converts JDF layouts into cut programs. These cut programs increase productivity and profit margins through unequaled automation and integration with your cutting machine, MIS, and prepress systems.\n\n• Customized Cuts\n• Time Saving\n• Reduce Cuts\n• Increase Throughput\n• Complete data collection & reporting\n• Reduce Paper Waste\n• Eliminate Complex Programming\n• Reduce labor costs\n• Minimize cutting errors\n• Integrates with Existing Systems",null,null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Cutters/Scissor-Hands-443.html",null,null,"Yes","Yes"]
[null,"Triumph™ Trimmers"]
[null,null,"TRIUMPH™ 1134","Solingen steel blade set may be resharpened. Manual clamp. Transparent Lexan® safety guard with integrated cutting line indicator. Precision side guides scaled in inches and metric system. Adjustable back gauge. Standard paper sizes indicated on table. Non-skid rubber feet for safe operation. Heavy duty blade. Mounting bracket. All-metal construction.\n\nDimensions (D x W x H), inches: 22 1/4\" x 13 1/4\" x 12\" \nShipping weight: 11 lbs.","TRIUMPH 1134\nCutting length 13 3/4\"\nSheet capacity 25*\nTable size (D x W)15\" x 12\"\nList Price US $279",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Trimmers/TRIUMPH-1134-250.html",null,null,"Yes","Yes"]
[null,null,"TRIUMPH™ 1135","Solingen steel blade set may be resharpened. Precision automatic clamp with \"Easy Lift\" release lever for easy paper removal. Transparent Lexan® safety guard with integrated cutting line indicator. Precision side guides scaled in inches and metric system. Adjustable back gauge. Standard paper sizes indicated on table. Non-skid rubber feet for safe operation. Solid cast aluminum blade. Mounting bracket with double pivot bearings for blade axle. All-metal construction.\n\nDimensions (D x W x H), inches: 23\" x 13 3/8\" x 12 3/4\" \nShipping weight: 13 lbs.","TRIUMPH 1135\nCutting length 13 3/4\"\nSheet capacity 25*\nTable size (D x W)15\" x 12\"\nList Price US $339\n",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Trimmers/TRIUMPH-1135-251.html",null,null,"Yes","Yes"]
[null,null,"TRIUMPH™ 1038","Solingen steel blade set may be resharpened. Transparent Lexan® safety guard automatically covers blade in every position. Solid hand clamp, independent of blade handle. precision side guides scaled in inches and metric system. Adjustable back gauge; front gauge is adjustable using a calibrated rotary knob with fine adjustment scale, lockable in every position. Narrow-strip cutting device. Fold-away paper supports on front gauge allow precise cutting of lightweight paper stocks. Standard paper sizes indicated on table. Non-skid rubber feet for safe operation. Solid cast aluminum blade mounting bracket with double pivot bearings for blade axle. All-metal construction.\n\nDimensions (D x W x H), inches: 31\" x 16\" x 10\" \nShipping weight: 29 lbs.","TRIUMPH 1038\nCutting length 15\nSheet capacity 50*\nTable size (D x W)23 3/4\" x 14\"\nList Price US $579",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Trimmers/TRIUMPH-1038-252.html",null,null,"Yes","Yes"]
[null,null,"TRIUMPH™ 1046","Solingen steel blade set may be resharpened. Precision automatic clamp with \"Easy Lift\" release lever for easy paper removal. Transparent Lexan® safety guard with integrated cutting line indicator. Precision side guides scaled in inches and metric system. Adjustable back gauge. Standard paper sizes indicated on table. Non-skid rubber feet for safe operation. Solid cast aluminum blade mounting bracket with double pivot bearings for blade axle. All-metal construction.\n\nDimensions (D x W x H), inches: 27 1/2\" x 15 1/4\" x 15\" \nShipping weight: 20 lbs.","TRIUMPH 1046\nCutting length 18\"\nSheet capacity 30*\nTable size (D x W)20\" x 14\"\nList Price US $519\n",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Trimmers/TRIUMPH-1046-253.html",null,null,"Yes","Yes"]
[null,null,"TRIUMPH™ 1058","Solingen steel blade set may be resharpened. Transparent Lexan® safety guard automatically covers blade in every position. Solid hand clamp, independent of blade handle. Precision side guides scaled in inches and metric system. Adjustable back gauge; front gauge is adjustable using a calibrated rotary knob with fine adjustment scale, lockable in every position. Narrow-strip cutting device. Fold-away paper supports on front gauge allow precise cutting of lightweight paper stocks. Standard paper sizes indicated on table. Non-skid rubber feet for safe operation. Solid cast aluminum blade mounting bracket with double pivot bearings for blade axle. All-metal construction.\n\nDimensions (D x W x H), inches: 31\" x 16\" x 10\" \nShipping weight: 42 lbs.","TRIUMPH 1058\nCutting length 22 1/2\"\nSheet capacity 40*\nTable size (D x W)23 3/4\" x 14\"\nList Price US $859",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Trimmers/TRIUMPH-1058-254.html",null,null,"Yes","Yes"]
[null,null,"TRIUMPH™ 1071","Solingen steel blade set may be resharpened. Transparent Lexan® safety guard. Solid hand clamp, independent of blade handle. Precision side guides scaled in inches and metric system. Adjustable back gauge; front gauge is adjustable using a calibrated rotary knob with fine adjustment scale, lockable in every position. Narrow-strip cutting device. Fold-away paper supports on front gauge allow precise cutting of lightweight paper stocks. Standard paper sizes indicated on table. Non-skid rubber feet for safe operation. Solid cast aluminum blade mounting bracket with double pivot bearings for blade axle. All-metal construction.\n\nDimensions (D x W x H), inches: 38 1/2\" x 22 1/4\" x 20 1/2\" \nShipping weight: 62 lbs.","TRIUMPH 1071\nCutting length 28 1/2\"\nSheet capacity 40*\nTable size (D x W)30\" x 20\"\nList Price US $1,049\nRelated Products",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Trimmers/TRIUMPH-1071-255.html",null,null,"Yes","Yes"]
[null,null,"TRIUMPH™ 1080","Solingen steel blade set may be resharpened. Special wide-angle blade cuts heavy materials such as matteboard, plastic, and metal foil. Transparent Lexan® safety guard blade lock. Foot pedal for positive clamping. Precision side guides scaled in inches and metric system. Adjustable back gauge; front gauge is adjustable using a calibrated rotary knob with fine adjustment scale, lockable in every position. Narrow-strip cutting device. Fold-down extension table provides support for large cutting jobs. Standard paper sizes indicated on table. Solid cast aluminum blade mounting bracket with double pivot bearings for blade axle. All-metal construction.\n\nDimensions (D x W x H), inches: 42 1/2\" x 26 1/4\" x 48\" (35\" W with fold-away extension table in working position)\nShipping weight: 158 lbs.","TRIUMPH 1080\nCutting length 31 1/2\"\nSheet capacity 20* (5/32\" cutting height)\nTable size (D x W)31 1/2\" x 23 7/8\"\nList Price US $1,849\n",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Trimmers/TRIUMPH-1080-256.html",null,null,"Yes","Yes"]
[null,null,"TRIUMPH™ 1110","Solingen steel blade set may be resharpened. Special wide-angle blade cuts heavy materials such as matteboard, plastic, and metal foil. Transparent Lexan® safety guard blade lock. Foot pedal for positive clamping. Precision side guides scaled in inches and metric system. Adjustable back gauge; front gauge is adjustable using a calibrated rotary knob with fine adjustment scale, lockable in every position. Narrow-strip cutting device. Fold-down extension table provides support for large cutting jobs. Standard paper sizes indicated on table. Solid cast aluminum blade mounting bracket with double pivot bearings for blade axle. All-metal construction.\n\nDimensions (D x W x H): 54 3/4\" x 32 1/2\" x 53 1/2\" (41 3/4\" W with fold-away extension table in working position)\nShipping weight: 182 lbs.","TRIUMPH 1110\nCutting length 43 1/4\"\nSheet capacity 20* (5/32\" cutting height)\nTable size (D x W)43 1/4\" x 30\"\nList Price US $2,659",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Trimmers/TRIUMPH-1110-257.html",null,null,"Yes","Yes"]
[null,null,"TRIUMPH™ 1030","Ergonomic safety cutting head with fully enclosed, hardened steel rotary blade. Transparent bar clamp with automatic clamping action. Extendable bracket with measurement scale can be used as a front or back gauge. Protractor with alignment indicators on clamp bar and cutting table for angle cuts. Dual measurement scales on cutting table. Constructed of sturdy, impact-resistant ABS plastic with non-slip rubber feet.\n\nDimensions (D x W x H), inches: 8 x 18 3/4 x 2 3/8\nShipping weight, pounds: 2","TRIUMPH 1030\nCutting width, inches 13\nCapacity, sheets 5-6*\nTable size (D x W), inches6 1/2 x 13\nList Price US $89",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Trimmers/TRIUMPH-1030-258.html",null,null,"Yes","Yes"]
[null,null,"TRIUMPH™ 1031","Ergonomic safety cutting head with fully enclosed, hardened steel rotary blade. Transparent bar clamp with automatic clamping action. Extendable bracket with measurement scale can be used as a front or back gauge. Protractor with alignment indicators on clamp bar and cutting table for angle cuts. Dual measurement scales on cutting table. Constructed of sturdy, impact-resistant ABS plastic with non-slip rubber feet.\n\nDimensions (D x W x H), inches: 8 x 22 1/2 x 2 3/8\nShipping weight, pounds: 2 1/2","TRIUMPH 1031\nCutting width, inches 17\nCapacity, sheets 5-6*\nTable size (D x W), inches6 1/2 x 17\nList Price US $99",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Trimmers/TRIUMPH-1031-259.html",null,null,"Yes","Yes"]
[null,null,"TRIUMPH™ 0055","Ergonomic safety cutting head with self-sharpening, hardened steel rotary blade. Stainless steel counter blade. Precision cross bar. Slotted side brackets for cutting oversized formats. Transparent bar clamp with automatic clamping action. Anodized aluminum cutting table. Dual measurement scales on cutting table. Side brackets constructed of sturdy, impact-resistant ABS plastic. Mounted on non-slip rubber feet.\n\nDimensions (D x W x H), inches: 15 x 31 1/2 x 4 1/4\nShipping weight, pounds: 13 1/2","TRIUMPH 0055\nCutting width, inches 21 1/2\nCutting height, inches 1/32*\nTable size (D x W), inches11 x 23\nList Price US $499",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Trimmers/TRIUMPH-0055-260.html",null,null,"Yes","Yes"]
[null,null,"TRIUMPH™ 0075","Ergonomic safety cutting head with self-sharpening, hardened steel rotary blade. Stainless steel counter blade. Precision cross bar. Slotted side brackets for cutting oversized formats. Transparent bar clamp with automatic clamping action. Anodized aluminum cutting table. Dual measurement scales on cutting table. Side brackets constructed of sturdy, impact-resistant ABS plastic. Mounted on non-slip rubber feet.\n\nDimensions (D x W x H), inches: 15 x 39 1/4 x 4 1/4\nShipping weight, pounds: 16","TRIUMPH 0075\nCutting width, inches 29 1/2\nCutting height, inches 1/32*\nTable size (D x W), inches11 x 29 1/2\nList Price US $599",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Trimmers/TRIUMPH-0075-261.html",null,null,"Yes","Yes"]
[null,null,"TRIUMPH™ 0105 U","Ergonomic safety cutting head with self-sharpening, hardened steel rotary blade. Stainless steel counter blade. Precision cross bar. Slotted side brackets for cutting oversized formats. Transparent bar clamp with automatic clamping action. Anodized aluminum cutting table. Dual measurement scales on cutting table. Side brackets constructed of sturdy, impact-resistant ABS plastic. Mounted on sturdy metal stand with collection tray and non-slip rubber feet.\n\nDimensions (D x W x H), inches: 15 x 51 x 38\nShipping weight, pounds: 46","TRIUMPH 0105 U\nCutting width, inches 41 1/4\nCutting height, inches 1/32*\nTable size (D x W), inches11 x 41 1/4\nList Price US $999\n",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Trimmers/TRIUMPH-0105-U-262.html",null,null,"Yes","Yes"]
[null,null,"TRIUMPH™ 0135","PAPER COLLECTION TRAY\nA convenient collection tray catches waste paper, ensuring a neat work area.PAPER HOLDER\nAn optional paper roll holder adds an added degree of versatility.\nProfessional model rotary trimmer ideal for cutting and trimming blueprints, drawings, posters, photos, and large format digital printouts. Smooth running safety cutting head with self sharpening, hardened steel rotary blade. Counter blade made of stainless knife steel. Automatic clamping system with transparent clamp bar. Paper collection tray. Sturdy metal stand. Optional paper roll holder.\n\nDimensions (D x W x H), inches: 19\" x 60 1/2\" x 37\" \nShipping weight: 84 lbs.","TRIUMPH 0135\nCutting width 53\"\nCutting height 1/32\"*\nTable depth 11 1/2\"\nTable height34\"\nList Price US $1,299",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Trimmers/TRIUMPH-0135-263.html",null,null,"Yes","Yes"]
[null,null,"TRIUMPH™ 0155","Professional model rotary trimmer with 61 inch cutting width ideal for cutting and trimming blueprints, drawings, posters, photos, and large format digital printouts. Smooth running safety cutting head with self sharpening, hardened steel rotary blade. Counter blade made of stainless knife steel. Automatic clamping system with transparent clamp bar. Paper collection tray. Sturdy metal stand. Optional paper roll holder.\n\nDimensions (D x W x H), inches: 19\" x 68 1/2\" x 37\" \nShipping weight: 88 lbs.","TRIUMPH 0155\nCutting width 61\"\nCutting height 1/32\"*\nTable depth 11 1/2\"\nTable height34\"\nList Price US $1,449",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Triumph-Trimmers/TRIUMPH-0155-264.html",null,null,"Yes","Yes"]
[null,"Folders"]
[null,null,"98M","The 98M is the new and improved model of the 93M. New features include Test Mode, a lock plate to separate the rollers to prevent them from deformation, and there’s no longer a need to reverse the second folding plate when performing a double fold job. Compact size (feed table and exit tray fold in for storage). Simple, push-button operation. Digital control panel. Programmable counter with batch and total functions. Color-coded fold plate graphics for quick and easy set-up. Powered exit conveyor. Exit tray extension for neat stacking of folded sheets. Automatic stop when last sheet is folded.  \n\nDimensions (D x W x H), inches: 14 x 25 x 16 3/4\nShipping weight, pounds: 39","98M\nSpeed, sheets per hour 7,200*\nPaper size, inches 4 x 5 to 8 1/2 x 14\nPaper weight, pounds 16 to 80*\nSheet capacity 150*\nElectrical requirements120 V, 60 Hz\nList Price US $1,099.00",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Folders/98M-421.html",null,null,"Yes","Yes"]
[null,null,"208J","3 roller friction feed system. Easy set-up for standard and custom folds. Control touch panel includes 4 digit counter with addition and subtraction functions. Test button folds 2 sheets for inspection. Extended exit tray for neat stacking of folded sheets. Automatic conveyor ensures smooth ejection of folded paper. Single sheet feeding automatically maintained for different weights of paper. Auxiliary paper guide for cross folding. Load and unload paper from same side. Display alert and audible signal in case of incorrect operation. Skew and micro-adjustment dials. Quick-release roller system for easy maintenance.\n\nDimensions (D x W x H), inches: 21 1/2 x 40 5/8 x 19 3/4\nShipping weight, pounds: 73","208J\nSpeed, sheets per hour Up to 14,400*\nPaper size, inches 3 1/2 x 5 to 11 x 17\nPaper weight, pounds 12 to 80*\nSheet capacity 500*\nElectrical requirements115 V, 60 Hz\nList Price US $2,699",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Folders/208J-433.html","https://www.youtube.com/watch?v=1Jq6lWqACHA",null,"Yes","Yes"]
[null,null,"408A","Automatic 3 roller friction feed system. Pre-programmed with 18 standard folds. Stores 12 custom folds in memory. Color LED touch screen control panel includes 4 digit addition / subtraction digital counter. Test button folds 2 sheets for inspection. Automatically senses and displays paper size. Extended exit tray for neat stacking of folded sheets. Automatic conveyor ensures smooth ejection of folded paper. Single sheet feeding automatically maintained for different weights of paper. Auxiliary paper guide for cross folding. Load and unload paper from same side. Display alert and audible signal in case of incorrect operation. Skew and micro-adjustment dials. Fully enclosed fold tables for quiet operation. Quick-release roller system for easy maintenance. Optional scoring, micro-perforating, and slitting units.\n\nDimensions (D x W x H), inches: 39 3/4 x 21 1/2 x 19 3/4\nShipping weight, pounds: 76","408A\nSpeed, sheets per hour Up to 14,400*\nPaper size, inches 3 1/2 x 5 to 11 x 17\nPaper weight, pounds 12 to 80*\nSheet capacity 500*\nElectrical requirements115 V, 60 Hz\nList Price US $3,899.00",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Folders/408A-430.html","https://www.youtube.com/watch?v=J_4htrhqNwg",null,"Yes","Yes"]
[null,null,"508A","Automatic 3 roller friction feed system. Pre-programmed with 18 standard folds. Stores 24 custom folds in memory. Automatic feed table elevation. Features paper feed pressure and separator pressure adjustment. Color LED touch screen control panel includes 4 digit addition and subtraction digital counter. Test button folds 2 sheets for inspection. Automatically recognizes and displays paper size. Extended exit tray for neat stacking of folded sheets. Automatic conveyor and self-setting exit rollers ensure smooth ejection of folded paper. Single sheet feeding automatically maintained for different weights of paper. Auxiliary paper guide for cross folding. Load and unload paper from same side. Display alert and audible signal in case of incorrect operation. Skew and micro-adjustment dials. Fully enclosed fold tables for quiet operation. Quick-release roller system for easy maintenance. Optional scoring, micro-perforating, and slitting units.\n\nDimensions (D x W x H), inches: 39 3/4 x 21 1/2 x 19 3/4\nShipping weight, pounds: 82","508A\nSpeed, sheets per hour Up to 14,400*\nPaper size, inches 3 1/2 x 5 to 11 x 17\nPaper weight, pounds 12 to 80*\nSheet capacity 500*\nElectrical requirements115 V, 60 Hz\nList Price US $4,799",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Folders/508A-432.html","https://www.youtube.com/watch?v=J_4htrhqNwg",null,"Yes","Yes"]
[null,null,"1800S","The 1800S by MBM is the new and improved model of the 1500S. The ultrasonic double feed sensor is new to this model. The 1500S could not detect double feeds on black or transparent sheets, but the new 1800S detects double feeds on any white, printed, transparent, black or mixture of colored sheets. Also new to the 1800S is the removable folding roller for easy maintenance, the adjustable folding roller pressure, and a spring loaded feed angle adjustment dial. The machine top cover opens and closes in two easy steps and the operator can now reach the air adjustment knob without disruption when the top cover is open. New “silver top” metal sheet for smoother paper run and better electric conductivity. Top feed, adjustable air suction feed system, suitable for digitally printed and coated stocks. Pre-programmed with 6 standard folds. Stores 30 custom folds in memory. One-touch memory keys for custom folds. Non-standard paper sizes can be stored in memory. Control touch panel includes 4 digit counter with batch and total functions. Test button folds 2 sheets for inspection. Extended exit tray for neat stacking of folded sheets. Automatic feed table ensures optimum feed pressure. Automatic conveyor belt and self-setting exit rollers ensure smooth ejection of folded paper. Single sheet feeding automatically maintained for different weights of paper. Display alert and audible signal in case of incorrect operation. Skew and micro-adjustment dials. All-metal construction. Optional micro-perforator, and scorer.\n\nDimensions (D x W x H), inches: 24 x 49 x 23\nShipping weight, pounds: 189","1800S\nSpeed, sheets per hour 18,000*\nPaper size, inches 4 1/2 x 8 1/4 to 13 x 19\nPaper weight, pounds 16 to 80*\nSheet capacity 800*\nElectrical requirements120 V, 60 Hz\nList Price US $7,599",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Folders/1800S-429.html",null,null,"Yes","Yes"]
[null,null,"352F","Dual roller friction feed system accepts a wide variety of stocks. Adjusts in seconds for standard and custom folds. Variable speed control. Powered exit conveyor. Sheet separation from top of fanned stack. Polyurethane foam rollers eliminate the need for fold roller pressure settings. Heavy-duty, non-flexing side frames. Needle bearings for high speed production. Optional extended delivery system, crossfold for right-angle folding, and slitting, scoring, and perforating attachments. UL and C UL approved.\n\nDimensions (D x W x H), inches: 22 1/4 x 41 3/4 x 14 1/2 \nShipping weight, pounds: 105","352F\nSpeed, sheets per hour 22,000*\nPaper size, inches 2 x 2 3/4 to 14 x 21 1/4\nPaper weight, pounds 13 to 110*\nSheet capacity 300*\nElectrical requirements115 V, 60 Hz\nList Price US $4,699",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Folders/352F-199.html",null,null,"Yes","Yes"]
[null,null,"352S","Air suction feed system, suitable for coated stocks. Adjusts in seconds for standard and custom folds. Variable speed control. Powered exit conveyor. Bottom-feed, top-loading design for continuous reloading and dependable sheet separation. Polyurethane foam rollers eliminate the need for fold roller pressure settings. Turbine blower fully enclosed for quiet operation. 2 fold plates. Heavy-duty, non-flexing side frames. Needle bearings for high speed production. Mounted on casters. Optional extended delivery system, crossfold for right-angle folding, and slitting, scoring, and perforating attachments. UL and C UL approved.\n\nDimensions (D x W x H), inches: 22 1/4 x 51 1/4 x 43 1/2 \nShipping weight, pounds: 312 lbs.","352S\nSpeed, sheets per hour 30,000*\nPaper size, inches 3 3/8 x 4 3/4 to 12 5/8 x 17 3/4\nPaper weight, pounds 13 to 110*\nSheet capacity 450*\nElectrical requirements115 V, 60 Hz\nList Price US $8,399",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Folders/352S-200.html",null,null,"Yes","Yes"]
[null,"Creasers"]
[null,null,"GoCrease™ 3000","This creasing and perforating machine is designed for the final processing of graphic materials up to 12.6” x 17.7” in paper size. Simple hand operated machine with a working width of 12.6” allows a crease and/or perf to be made with the same quality as the electric GoCrease™ 4000/SEMI. Eccentric wheel of operating mechanism demands only minimum effort to process the paper, even for heavy stocks or laminated documents. Skew paper can also be creased/perforated due to thumb wheel angle adjustment of side guide. The GoCrease 3000 has an exchangeable creasing and perforating knife, as well as 3 different creasing channel widths. \n\nDimensions (D x W x H), inches: 14.5 x 19 x 15.5\nShipping weight, pounds: 27.5","GoCrease 3000\nMin/max working width 1\" to 12.6\"\nPaper weight, pounds 80-400 gsm (creasing), 80-250 gsm (perforating)\nWidth of crease 0.04 / 0.05 / 0.06\"\nMax working width12.6\"\nList Price US $899",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Creasers/GoCrease-3000-424.html",null,null,"Yes","Yes"]
[null,null,"GoCrease™ 4000","This creasing and perforating machine with a working width of 18” is designed for the final processing of graphic materials up to 18” x 23.4”. Creasing enables high-quality folds of digitally printed paper. The machine can also be controlled via a foot pedal. The GoCrease™ 4000 is built with high quality anvil perforation, as well as 3 different creasing channel widths.\n\nDimensions (D x W x H), inches: 23.5 x 28 x 12\nShipping weight, pounds: 92.6","GoCrease 4000\nMin/max working width 1\" to 18\"\nPaper weight, pounds 80-400 gsm (creasing), 80-250 gsm (perforating)\nMax working width 18\"\nWidth of crease 0.04 / 0.05 / 0.063\"\nElectrical requirements120 V, 60 Hz\nList Price US $1,999",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Creasers/GoCrease-4000-425.html","https://www.youtube.com/watch?time_continue=2&v=UPQ1TQBXMbo",null,"Yes","Yes"]
[null,null,"GoCrease™ SEMI","The GoCrease™ SEMI is a creasing and / or perforating machine with programmable control and a working width of 18”. Manual paper input, paper movement powered by motor. Creasing enables high-quality folds of digitally printed paper. Up to 5 pre-set applications can be stored in program memory. Automatically measures sheet size. 3 sizes of creasing bars included (2 x CITO technology, 1 x iron channel). Available with 8 languages (English, German, French, Spanish, Italian, Russian, Greek, and Czech). \n\nDimensions (D x W x H), inches: 23.5 x 45 x 12\nShipping weight, pounds: 120","GoCrease SEMI\nSpeed, sheets per hour 1500\nPaper weight, pounds 80-400 gsm (crease), 80-250 gsm (perf)\nMin/max working width 4\" to 18\"\nMax. creases per sheet 15\nPreprogrammed types of folds 1/2, 1/3, 1/4, gate, book cover\nMin. distance of creases 0.07\"\nWidth of crease, inches 0.04 / 0.05 / 0.063\nElectrical requirements120 V, 60 Hz\nList Price US $5,399",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Creasers/GoCrease-SEMI-426.html","https://www.youtube.com/watch?v=s6tPDYZfa6Y",null,"Yes","Yes"]
[null,null,"GoCrease™ F-SPEED","The GoCrease™ F-SPEED features a unique friction feed system enabling fast and high production of creased and perforated sheets. This machine also offers a wide range of “easy change” punching tools commonly used for wire binding and calendar production. A mobile table is included for easy and diverse use. Predefined fold types include: 1/2, 1/3, 1/4, gate, and book cover. 2.25” stack height. Automatically measures sheet size. Batching, a telescopic feed table, adjustable feed pressure, and two widths of creasing channels come standard with the GoCrease™ F-SPEED. Available with 8 languages (English, German, French, Spanish, Italian, Russian, Greek, and Czech). \n\nDimensions (D x W x H), inches: 26.5 x 50 x 20.5 (48 with table)\nShipping weight, pounds: 346 (includes mobile table)","GoCrease F-SPEED\nSpeed, sheets per hour 2,500*\nPaper weight, gsm 80-400 gsm (creasing), 80-250 gsm (perforating), 80-400 gsm (punching)\nMax. working width, inches 18 (creasing & perforating) 17.7 (punching)\nCustom programs 5\nMax. number of creases per sheet 15\nMin. distance of creases, inches 0.03\nElectrical requirements120 V, 60 Hz\nList Price US $8,950",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Creasers/GoCrease-FSPEED-428.html","https://www.youtube.com/watch?v=YYUeNsZ2RcQ",null,"Yes","Yes"]
[null,null,"GoCrease™ AutoAir","The GoCrease™ AutoAir features a unique air feed system enabling creasing of all types of paper within 80-400 gsm. Accuracy, feeding reliability, versatility of use, optional rotary perforating & cutting tools, high speed, and input capacity - are all main features of this model. The 7” color touch screen display makes the GoCrease™ AutoAir very user friendly. Skew adjustment, program storage, batching, and two widths of creasing channels comes standard on the machine. 2.75” stack height. Automatically measures sheet size. A mobile table is included for easy and diverse use, as well as 2 creasing tools, a perforating tool, and a perforating wheel. Predefined fold types include: 1/2, 1/3, 1/4, gate, and book cover.\n\nDimensions (D x W x H), inches: 31 x 48 (57) x 28.5 (48 with table)\nShipping weight, pounds: 415.6 (includes mobile table)","GoCrease AutoAir\nSpeed, sheets per hour 3,000* (1 crease), 4,300* (0 crease)\nPaper weight, gsm 80-400 gsm (creasing), 80-250 gsm (perforating)\nCustom programs 60\nMax.working width, inches 18 (creasing & perforating) 17.7 (punching)\nMax. creases per sheet 40\nMax. perfing wheels 13\nMin. distance of creases 0.03\"\nElectrical requirements120 V, 60 Hz\nList Price US $12,999",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Creasers/GoCrease-AutoAir-427.html","https://www.youtube.com/watch?v=P7GLa8iW_tU",null,"Yes","Yes"]
[null,null,"GoCrease™ FOLD","Paper weight: 100-350 gsm\nPaper formats with pre-set folds: 8.5 x 11’’ 11 x 17’’ 13 x 18’’ 14 x 20’’\nMax. width of paper: 14.17’’\nMin. width of paper: 4.52”\nFold types*: Half-Fold, Z-Fold, C-Fold, Roll Fold, 3-Panel Gate Fold\nSpeed: Separate speed controls for transport belts and folding rollers. Speed is sufficient for maximum speed of GoCrease AutoAir, which is 4500 sheets per hour.\nFeeding capacity: Based on capacity of creaser\nCommunication with F-SPEED/AutoAir creaser: By cable\nVoltage/frequency: 120/60 Hz\nGross weight: 326 lb.\nNet weight: 249 lb.\nPackaging: wooden box on pallet: 47.2” x31.5” x 28.3’’\n\n*may vary due to variations in paper weight",null,null,"https://www.mbmcorp.com/Paper-Finishing-Products/Creasers/GoCrease-FOLD-441.html",null,null,"Yes","Yes"]
[null,"Digital Paper Finishing Products"]
[null,null,"AEROCUT PRIME","The Aerocut Prime is an ideal solution for finishing, especially for short-run digitally printed applications, such as business cards, post cards, invitations, greeting cards, leaflets, tickets and more. The complete package offers full versatility and convenience of the machine. The Prime has the capability to perforate stocks both across and along feeding direction by adding on an optional perforating unit. Flex mode allows operators to cut multiple size cards from a page and add the desired number of creases on these; It enables designers and printers to create new aspects of applications. The Prime saves time and costs for any print shop, in-house printer, commercial printer, etc. Channel creasing is equipped on every unit, allowing the machine to offer world-class creases on digitally printed stocks. Creasing pressure can be adjusted in 5 levels instantly by shifting the lever. The Aerocut Prime features 2 single blade slitters to trim top & bottom margins, and 2 double blade slitters for center gutters and precise accuracy. The durable blades cut stocks up to 400 gsm. The air-suction top feeding system easily feeds coated, digital, gloss and other stocks precisely without damage. All-metal construction. Mounted on lockable, heavy-duty casters. Safety access cover—machine will not operate with cover in open position. The Prime Complete comes with a conveyor / stacker. It replaces the rear table for higher production output. Includes the new Lytrod Intellicut software to easily impose artwork + address data to seamlessly create PDF layouts with job barcodes and cut marks for the Prime.\n\nProduct dimensions (D x W x H), inches: 30.3 x 57.6 x 41.13\nShipping weight: 573 lbs.\n\nNote: Exit tray is available as an option on the Prime Complete. The Aerocut Prime is a restricted product. Please contact your sales representative for terms.","AEROCUT PRIME\nSpeed 24 sheets/min*\nSheet capacity 4\"\nPaper size 8.27 x 8.27 to 14.5 x 26.75\nPaper weight 120 - 400 gsm.**\nPower supply100 - 120 V, 50/60 Hz\nList Price US Prime: $46,999 Prime Complete: 49,999",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Digital-Finishing-Solutions/AEROCUT-PRIME-418.html","https://www.youtube.com/watch?v=Yc8g2a9RC-A",null,"Yes","Yes"]
[null,null,"AEROCUT VELOCITY","The Aerocut Velocity is the refined model of the Aerocut Classic slitter/cutter/creaser and features enhanced productivity and user-friendliness. Feeding is an important and essential part for any print finishing device. This machine has an innovative patented feeding mechanism, that drastically reduces the risk of double feeds and mis-feeds. An optional perforating unit is located inside for an accurate registration. The Velocity is twice as fast and includes more adjustments than base Aerocut Classic with a greater (4”) sheet capacity. The robust all-metal construction keeps top level accuracy and finishing quality on every job. Includes 263 preset cutting jobs and up to 150 additional custom programs can be stored in memory. The Velocity is an ideal solution for finishing, especially for short-run digital printed applications, such as business cards, post cards, invitations, greeting cards, leaflets, tickets and more. Flex mode allows operators to cut multiple size cards from a page and add the desired number of creases on these; It enables designers and printers to create new aspects of applications. Self-correcting cut mark registration function and air suction feed system ensure accurate cuts every time.  The Velocity saves times and costs for print shops, in-house printers, commercial printers etc. Velocity uses channel creasing, allowing the machine to offer world-class quality creases on digitally printed stocks. Creasing pressure can be adjusted in 5 levels instantly by shifting the lever. Magnetic paper guides are easily adjustable for various stock sizes. Handy business card collection tray snaps into place for neat stacking of finished cards. Velocity also features 2 single blade slitters to trim the top and bottom margins, and 2 double blade slitters for center gutters and precise accuracy. The durable blades cut stocks up to 400 gsm. The air-suction top feeding system easily feeds coated, digital, gloss and other stocks precisely without damage. Includes the new Lytrod Intellicut software to easily impose artwork + address data to seamlessly create PDF layouts with job barcodes and cut marks for the Velocity.\n\nDimensions (D x W x H), inches: 28 x 75.35 x 42\nShipping weight: 529 lbs.\n\nNote: The Aerocut Velocity is a restricted product. Please contact your sales representative for terms.","AEROCUT VELOCITY\nSpeed 20 sheets/min.*\nSheet capacity 4\"\nPaper size 8.25 x 8.25 to 14.5 x 20.47\nPaper weight 120 - 400 gsm.**\nPower supply115 V, 60 Hz\nList Price US $29,999",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Digital-Finishing-Solutions/AEROCUT-VELOCITY-412.html","https://www.youtube.com/watch?v=Nr3AfKzhjM8",null,"Yes","Yes"]
[null,null,"AEROCUT NanoPLUS","Slitter: 4 sets (6 slitter blades)\nCutter: 1 set\nMax. paper size: 13” x 19”\nMin. paper size: 8.25” x 8.25”\nMin. work size: 3.5” x 2”\nPaper weight: 32 lb (bond) - 130 lb (Cover stock) (120 - 350g/m2)\nPaper feeding method: Air Suction\n\nDimensions (D x W x H): 24.9” x 30.2” x 39.9”\nShipping weight: 212 lbs.",null,null,"https://www.mbmcorp.com/Paper-Finishing-Products/Digital-Finishing-Solutions/AEROCUT-NanoPLUS-442.html",null,null,"Yes","Yes"]
[null,null,"AEROCUT NANO","Stable air feed mechanism takes a wide range of paper stocks. Cuts and cross cuts prints in one pass. Elevated feed table separates digital stocks to avoid mis-feedings, damages and roller marks. Density sensor for true double feed detection. 2 single blade margin slitters and 2 double blade gutter slitters are easily adjustable for various stock sizes. InstaSet bar indicates and fixes slitter positions accurately. Intuitive touch screen holds 16 pre-programmed jobs and 40 customized jobs. Includes the Lytrod VisionFocus software to simplify the task of formatting, imposing, and adding personalized information to documents for fast and efficient cutting on the Nano.\n\nDimensions (D x W x H): 25\" x 22\" x 37 1/2\" \nShipping weight: 155 lbs.","AEROCUT NANO\nSpeed, sheets per minute 22*\nPaper size, inches 8 1/4 to 13 x 19\nMinimum finished size, inches 3.3 x 2\nLoading capacity, inches 1 3/16\nPower supply120 V, 60 Hz\nList Price US $10,499",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Digital-Finishing-Solutions/AEROCUT-NANO-305.html","https://www.youtube.com/watch?v=F9Ax79SobNY",null,"Yes","Yes"]
[null,"Bookletmakers"]
[null,null,"SPRINT™ 3000","Jogs, staples, and folds in one operation. Quick and easy set-up and adjustment. Variable speed produces booklets up to 100 pages (off-line).* 2 stapling heads, 4 stapling positions. Uses 210-staple sticks. Powered exit conveyor. Transparent safety access cover—machine will not operate with cover in open position. Mounted on heavy-duty casters. Interfaces with wide range of collators including the MBM® FC 10. Optional face trimmer.\n\nDimensions (D x W x H), inches: 23\" x 46\" x 36\"\n(20\" W with conveyor stored) \nShipping weight: 280 lbs.","SPRINT 3000\nSpeed 1,500 sets/hr.*\nSheet capacity 25\nPaper size 5 1/2\" x 8\" to 12\" x 18\"\nPower supply115 V, 60 Hz\nList Price US $7,499",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Bookletmakers/SPRINT-3000-273.html",null,null,"Yes","Yes"]
[null,null,"SPRINT™ 5000","Jogs, staples, and folds in one operation. Quick and easy set-up and adjustment. Variable speed produces booklets up to 88 pages (off-line).* On-line saddle, corner, and side stapling capability. \"Fold only\" capability. Heavy-duty staple clinchers produce \"flat-finish\" staples. 2 stapling heads, 5 stapling positions uses high-capacity, 5,000-staple cartridges. Auto-stop and signal when staple cartridge is empty. Powered exit conveyor. Transparent safety access cover—machine will not operate with cover in open position. Mounted on heavy-duty casters. Interfaces with wide range of collators including the MBM® FC 10. Optional face trimmer.\n\nDimensions (D x W x H), inches: 23\" x 46\" x 36\"\n(20\" W with conveyor stored) \nShipping weight: 280 lbs.","SPRINT 5000\nSpeed 1,500 sets/hr.*\nSheet capacity 22\nPaper size 5 1/2\" x 8\" to 12\" x 18\"\nPower supply115 V, 60 Hz\nList Price US $8,199",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Bookletmakers/SPRINT-5000-274.html",null,null,"Yes","Yes"]
[null,null,"iBOOKLET","The iBOOKLET has a built in LCD counter that clearly shows job progress and settings. In case of an error, the icon based control panel clearly indicates what has happened (such as a paper jam or an empty staple magazine) which makes it easy to diagnose and resolve issues. This tabletop bookletmaker automatically adjusts stapling and folding position according to the selected paper size. It has standard paper size buttons such as letter, legal, ledger, etc. adding to the ease of use. If odd sized booklets are needed, custom paper length is programmable by pushing the FREE button, and the +/- buttons. The iBOOKLET has automatic mode and manual mode. In automatic mode, the sensor on the feeding section detects sheets fed and staples / folds automatically. In manual mode, it staples and folds sheets as soon as the START button is pushed. Count mode is selectable from addition and subtraction mode. After finishing a booklet, increase / decrease the number according to selected count mode. 3 modes can be easily switched: staple only / fold only / staple & fold. The iBOOKLET has a patent-pending stapling mechanism, which enables it to select ordinary clinch and flat clinch. Flat clincher makes booklets and documents beautifully finished and saves space. at 800 sets of booklets produced per hour, the iBOOKLET has the fastest production speed in its class. \n\nDimensions (D x W x H), inches: 19.6 x 19.6 x 15.7\nShipping weight: 55 lbs.","iBOOKLET\nSpeed 800 sets/hr*\nSheet capacity Up to 16*\nPaper size 4.3\" x 8.25\" to 13\" x 18.4\"\nPaper weight 16 to 80 lbs.*\nStaple modesaddle, side, corner staple\nList Price US $1,999.00",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Bookletmakers/iBOOKLET-420.html",null,null,"Yes","Yes"]
[null,null,"SF 2","Wire-fed stitching system provides lower operating costs than bookletmakers using pre-formed staples. Produces booklets up to 100 pages.* Low maintenance—jogs, stitches, and folds up to 65,000 booklets without replacing wire spools. Runs on-line with a variety of collators (interface is included) including the MBM® FC 10. Easy to use, push-button controls with 6 digit counter staple. Leg adjustment feature allows staple length to be custom fit to the size of book being run. Heavy-duty clutch and bearings. Moveable, magnetic stitching heads. One-step threading for quick and easy set-up. Knife fold with dual fold rollers for crisp, consistent folds. Powered exit conveyor. Transparent safety access covers—machine will not operate with covers in open position. Includes back jog, and stand with casters. Optional activated clinch, and on-line corner/side stitch gate.\n\nDimensions (D x W x H): 21\" x 52\" x 24 1/2\" \nShipping weight: 400 lbs.\n\nOPTIONAL FACE TRIMMER FOR SF 2 BOOKLETMAKER\nOperates on-line with SF 2 booklet maker. Trims booklets up to 100 pages.* Powered exit conveyor. Transparent safety access cover—machine will not operate with cover in open position.\n\nDimensions (D x W x H): 24 1/4\" x 48 1/2\" x 24\" \nShipping weight: 402 lbs.","SF 2\nSpeed 2,300 sets/hr.*\nSheet capacity 25*\nPaper size (bookletmaker) 4 3/4\" x 8 1/2\" to 12 3/4\" x 18 1/2\"\nPaper size (trimmer) 4 3/4\" x 8 3/4\" to 12 11/16\" x 18 1/4\"\nPower supply115 V, 60 Hz\nList Price US SF2 On line $15,013.95 SF2 Off line $14,089.95",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Bookletmakers/SF-2-275.html",null,null,"Yes","Yes"]
[null,null,"STITCHMASTER","Wire-fed magnetic stitching head. Compact size. Heavy-duty work table switches from flat to saddle stitching and back again in seconds. One-step threading for quick and easy set-up. Adjustable side guides. Movable clinchers ensure a tight stitch. Single knob adjustment for thickness and centering. Pop-up pins for convenient corner stapling. Foot pedal operation. Mounts easily to most work tables. Transparent safety guard. Optional adjustable stand (shown above), and conversion kit that allows two StitchMasters to be combined into a dual head stitcher.\n\nDimensions (D x W x H), inches: 15\" x 16\" x 24\" \nShipping weight: 50 lbs.","STITCHMASTER\nSheet capacity 60*\nPaper size 2\" x 2\" to 11\" x 17\"\nPower supply115 V, 60 Hz\nList Price US $2,628.15",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Bookletmakers/STITCHMASTER-276.html",null,null,"Yes","Yes"]
[null,"Collators"]
[null,null,"FC 10","Collates variety of paper stocks and weights at speeds up to 3,600 sets per hour.* 275 sheet bin capacity.* Touch-button control panel with LED 4 digit counter simplifies set-up and operation. Programming modes include preset batch, insertion, and an alternate bin mode for continuous production. Adjustable stacking table for straight or criss-cross stacking. Self-centering feed guides eliminate the need to reposition on-line bookletmakers for different size stock. Adjustable feed and separator pressures on each bin. Bin empty sensor. Extra large, detachable feed trays. Optional base with casters, twin tower transport unit, high capacity stacker, and corner stapler UL and C UL approved.\n\nDimensions (D x W x H), inches: 21\" x 28\" x 41 1/4\" (34\" W, 63\" H with base) \nShipping weight: 231 lbs. (281 with base)","FC 10\nNumber of bins 10\nBin capacity 275 sheets*\nPaper size 3 3/4\" x 5 7/8\" to 12 7/8\" x 18 1/2\"\nPaper weight 20 to 100 lbs.\nSpeed 3,600 sets/hr.*\nPower supply110 V, 60 Hz\nList Price US $6,799",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Collators/FC-10-287.html",null,null,"Yes","Yes"]
[null,null,"FC 10 TWIN TOWER SYSTEM","Collates variety of paper stocks and weights at speeds up to 3,600 sets per hour.* 275 sheet bin capacity.* Collator units can be used in tandem or separately while connected. Touch-button control panel with LED 4 digit counter simplifies set-up and operation. Programming modes include preset batch, insertion, and an alternate bin mode for continuous production. Adjustable stacking table for straight or criss-cross stacking. Self-centering feed guides eliminate the need to reposition on-line bookletmakers for different size stock. Adjustable feed and separator pressures on each bin. Bin empty sensor. Extra large, detachable feed trays. Optional bases with casters, and high capacity stacker, necessary when using system off-line. UL and C UL approved.\n\nDimensions (D x W x H), inches: 27 5/8\" x 86 1/2\" x 41 1/4\" (90 1/2\" W, 63\" H with bases) \nShipping weight: 487 lbs. (587 with bases)","FC 10 TWIN TOWER SYSTEM\nNumber of bins 20\nBin capacity 275 sheets (20 lb. bond)\nPaper size 3 3/4\" x 5 7/8\" to 12 7/8\" x 18 1/2\"\nPaper weight 20 to 100 lbs.\nSpeed 3,600 sets/hr.*\nPower supply110 V, 60 Hz\nList Price US $14,148",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Collators/FC-10-TWIN-TOWER-SYSTEM-288.html",null,null,"Yes","Yes"]
[null,"Support Products"]
[null,null,"JT 7","Significantly reduces misfeeds and double feeds in printers, folders, and collators. Space saving, compact footprint. V-shaped, adjustable-angle table. 4 inch tray thickness. Foot pedal operation or continuous. All-metal construction.\n\nDimensions (D x W x H), inches: 12 1/2\" x 21\" x 17 1/4\" \nShipping weight: 46 lbs.","JT 7\nPaper size 5\" x 7 3/8\" to 12 7/8\" x 17 3/4\"\nSheet capacity 1,000*\nPower supply115 V, 60 Hz\nList Price US $1,249",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Support-Products/JT-7-297.html",null,null,"Yes","Yes"]
[null,null,"AJ 700","Air-feed feature forces air between sheets to reduce jogging time and eliminate powder buildup. Press sheets and digital copies can be air dried immediately to prevent offset. Air-only and vibrate-only functions. Significantly reduces misfeeds and double feeds in printers, folders, and collators. V-shaped, adjustable-angle table. 4 inch tray thickness. Foot pedal operation or continuous. Automatic timer. All-metal construction. Mounted on casters.\n\nDimensions (D x W x H), inches: 17\" x 22\" x 45 1/4\" \nShipping weight: 84 lbs.","AJ 700\nPaper size 5\" x 7 3/8\" to 12 7/8\" x 17 3/4\"\nSheet capacity 1,000*\nPower supply115 V, 60 Hz\nList Price US $2,199",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Support-Products/AJ-700-298.html",null,null,"Yes","Yes"]
[null,null,"MBM® 25","2 inch drilling capacity. 5 pre-set patterns available at the turn of a dial. Easy-glide table moves on bearings. Side guides are self-centering for quick changes. Quick-release clamp accommodates 5/32\", 13/64\", 7/32\", and 1/4\" drill bits. High quality, 1/4\" bit included along with sharpener and honing stone.\n\nDimensions (D x W x H), inches: 14 1/8\" x 18 7/8\" x 18 1/2\" \nShipping weight: 39 lbs.","MBM 25\nDrilling capacity 2\"\nMaximum throat depth 1 3/8\"\nMaximum paper length 14 3/4\"\nTable size 18 7/8\" x 10\"\nMaximum horsepower 1/4\nPower supply115 V, 60 Hz\nList Price US $949",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Support-Products/MBM-25-299.html",null,null,"Yes","Yes"]
[null,null,"MBM® 55","2 inch drilling capacity. 5 pre-set patterns available at the turn of a dial. Easy-glide table moves on bearings. Side guides are self-centering for quick changes. Quick-release clamp accommodates 7/64\" to 1/2\" drill bits. 2 high quality bits (1/4\" and 5/16\") included along with sharpener and honing stone.\n\nDimensions (D x W x H), inches: 17\" x 18 7/8\" x 24 1/2\" \nShipping weight: 81 lbs.","MBM 55\nDrilling capacity 2\"\nMaximum throat depth 1 3/8\"\nMaximum paper length 14 3/4\"\nTable size 18 7/8\" x 10\"\nMaximum horsepower 1/2\nPower supply115 V, 60 Hz\nList Price US $1,369\n",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Support-Products/MBM-55-300.html",null,null,"Yes","Yes"]
[null,null,"FMM3","2 inch drilling capacity. Easily adjustable head design. Easy-glide table moves on bearings. Measuring scale on table. Accommodates 1/8\" to 1/2\" drill bits. 3 high quality, 1/4\" bits included. Bit sharpener with solid carbide head included.\n\nDimensions (D x W x H), inches: 15\" x 32\" x 52\" \nShipping weight: 292 lbs.\n\n","FMM3\nDrilling capacity 2\"\nMaximum throat depth 3 3/4\"\nMaximum paper length 32\"\nTable size 32 \" x 15\"\nMaximum horsepower 3/4\nPower supply115 V, 60 Hz\nList Price US $4,999",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Support-Products/FMM3-301.html",null,null,"Yes","Yes"]
[null,null,"ES 2000","Quickly and easily folds and seals single-sheet self mailers. Provides an environmentally friendly mailing solution by eliminating envelopes. Can be used for a wide variety of applications including paychecks, invoices, tax forms (W2, 1099, etc.), medical reports, and ID cards. Compact, desktop design and quiet operation make it ideal for corporate environments. Easy to set up and maintain. Proprietary angled seal technology provides exceptional fold and seal quality. 4 fold settings (Z, V, EZ, double parallel).\n\nDimensions (D x W x H), inches: 15\" x 13\" x 11\" \nShipping weight: 80 lbs.","ES 2000\nSpeed 2,200 sheets/hr\nPaper size 6\" x 8\" to 9 1/4\" x 14\"\nPaper weight 24 to 28 lbs.\nSheet capacity 150*\nPower supply115 V, 60 Hz\nList Price US $2,514\n",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Support-Products/ES-2000-306.html",null,null,"Yes","Yes"]
[null,null,"ES 5000","Quickly and easily folds and seals single-sheet self mailers. Provides an environmentally friendly mailing solution by eliminating envelopes. Can be used for a wide variety of applications including paychecks, invoices, tax forms (W2, 1099, etc.), medical reports, and ID cards. Compact, desktop design and quiet operation make it ideal for corporate environments. Quick and easy set-up and adjustment. Entire folding unit slides out for easy maintenance. Manual feeder for pre-folded forms. Anti-jam system. 4 fold settings (Z, V, C, double parallel). Optional drum for Z and EZ folds on legal.\n\nDimensions (D x W x H), inches: 16\" x 17\" x 10\" \nShipping weight: 100 lbs.","ES 5000\nSpeed 4,250 sheets/hr\nPaper size 6\" x 8\" to 9 1/4\" x 14\"\nPaper weight 24 to 28 lbs.\nSheet capacity 150*\nPower supply115 V, 60 Hz\nList Price US $3,879",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Support-Products/ES-5000-308.html",null,null,"Yes","Yes"]
[null,null,"ES 5500","Double feed detection to stop misfeeds. Exclusive angled seal technology. LCD touch pad controls with counter. Processes more than 5,000 forms per hour. Deep 150 sheet feed table. Seals single-sheet self mailers. No envelope needed. Compact and dynamic design which features a small foot print ideal for the office desktop.\n\nDimensions (W x L x H): 13\" x 15\" x 11\" \nShipping weight: 54 lbs.","ES 5500\nSpeed, forms per hour 5,000\nForm sizes, inches Up to 14 depth, up to 9 width\nInput tray 150 pressure seal forms\nCounter Item and batch\nNoise levelLess than 45 db\nList Price US $3,984",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Support-Products/ES-5500-309.html",null,null,"Yes","Yes"]
[null,null,"ES 8000","Large capacity elevator infeed table holds 700 pressure seal forms. Processes up to 8,000 forms per hour. User friendly operator panel. Multi-sensor monitoring system. Built-in 350 sheet catch tray. Quick set manual fold setting. Optional inline kit to select printers for easy printer interface. Automatically detects double feeds.\n\nDimensions (W x L x H): 17\" x 24\" x 15\" \nShipping weight: 115 lbs.","ES 8000\nSpeed, forms per hour 8,000\nForm sizes, inches Up to 14 depth, up to 9 width\nPaper weights, pounds 20-28\nFeeder capacity700 pressure seal forms\nList Price US $7,659",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Support-Products/ES-8000-310.html",null,null,"Yes","Yes"]
[null,null,"IM 8100","Quick set manual fold setting. Reverse friction roller infeed type. Job counter and batch counter. Automatically detects, singulates, and corrects double feeds without any operator intervention for increased productivity. Stacking capacity of 350 sheets or 650 sheets with the optional side conveyor.\n\nDimensions (W x L x H): 17\" x 24\" x 15\" \nShipping weight: 106 lbs.","IM 8100\nSpeed, forms per hour Up to 7,000 standalone*\nForm sizes, inches Up to 14 depth, up to 9 width\nPaper weights, pounds 16-30\nFeeder capacity, sheets700 in standalone mode\nList Price US $8,709",null,"https://www.mbmcorp.com/Paper-Finishing-Products/Support-Products/IM-8100-311.html",null,null,"Yes","Yes"]
["Air Purifiers"]
[null,null,"ideal.™ AP15","Air purifier with highly effective AEON Blue cleaning system – cleans indoor air more effectively than almost any other air purifier. The ideal.™ AP15 combines HEPA, activated carbon and plasma air cleaning in one compact unit. Very effectively filters harmful substances out of the air: fine dust, pollen and other allergens, viruses and bacteria, mold spores, pet hair, cigarette smoke and even chemical fumes and odors. What’s more, it enriches the air with charged ions. Purified and ionized air – a simple and natural principle with a refreshing result: a vitalizing effect on mind and body, strengthening the immune system as well as protecting against cell damage and premature aging processes, fatigue or diseases. And all this running at very low energy and quiet as a whisper – for optimum use in offices, bedrooms or medical practices – wherever you’re looking for ideal indoor air.\n\nDimensions (D x W x H), inches: 9 x 13.7 x 18.5\nShipping weight, pounds: 17","ideal.™ AP15\nPower supply 120 V, 60 Hz\nFan speed 4 steps (adjustable)\nNoise levels (dB) 26 / 35 / 43 / 52\nRoom size (square feet) 150\nPlacingFloor, tables\nList Price US $189.00",null,"https://www.mbmcorp.com/ideal-Air-Purifiers/ideal-AP15-377.html","https://www.youtube.com/watch?v=_5F-K7fuE-M",null,"Yes","Yes"]
[null,null,"ideal.™ AP30","Air purifier with highly effective AEON Blue cleaning system – cleans indoor air more effectively than almost any other air purifier. The ideal.™ AP30 combines HEPA, activated carbon and plasma air cleaning in one compact unit. Very effectively filters harmful substances out of the air: fine dust, pollen and other allergens, viruses and bacteria, mold spores, pet hair, cigarette smoke and even chemical fumes and odors. What’s more, it enriches the air with charged ions. Purified and ionized air – a simple and natural principle with a refreshing result: a vitalizing effect on mind and body, strengthening the immune system as well as protecting against cell damage and premature aging processes, fatigue or diseases. And all this running at very low energy and quiet as a whisper – for optimum use in offices, bedrooms or medical practices – wherever you’re looking for ideal indoor air.\n\nProduct dimensions (D x W x H), inches: 10.4 x 16.3 x 21.6\nShipping weight, pounds: 23","ideal.™ AP30\nPower supply 120 V, 60 Hz\nFan speed 4 steps (adjustable)\nNoise levels (dB) 26 / 35 / 46 / 55\nRoom size (square feet) 300\nPlacingFloors, tables\nList Price US $249.00",null,"https://www.mbmcorp.com/ideal-Air-Purifiers/ideal-AP30-378.html","https://www.youtube.com/watch?v=_5F-K7fuE-M",null,"Yes","Yes"]
[null,null,"ideal.™ AP45","Air purifier with highly effective AEON Blue cleaning system – cleans indoor air more effectively than almost any other air purifier. The ideal.™ AP45 combines HEPA, activated carbon and plasma air cleaning in one compact unit. Very effectively filters harmful substances out of the air: fine dust, pollen and other allergens, viruses and bacteria, mold spores, pet hair, cigarette smoke and even chemical fumes and odors. What’s more, it enriches the air with charged ions. Purified and ionized air – a simple and natural principle with a refreshing result: a vitalizing effect on mind and body, strengthening the immune system as well as protecting against cell damage and premature aging processes, fatigue or diseases. And all this running at very low energy and quiet as a whisper – for optimum use in offices, bedrooms or medical practices – wherever you’re looking for ideal indoor air.\n\nProduct dimensions (D x W x H), inches: 11.7 x 18.8 x 25.6\nShipping weight, pounds: 30","ideal.™ AP45\nPower supply 120 V, 60 Hz\nFan speed 4 steps (adjustable)\nNoise levels (dB) 27 / 38 / 50 / 60\nRoom size (square feet) 450\nPlacingFloor, tables\nList Price US $379.00",null,"https://www.mbmcorp.com/ideal-Air-Purifiers/ideal-AP45-379.html","https://www.youtube.com/watch?v=_5F-K7fuE-M",null,"Yes","Yes"]
[null,null,"ideal.™ AP40 Med Edition","Professional air cleaner with individually replaceable high-quality filter elements. Filters pollutants such as fine dust, pollen and acarid allergens, pathogens such as viruses, bacteria, and mold spores, cigarette smoke, exhaust fumes, chemical vapors, and odors from the air. The antimicrobial CleanCel® equipment of the device and the antimicrobial coating “MedShield” of the HEPA filter inhibit the growth of microbes and removes pathogens. Optimally selectable PlasmaWave® technology supports the removal of bacteria, viruses and mold spores from the indoor air. When switched off, the device automatically seals the outlet thus keeping its interior clean in this state as well. High-quality touch display for intuitive control. Provides function modes such as Auto/manual/sleep/turbo. In AutoMode, continually monitors the air quality with intelligent sensor technology (sensors for fine dust, gas, odors and brightness) and automatically controls power. Additional adjustment options: fan speed can be manually adjusted at 5 levels (Sleep/low/middle/high/turbo). PlasmaWave® system can be turned on/off with touch of a button. A timer can optionally be preset to a run time of 1, 4 or 8 hours. Child-proof lock function. Convenient function indicators show the current operational state at any time. The filter change display informs a pending filter change. On an average, the filters have to be changed after 12 months.\n\nProduct dimensions (D x W x H), inches: 9.6 x 16.3 x 23.6\nShipping weight, pounds: 28","ideal.™ AP40\nPower supply 120 V, 60 Hz\nFan speed 5 levels (manual/auto)\nNoise levels (dB) 28 / 30 / 44 / 56\nRoom size (square feet)400\nList Price US $399.00",null,"https://www.mbmcorp.com/ideal-Air-Purifiers/ideal-AP40-Med-Edition-408.html",null,null,"Yes","Yes"]
[null,null,"ideal.™ AP60 Pro","The \"Made in Germany\" AP60 Pro is a professional air purifier with a high performing 360° multi-layer filter. Filters pollutants such as fine dusts (PM10, PM2.5, PM0.3, PM0.1), pollen and acarid allergens, pathogens such as bacteria and mold spores, cigarette smoke, exhaust fumes, chemical vapors (Formaldehyde, Toluol, n-Butane, VOC’s, etc.) and odors from the indoor air. User-friendly control panel provides function modes such as auto / manual / turbo. In auto mode, AP60 Pro continually monitors the air quality with intelligent sensor technology (sensors for fine dust, gas, odors) and automatically controls the power. In turbo mode, AP60 purifies the indoor air in a short period of time. In addition to the automatic and turbo adjustment, the fan speed can be manually adjusted at 5 levels with a separate super-quiet night mode. Timer function can be preset to a run time of 1, 2, 4, or 8 hours. Child-proof lock function. The current operational state is displayed. AP60 Pro automatically informs when to change the 360° filter by showing a red “F“ on top of the device. On average, the 360° filter has to be changed after 12 months, depending on the intensity of the usage.  \n\nProduct dimensions (D x W x H), inches: 10.8 x 18.4 x 26.3\nShipping weight, pounds: 33","ideal.™ AP60 Pro\nPower supply 120 V, 50 / 60 Hz\nFan speed 5 levels\nNoise levels (dB) 19 / 27 / 33 / 42 / 55\nRoom size (square feet) 600\nPlacingFloor\nList Price US $999.00",null,"https://www.mbmcorp.com/ideal-Air-Purifiers/ideal-AP60-Pro-434.html","https://www.youtube.com/watch?v=46HtVIsHxZI",null,"Yes","Yes"]
[null,null,"ideal.™ AP80 Pro - with WiFi","The AP80 Pro is a professional air purifier with a high performing 360° multi-layer filter. Filters pollutants such as fine dusts (PM10, PM2.5, PM0.3, PM0.1), pollen and acarid allergens, pathogens such as bacteria and mold spores, cigarette smoke, exhaust fumes, chemical vapors (Formaldehyde, Toluol, n-Butane, VOC’s, etc.) and odors from the indoor air. User-friendly control panel provides function modes such as auto / manual / turbo. In auto mode, AP80 Pro continually monitors the air quality with intelligent sensor technology (sensors for fine dust, gas, odors) and automatically controls the power. In turbo mode, AP80 purifies the indoor air in a short period of time. In addition to the automatic and turbo adjustment, the fan speed can be manually adjusted at 5 levels with a separate super-quiet night mode. Timer function can be preset to a run time of 1, 2, 4, or 8 hours. Child-proof lock function. The current operational state is displayed. AP80 Pro automatically informs when to change the 360° filter by showing a red “F“ on top of the device. On average, the 360° filter has to be changed after 12 months, depending on the intensity of the usage.\n\nProduct dimensions (D x W x H), inches: 10.8 x 18.4 x 26.3\nShipping weight, pounds: 33","ideal.™ AP80 Pro\nPower supply 220 - 240 V, 50 / 60 Hz\nFan speed 5 levels\nNoise levels (dB) 18.7 / 28.8 / 37.3 / 46.7 / 63.4\nRoom size (square feet) 800\nPlacingFloor\nList Price US $1,199.00",null,"https://www.mbmcorp.com/ideal-Air-Purifiers/ideal-AP80-Pro-with-WiFi-437.html",null,null,"Yes","Yes"]
[null,null,"ideal.™ AP100 Med Edition","Professional air cleaner with individually replaceable high-quality filter elements. The 7-level cleaning system filters pollutants such as fine dust, pollen and acarid allergens, pathogens such as viruses, bacteria, and mold spores, cigarette smoke, exhaust fumes, chemical vapors and odors from the air**. Level 1: Fine prefilter - filters particles such as dust, hairs, pollen, lint. Level 2: CleanCel® equipment - inhibits the growth of microbes. Level 3: PM2.5 filter - filters ultra-fine air pollutants of a size of 2.5 µm. Level 4: Antimicrobial coating “MedShield” - removes 99.9% pathogen viruses, bacteria, and mold spores from the air. Level 5: High performance activated carbon filter - removes various odors and harmful gases such as tobacco smoke, food odors, acetic acid, disinfectants, ammonia, formaldehyde, toluol, VOCs, and others. Level 6: Optionally selectable PlasmaWave® system – actively supports the removal of bacteria, viruses, mold spores and ultra fine particles from the indoor air. Level 7: True HEPA Filter – filters 99.97% of the ultra-fine particles of 0.3µm such as fine dust, dental dust, and sooty particles. The antimicrobial CleanCel® equipment of the device’s interior inhibits the growth of microbes. Provides function modes such as Auto/manual/sleep/turbo. In AutoMode, continually monitors the air quality with intelligent sensor technology (sensors for fine dust, gas, odors and brightness) and automatically controls the power. However, manual operation and adjustment is possible. The air cleaner can be controlled intuitively using a 4-inch LCD touch screen for timer function, night function, displaying individual filter conditions, weather data and air quality data. Operational guidance in three languages. Inclusion into a WLAN is possible. Even more comprehensive operation and data is available from the device using the ideal.™ air app (free in the App Store or with Google Play). Mobile thanks to castors.\n\nProduct dimensions (D x W x H), inches: 17 x 17 x 39.8\nShipping weight, pounds: 67","ideal.™ AP100\nPower supply 120 V, 60 Hz\nFan speed 5 levels (manual /auto)\nNoise levels (dB) 29 / 34 / 41 / 48 / 56\nRoom size (square feet)1,000\nList Price US $1,499.00",null,"https://www.mbmcorp.com/ideal-Air-Purifiers/ideal-AP100-Med-Edition-409.html",null,null,"Yes","Yes"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]
[{"$nulls":9},"No","Not Yet"]

{"sheet":"FP","index":7,"n_rows":63,"n_cols":12,"rows_kept":63,"cut":false,"hidden":false,"merged":[[33,6,34,6],[56,6,58,6],[33,8,34,8]]}
["Category","Sub-Category (if applicable)","Product Name","Product Description","Specifications","Serial #","Vendor Site URL","Video Content URL(s)","Downloadable Content URL(s)","Pictures Saved?","Migrated?","Alternative Site URL"]
["Meters"]
[null,null,"PostBase mini","Small office, home office Postage Meter, affordable postage for small business and power sellers",null,null,"https://www.fp-usa.com/postage-meters/postbase-mini/",null,"http://download.fp-usa.com/product_docs/postbase_mini/postbase-mini-brochure.pdf","Yes","Not Yet"]
[null,null,"PostBase econ","Low volume postage system at up to 30 cycles per minute for small businesses, cost saving, accurate, and efficient.",null,null,"https://www.fp-usa.com/postage-meters/postbase-econ/",null,"https://portal.fp-usa.com/_pdf/product_brochures/PostBase20_Brochure.pdf","Yes","Not Yet"]
[null,null,"PostBase semi","The perfect Postage Meter option for your office. The PostBase semi postage meter line does up to 45 cycles per minute with semi-automatic feeder.",null,null,"https://www.fp-usa.com/postage-meters/postbase-semi/",null,"https://portal.fp-usa.com/_pdf/product_brochures/PostBasesemi_temp.pdf","Yes","Not Yet"]
[null,null,"PostBase auto","This Postage Meter features an Automatic feeding system as a standard that can post up to 85 envelopes per minute, quick and simple to use.",null,null,"https://www.fp-usa.com/postage-meters/postbase-auto/",null,"https://portal.fp-usa.com/_pdf/product_brochures/PostBase_auto_temp.pdf","Yes","Not Yet"]
[null,null,"PostBase pro","Our PostBase pro Postage system blast through up to 140 envelopes per minute with automatic feeder as standard, flexible and fast.",null,null,"https://www.fp-usa.com/postage-meters/postbase-pro/",null,"https://issuu.com/fpusa/docs/postbase_pro_web3?e=25839527/44510004","Yes","Not Yet"]
[null,null,"PostBase proDS","The Postbase pro DS postage system has incredible dynamic feeding capabilities and up to 110 letters per minute with dynamic scale activated, simple and fast.",null,null,"https://www.fp-usa.com/postage-meters/postbase-prods/","https://www.youtube.com/watch?v=9DV4F5jo-WY&feature=youtu.be","https://issuu.com/fpusa/docs/postbase_prods_web3?e=25839527/44510140","Yes","Not Yet"]
[null,null,"PostBase ONE","Unique dynamic vertical feed for true mixed mail weighing a, no pre-sorting. PostBase ONE is the ultimate Postage Machine",null,null,"https://www.fp-usa.com/postage-meters/postbase-one/","https://www.youtube.com/watch?v=DiSH63iskNg&feature=youtu.be","https://issuu.com/fpusa/docs/postbase_one_web4?e=25839527/44510966","Yes","Not Yet"]
["Inserters"]
[null,null,"FPi 600","Feed. Fold. Seal. There’s nothing our FPi 600 folder inserter machine does better! Expect efficiency and simplicity in every folder inserter model from the FP Mailing Solutions line.",null,null,"https://www.fp-usa.com/folder-inserters/fpi-600/",null,null,"Yes","Yes"]
[null,null,"FPi 2300","The FPi 2300 folder inserter gives you the best solution for folding your business documents into C6, C6/5 and C5 envelopes.",null,null,"https://www.fp-usa.com/folder-inserters/fpi-2300/",null,"https://portal.fp-usa.com/_pdf/product_brochures/FPi-2300_Brochure_071913.pdf","Yes","Yes"]
[null,null,"FPi 4700","The FPI 4700 folder inserter automatically organizes every document for perfect sequence and collation.",null,null,"https://www.fp-usa.com/folder-inserters/fpi-4700/",null,"https://issuu.com/fpusa/docs/fpi4700-brochure_final_web?e=25839527/42128583","Yes","Yes"]
[null,null,"FPi 5600","The FPI-5600 folder inserter makes tackling business mail a cinch. Easily feed, fold and insert documents into envelopes with the touch of a button.",null,null,"https://www.fp-usa.com/folder-inserters/fpi-5600/",null,"https://portal.fp-usa.com/_pdf/product_brochures/FPi-5600_6600%20Brochure_040113.pdf","Yes","Yes"]
[null,null,"FPi 6600-2","The FPI 6600-2 folder inserter is our top-of-the-line product, assembling mailings with superior finish in no time. High-volume mailrooms benefit from reliable output and the simplification of complex mail pieces.",null,null,"https://www.fp-usa.com/folder-inserters/fpi-6600/",null,"http://download.fp-usa.com/product_docs/fpi-6600/fpi-6600-brochure.pdf","Yes","Yes"]
[null,null,"A.M.P.","Analyze. Match. Print (AMP) technology simplifies blind match mailings by analyzing documents barcodes, matching the barcodes to the recipients, and printing addresses onto envelopes.",null,null,"http://www.fp-usa.com/folder-inserters/a-m-p","https://www.youtube.com/watch?v=j8uAvE3ddU8&feature=youtu.be","https://issuu.com/fpusa/docs/amp-web-cut-sheet?e=25839527/39583727","Yes","Yes"]
["Software"]
[null,null,"MailOne","MailOne 2.0 software is the ultimate tool to monitor, manage, track and reduce your postal expenditures.",null,null,"https://www.fp-usa.com/software/mailone/",null,"https://issuu.com/fpusa/docs/mail_one_broch_-web?e=25839527/53223957","Yes","Yes"]
[null,null,"RemoteOne","RemoteOne Software enables its users to remotely control all functions of their postage meter through their PC.",null,null,"https://www.fp-usa.com/software/remoteone/",null,"N/A","Yes","Yes"]
[null,null,"ReportOne","ReportOne, an upgrade to the standard RemoteOne software adds detailed transaction reporting & exporting.",null,null,"https://www.fp-usa.com/software/reportone/",null,"N/A","Yes","Yes"]
[null,null,"QTrak","Tracking packages has never been easier. Never lose a package again. QTrak allows you to monitor package status from the moment they enter your facility until they reach their intended recipient.",null,null,"https://www.fp-usa.com/software/qtrak/","https://www.youtube.com/watch?v=dojXL7D9Kpw&feature=youtu.be","N/A","Yes","Yes"]
[null,null,"FlexMail","FlexMail software makes it easy to connect to, clean and organize address data from any source and print graphically rich personalized envelopes on any printer.",null,null,"https://www.fp-usa.com/software/flexmail/",null,"https://portal.fp-usa.com/_pdf/product_brochures/FlexMail4Brochure42612.pdf","Yes","Yes"]
[null,null,"FlexStream","FlexStream is an Output Management Solution that enhances business operations by automating the processing and distribution of business critical documents.",null,null,"https://www.fp-usa.com/software/flexstream/",null,"https://portal.fp-usa.com/_pdf/product_brochures/FlexStreamBrochureUSFeb12016.pdf","Yes","Yes"]
[null,null,"MailCredit","MailCredit technology allows postage downloads via a connected Windows computer using today’s high-speed digital connections, while retaining the flexibility and choice of using traditional analog phone lines (teleset™) as well.",null,null,"https://www.fp-usa.com/software/mailcredit/",null,"https://issuu.com/fpusa/docs/qtrak_brochure?e=25839527/50217752","Yes","Yes"]
["Solutions","Folder"]
[null,null,"FP 1001","With the FP 1001, anyone can save time and eliminate tedium with automated folding at up to 140 sheets per minute.",null,null,"https://www.fp-usa.com/folder/fp-1001",null,"http://portal.fp-usa.com/_pdf/product_brochures/FP1001_Brochure102312.pdf","Yes","Not Yet"]
[null,null,"DF 755","The DF 755 has six popular pre-programmed folds and a multitude of custom folds that offer crisp and accurate folding for a variety of applications.",null,null,"https://www.fp-usa.com/folders/df-755",null,"http://portal.fp-usa.com/_pdf/product_brochures/DF755_Brochure_071812.pdf","Yes","Not Yet"]
[null,null,"DF 777","The DF 777 is built on the same platform as the DF 755, adding greater speed and electronically operated automatic job setup.",null,null,"https://www.fp-usa.com/folder/df-777/",null,"http://portal.fp-usa.com/_pdf/product_brochures/DF777_Brochure_071812.pdf","Yes","Not Yet"]
[null,null,"DF 915","Let Duplo’s DF 915 Automatic Tabletop Folder take care of all your folding needs. High-speed folding up to 280 sheets per minute has never been easier.",null,null,"https://www.fp-usa.com/folders/df-915/",null,null,"Yes","Not Yet"]
[null,null,"DF 970","The DF 970 is one of the quietest and fastest tabletop folders, perfect for offices that have a regular need for paper folding.",null,null,"https://www.fp-usa.com/folders/df-970/",null,"http://portal.fp-usa.com/_pdf/product_brochures/DF970_Brochure.pdf","Yes","Not Yet"]
[null,null,"DF 980","The DF 980 is the quietest tabletop folder in its class, making it ideal for operation in office environments.",null,null,"https://www.fp-usa.com/folders/df-980/",null,"http://portal.fp-usa.com/_pdf/product_brochures/df980_brochure.pdf","Yes","Not Yet"]
[null,null,"DF 1200","The DF 1200 uses unique suction technology to move paper with remarkable ease and reliability.",null,null,"https://www.fp-usa.com/folders/df-1200",null,"http://portal.fp-usa.com/_pdf/product_brochures/df1200_brochure.pdf","Yes","Not Yet"]
[null,"Scales"]
[null,null,"Flexiscale 70","The ideal scale for large packages.\n\nCapacity 70 lbs.\nInterfrace to FP postage meters (OptiMail™ 30, UltiMail™, CentorMail™ MAX)",null,null,"https://www.fp-usa.com/scales/",null,"N/A","Yes","Yes"]
[null,null,"Excelscale 30,70","Non-rate-calculating scales for use with FP™ MailOne™ Software.\n\nCapacity 30 or 70 lbs.\nInterface to PC via USB connection with MailOne™ 2.0.",{"$nulls":5},"Yes","Yes"]
[null,"Address Printers/Edge Print Series"]
[null,null,"FP EDGE","With the FP EDGE, effortlessly print marketing messages and vibrant designs that grab the attention of your recipients at a very low cost per print.",null,null,"https://www.fp-usa.com/edge/the-edge/",null,"https://issuu.com/fpusa/docs/edge_print_series_issu?e=25839527/53695703","Yes","Yes"]
[null,null,"Double EDGE","The Double EDGE takes your print efficiency to the next level with its duplex print capability. Easily print on both sides of your mail piece with one click of a button.",null,null,"https://www.fp-usa.com/edge/the-double-edge/",null,"https://issuu.com/fpusa/docs/edge_print_series_issu?e=25839527/53695703","Yes","Yes"]
[null,null,"EDGE xs","An entirely new way to print, the EDGE xs inkjet label printer introduces the solution for continuous, high-quality, digital labels at a lower cost than traditional print methods.",null,null,"https://www.fp-usa.com/edge/the-edge-xs/",null,"https://issuu.com/fpusa/docs/edge_xs?e=25839527/53695116","Yes","Yes"]
[null,null,"AJ-5000","The AJ-5000 is an entry-level inkjet address printer and has the ability to print in brilliant, full-process color.",null,null,"https://www.fp-usa.com/address-printers/aj-5000/",null,"https://portal.fp-usa.com/dashboard/Products/OEM%20Equipment/Desktop%20Imager_Brochure050813.pdf","Yes","Yes"]
[null,null,"AJ 500","The AJ-500 has a fixed-head and is an entry-level inkjet address printer.",null,null,"https://www.fp-usa.com/address-printers/aj-500",null,"https://portal.fp-usa.com/dashboard/Products/OEM%20Equipment/Desktop%20Imager_Brochure050813.pdf","Yes","Yes"]
[null,null,"AJ 1000","The FP AJ-1000 is versitile due to its feed system that has three rows of high grip rollers and the capacity for materials up to 1/4“ thick.",null,null,"https://www.fp-usa.com/address-printers/aj-1000/",null,"https://portal.fp-usa.com/dashboard/Products/OEM%20Equipment/Desktop%20Imager_Brochure050813.pdf","Yes","Yes"]
[null,null,"AJ 2650/2800","Print graphics as well as logos, and barcodes at up to 600 dpi with the AJ-2650 a six-head printer, and AJ-2800, an eight-head printer.",null,null,"https://www.fp-usa.com/address-printers/aj-2650aj-2800/",null,"https://portal.fp-usa.com/dashboard/Products/OEM%20Equipment/Desktop%20Imager_Brochure050813.pdf","Yes","Not Yet"]
[null,null,"AJ 3600/3800","Print addresses, in addition to attention lines, postal barcodes, return addresses, and permit indicia – this complete selection provides the\nflexibility you need to cost-effectively boost productivity and enhance image quality.",null,null,"https://www.fp-usa.com/address-printers/aj-3600aj-3800/",null,"N/A","Yes","Not Yet"]
[null,null,"IB 9000","Print addresses, attention lines, postal barcodes, return addresses, in addition to permit indicia – this complete selection provides the\nflexibility you need to cost-effectively boost productivity and enhance image quality.",null,null,"http://www.fp-usa.com/address-printers/ib-9000",null,"N/A","Yes","Not Yet"]
[null,"Tabbing/Labeling/Stamping"]
[null,null,"ATS 12","This fixed-speed, single tabber gives you all the advantages and cost savings of high-speed tabbing in one compact and economical unit.",null,null,"https://www.fp-usa.com/tabbing-labeling-stamping/ats-12/",null,"http://download.fp-usa.com/product_docs/Tabbers/ATS-12%20Brochure.pdf","Yes","Yes"]
[null,null,"ATS 309","Whether it‘s side-to-side or single tabbing, the ATS-309 tabbing machine will make your job more productive and efficient with speeds up to 25,000 pieces per hour. It also meets the newest postal regulations to ensure accuracy every time.",null,null,"https://www.fp-usa.com/tabbing-labeling-stamping/ats-309/",null,"https://portal.fp-usa.com/_pdf/product_brochures/ATS-309_Tabber.pdf","Yes","Yes"]
[null,null,"ATS 8900","This multiple tabber/stamp affixer is the only machine available in its price range that tabs 1 to 3 tabs or stamps in-line.",null,null,"https://www.fp-usa.com/tabbing-labeling-stamping/ats-8900",null,"https://portal.fp-usa.com/_pdf/product_brochures/ATS-8900_Tabber.pdf","Yes","Yes"]
[null,null,"ATS 9900/9950","Fast and versatile, these top-of-the-line, high-end tabletop labelers/tabbers handle up to 35,000 pcs./hr. and up to three tabs in one pass.",null,null,"https://www.fp-usa.com/tabbing-labeling-stamping/ats-9900ats-9950",null,"https://portal.fp-usa.com/_pdf/product_brochures/ATS-9900_9950_Tabber.pdf","Yes","Yes"]
[null,null,"ATS 9600/9700","Unlike most tabbers in their class that can only output paper tabs, the fast and versatile ATS-9600 high-speed labeler/tabber and ATS-9700 labeler/tabber/ stamper affixer handles up to 25,000 pieces an hour on a typical tri-fold mailer.",null,null,"https://www.fp-usa.com/tabbing-labeling-stamping/ats-9600ats-9700/",null,"https://portal.fp-usa.com/_pdf/product_brochures/ATS-9600_9700_Tabbers.pdf","Yes","Yes"]
[null,"Paper Jogger"]
[null,null,"Paper Jogger 400",null,null,null,"https://www.fp-usa.com/accessories/paper-jogger-400/",null,"https://portal.fp-usa.com/_pdf/product_brochures/PaperJogger400Brochure.pdf","Yes","Yes"]
[null,"Furniture"]
[{"$nulls":6},"https://www.fp-usa.com/accessories/furniture/",null,"http://download.fp-usa.com/product_docs/furniture/fp%20mail%20equipment%20furniture%20brochure.pdf","Yes","Not Yet"]
[null,"Power Conditioning"]
[null,null,"LC315","The industry’s most effective way to manage power protection for your fleet. LC315 offers the same industry-leading power protection and data capture as our SmartProtect solution. Additionally it offers real-time fleet visibility and control.",null,null,"https://www.fp-usa.com/accessories/power-conditioning/",null,"N/A","Yes","Yes"]
[null,null,"LC215","This is protection for all power anomalies which means less equipment errors, failures and downtime. More than just surge or filter solutions, Our CoreProtect protects from damaging power disturbances so your office equipment can not be harmed.",{"$nulls":4},"N/A","Yes","Yes"]
[null,null,"LC115","This is protection for all power anomalies which means less equipment errors, failures and downtime. More than just surge or filter solutions, Our CoreProtect protects from damaging power disturbances so your office equipment can not be harmed.",{"$nulls":4},"N/A","Yes","Yes"]
[null,"Letter Opener"]
[null,null,"Letter Opener 440A","The LO 440 letter opener is the perfect solution for small to mid-size companies. Make quick work of processing mail with\nthis efficient, automatic letter opener. At a speed of up to 25,000 pieces per hour, this machine makes the chore of daily\nmail opening a breeze.",null,null,"https://www.fp-usa.com/letter-opener/lo-440a/",null,"http://download.fp-usa.com/product_docs/letter_openers/LO440%20Letter%20Opener%20Brochure.pdf","Yes","Yes"]
[null,null,"Letter Opener 2112","The 2112 can open long runs of mixed-size envelopes at up to 24,000 pieces per hour. Instead of struggling to keep pace with medium-to-high volumes of incoming mail, you’ll relax as the 2112 gives you a long life of reliable, efficient operation.",null,null,"https://www.fp-usa.com/letter-opener/lo-2112/","https://www.youtube.com/watch?v=kUpvCJxXE3I&feature=youtu.be","http://download.fp-usa.com/product_docs/letter_openers/2112%20Letter%20Opener%20Brochure.pdf","Yes","Yes"]
[null,null,"Letter Opener 306","The 306 offers the speed and features needed in high volume incoming mail centers. Able to open 100 letters in under 10 seconds (40,000 pieces per hour), this machine will make quick work of all your envelopes, including large flats and overnights up to ½” thick.",null,null,"https://www.fp-usa.com/letter-opener/lo-306/","https://www.youtube.com/watch?v=vU41R2hDlN4&feature=youtu.be","http://download.fp-usa.com/product_docs/letter_openers/306%20Letter%20Opener%20Brochure.pdf","Yes","Yes"]